# Pass through

## 1. Summary

In this page you can edit the settings of the pass through function.
If you enable the pass through function, you can forward special frames that are usually discarded.

## 2. Top page

This is the top page for pass through.

### 2.1. EAP pass through setting

- The current setting is shown as to whether the EAP pass through is enabled.

- If the EAP pass through is enabled, the device forwards the received EAPOL frames so that the device can be placedbetween the IEEE 802.1X authentication switch and PCs.

- Press the "Setting" button to access a page where you can change the settings.

## 3. EAP pass through settings page

In this page you can specify whether the EAP pass through is enabled.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

### 3.1. EAP pass through setting

- EAP pass through

  - Enable

    - Forwards received EAPOL frames.

  - Disable

    - Discards received EAPOL frames.

Search result
No more search results.
There are no topics that match your search query.