# Apply access list

## 1. Summary

Apply the access list for the interface on this page.

## 2. Top page

This is the top page for applying the access list.

### 2.1. Interface list

- The access list information applied to the interface is displayed.

- The table items are explained below.

  - I/F

    - Displays the interface name.

  - Access list (IN)

    - The information listed below for the access list applied to the input side of the interface is shown here.

      - ID

        - The access list ID will be displayed.

      - Type

        - The access list type will be displayed.

      - Description

        - The description text set in this access list will be displayed.

  - Access list (OUT)

    - Information for the access list applied to the input side of the interface is shown here.

    - Information similar to the access list (IN) will be displayed.

- Press the "Setting" button to display the page for configuring the selected interface.

- Press the "Specify all" button to configure the settings for all interfaces with the check box selected.

- Press the "Return to defaults" button to initialize the settings for all interfaces with the check box selected.

### 2.2. VLAN interface list

- The access list information applied to the interface is displayed.

- The table items are explained below.

  - I/F

    - Displays the interface name.

  - Access list (IN)

    - The information listed below for the access list applied to the input side of the interface is shown here.

      - ID

        - The access list ID will be displayed.

      - Type

        - The access list type will be displayed.

      - Description

        - The description text set in this access list will be displayed.

  - Access list (OUT)

    - Information for the access list applied to the input side of the interface is shown here.

    - Information similar to the access list (IN) will be displayed.

- Press the "Setting" button to display the page for configuring the selected interface.

- Press the "Specify all" button to configure the settings for all interfaces with the check box selected.

- Press the "Return to defaults" button to initialize the settings for all interfaces with the check box selected.

## 3. Selection page for access lists to apply

This page is for selecting the access list to apply to the interface.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

### 3.1. Select access list to apply

- Applicable interface

  - The interface on which the access list will be applied is displayed.

- Access list to apply (IN)

  - Select the access list to apply to the input side of the interface.

  - Press the "Select" button to display the file "Access list selection" dialog box.

  - On the "Access list selection" dialog, you can select the check box for an access list and press the "OK" button to select the access list to apply.

  - Press the "Detail" button in the "Access list selection" dialog box to display the targeted access list.

  - In the IPv4 access list which specifies port numbers by range, only one interface can be applied for the entire system.

  - The number of control conditions that can be applied to an interface is 6112 for the entire system.

  - Applying an access list to one interface will decrease the number of applicable control conditions equal to the control conditions included in the access list.

  - For example, when an access list with five specified control conditions is applied to the input side of port1.1, the number of control conditions that can be applied is decreased by 5.

  - Note that the number of control conditions that can be actually applied is less than 6112, because the control conditions are also used in the system and other functions.

- Access list to apply (OUT)

  - Select the access list to apply to the output side of the interface.

  - The setting details for the access list (OUT) to be applied are equivalent to the access list (IN) to be applied.

  - IPv4 access lists which specify port numbers by range cannot be applied to the output side.

  - MAC access lists cannot be applied to the output side of an interface.

  - Access lists cannot be applied to the output side of a logical interface.

Search result
No more search results.
There are no topics that match your search query.