# Port mirroring settings

## 1. Summary

This page is for changing the port mirroring settings.

## 2. Top page

This is the top page for the port mirroring settings.

### 2.1. Port mirroring settings

- The current settings for the port mirroring are shown.

- The table items are explained below.

  - Check box

    - Select the check box to delete the sniffer port setting.

  - Sniffer port

    - Displays the interface name of a sniffer port.

  - Monitored port

    - Displays the interface name of monitored ports.

  - Monitoring direction

    - Displays the monitoring direction for a monitored port.

- Press the "New" button to display a page where you can create new settings for a sniffer port.

- Press the "Setting" button to display the page where you can change the settings of a sniffer port.

- If you press the "Delete" button, all sniffer ports whose check boxes are selected will be deleted.

- Up to 1 sniffer port can be configured.

## 3. Port mirroring settings page

This page is for changing the port mirroring settings.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

### 3.1. Port mirroring settings

- Sniffer port

  - When configuring new settings

    - This page is for changing the port mirroring settings.

    - Select the interface to operate as a sniffer port.

    - Press the "Select" button to display the "Sniffer port selection" dialog.

  - When changing settings

    - You can select a sniffer port by checking the port check box and clicking the "OK" button in the "Sniffer port selection" dialog.

  - You cannot specify the port where sampling rate is set in sFlow as a sniffer port.

- Monitored port

  - Select the ports that will be monitored from a selected sniffer port.

  - Press the "Select" button to display the "Monitored port selection" dialog.

  - Monitored ports can be selected in the "Monitored port selection" dialog by placing a checkmark in the corresponding checkbox, selecting the monitoring direction, and pressing the "OK" button.

  - You cannot specify the port where sampling rate is set in sFlow as a monitored port.

Search result
No more search results.
There are no topics that match your search query.