# microSD

## 1. Summary

On this page you can perform operations with the microSD card.

The microSD card will automatically be mounted when it is inserted into this unit.

When removing the microSD card from this unit while the unit is powered on, be sure to unmount the microSD card first.

If the stack function is enabled, you can perform operations with the microSD card that is inserted to the main switch.

## 2. Top page

This is the microSD top page.

Displays the mounting status of the microSD card.You canalso begin the steps here for switching the mounting status of themicroSD card.

### 2.1. Mounting switch for microSD card

- Displays the mounting status of the microSD card.

- Press the "Next" button to begin the steps for switching the mounting status of the microSD card.

## 3. microSD card mounting switch page

This page is for switching the microSD card mounting status.

Press the "OK" button to switch the mounting status of the microSD card.

If the microSD card is already mounted, it will be unmounted; and if the microSD card is already unmounted, it will be mounted.

Search result
No more search results.
There are no topics that match your search query.