# Default Settings List

The default settings for the SWX2320-30MC/SWX2322P-30MC are indicated below.

- System-wide default settings

  Category | Setting Parameter | Setting value
  --- | --- | ---
  Console | Console timeout | 600 sec
  Number of VTYs | 8
  Number of lines displayed | 24
  Password | Default administrative user | User name: admin Password: admin
  Administrative password | admin
  Encrypt password | Not encrypted
  Time Management | Time zone | JST (UTC＋9.0)
  NTP server | None
  NTP update cycle | Once per hour
  SNMP | Action | Disabled
  RMON | Action | Enabled
  sFlow | Action | Disabled
  SYSLOG | debug level log output | OFF
  information level log output | ON
  error level log output | ON
  SYSLOG server | None
  Firmware Update | Download URL | SWX2320-30MC: http://www.rtpro.yamaha.co.jp/firmware/revision-up/swx2320-30mc.bin SWX2322P-30MC: http://www.rtpro.yamaha.co.jp/firmware/revision-up/swx2322p-30mc.bin
  Permit downward revision | Prohibit
  Timeout | 300 sec
  LLDP | Action | Enabled
  Automatic setting function | Enabled
  L2MS | Action | Enabled
  Role | Agent
  Stacking | Action | Disabled
  Stack ID | 1
  IP address range used for stack port | 192.168.250.0/24
  Access control | Telnet server status | Start
  Telnet server access | Allow only VLAN #1
  SSH server status | Do not start
  TFTP server status | Do not start
  HTTP server status | Start
  HTTP server access | Allow only VLAN #1
  Secure HTTP server status | Do not start
  Maintenance VLAN | VLAN interface | VLAN #1
  Interface control | Link aggregation | None
  Port authentication | Disabled
  Port security | Disabled
  PoE supply | SWX2320-30MC: - SWX2322P-30MC: Enabled
  Layer 2 functions | Automatic MAC address acquisition | Enabled
  Automatic MAC address acquisition aging time | 300 sec
  Spanning tree | Enabled
  Unique Loop Detection | Disabled
  Multiple VLAN | None
  Multiple VLAN YMPI frame transmission | Disabled
  Layer 3 functions | Static routing | None
  Routing between VLANs | Disabled
  Policy-based routing | -
  OSPF | -
  RIP | -
  VRRP | -
  IP multicast | IGMP snooping | Disabled
  MLD snooping | Disabled
  IGMP | -
  PIM | -
  DNS client | Action | Enabled
  Traffic control | QoS | Disabled
  QoS (DSCP - Transmission queue ID conversion table) | None
  Flow control (IEEE 802.3x) | Disabled
  ACL | None
  AP layer functionality | DHCP server | -
  DHCPv6 server | -
  DHCP relay | -
  DNS relay | -
  RADIUS server | Disabled
  WebGUI | Language setting | Japanese
  Buzzer | Action | Disabled
  Buzzer trigger | All disabled

- Default settings for each LAN/SFP port

  Category | Setting Parameter | Setting value
  --- | --- | ---
  Basic settings | Speed/communication mode setting | auto
  Cross/straight automatic detection | Enabled
  MRU | 1,522 Byte
  Port description | None
  EEE | Disabled
  Port Mode | Access
  Associated VLAN ID | 1 (default VLAN)
  L2MS | L2MS filter | Disabled
  L2 switching | Spanning tree | Enabled
  Unique Loop Detection | Enabled
  Traffic control | QoS trust mode | CoS
  Flow control (IEEE 802.3x) | Disabled
  Storm Control | Disabled
  LLDP agent | Transmit/receive mode | Transmit and receive
  Basic management TLVs | Enabled
  PoE supply | Power supply actions | SWX2320-30MC: - SWX2322P-30MC: Enabled
  PoE power priority | SWX2320-30MC: - SWX2322P-30MC: Low

- Settings for default VLAN (vlan1)

  Category | Setting Parameter | Setting value
  --- | --- | ---
  Layer 3 functions | IPv4 address | 192.168.100.240/24
  IP multicast | Multicast frame forwarding | 239.192.128.250 (for Y-UNOS)
  IGMP Snooping | Action | Disabled
  Querier | Disabled
  Fast-Leave | Disabled
  Check TTL | Enabled
  Check RA | Disabled
  Check ToS | Disabled
  Report-Suppression | Enabled
  Report-Foward | Disabled
  Mrouter-Port Data-Suppression | Disabled
  MLD Snooping | Action | Disabled
  Querier | Disabled
  Fast-Leave | Disabled
  Report-Suppression | Enabled

Search result
No more search results.
There are no topics that match your search query.