# Tag VLAN

## 1. Summary

In this page you can make settings for tagged VLANs.

## 2. Top page

This is the top page for tagged VLANs.

### 2.1. Tag VLAN settings

- The various settings for tagged VLANs are shown for each LAN/SFP port and logical interface

  - "Frame types that can be received" isdisplayed according to the operating mode and the VLAN settings. (Thisitem cannot be set in the settings page.)

- Press the "Setting" button to access a page where you can change the settings for the tagged VLAN of the selected interface

- If you press the "Specify all" button, thesettings can be changed for all LAN/SFP ports and logical interfaceswhose check box contains a check mark

- If you press the "Return to defaults" button,the settings will be initialized for all LAN/SFP ports and logicalinterfaces whose check box contains a check mark.

  - Default settings for a tagged VLAN are as follows

    - Operating mode: Access

    - Assigned VLAN: Default VLAN (VLAN ID == 1)

- Settings for the LAN/SFP port assigned to a private VLAN cannot be changed

- Settings for the LAN/SFP port assigned to a voice VLAN cannot be changed

- If the operation mode is "Trunk," both the native VLAN and the trunk VLAN are shown as assigned VLANs.

## 3. Tagged VLAN settings page

In this page you can make various settings related to tagged VLANs.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

### 3.1. Tag VLAN settings

- Port

  - The LAN/SFP port or logical interface for which settings are made is shown

- Operation mode

  - Access

    - The corresponding port is specified as the access (untagged) port

  - Trunk

    - The corresponding port is specified as the trunk (tagged) port

- AccessVLAN

  - This item is shown only if the operating mode is "Access".

  - From the list, select the access port’s assigned VLAN

  - However, the following cannot be selected as access VLAN.

    - PrivateVLAN

    - VoiceVLAN

    - VLAN for which frame forwarding is invalid

- NativeVLAN

  - This item is shown only if the operating mode is "Trunk".

  - From the list, select the assignment-destination VLAN (native VLAN) for untagged frames received from the trunk port.

  - However, the following cannot be selected as native VLAN.

    - VLAN selected as trunk VLAN

    - PrivateVLAN

    - VoiceVLAN

    - VLAN for which frame forwarding is invalid

- TrunkVLAN

  - This item is shown only if the operating mode is "Trunk".

  - Specify the assignment-destination VLAN (trunk VLAN) for tagged frames received at the trunk port.

  - When you press the "Select" button, a list of the selectable VLAN IDs appears in a separate window

  - However, the following cannot be selected as trunk VLAN.

    - VLAN selected as native VLAN

    - PrivateVLAN

    - VoiceVLAN

    - VLAN for which frame forwarding is invalid

  - Place a check mark in the check box of the VLAN ID that you want to specify, and press the "OK" button

- Ingress filter

  Select the ingress filter from the following items. This item is shown only if the operating mode is "Trunk."

  - Enabled ( Receive only if the VLAN ID of the incoming frame is the same as the associated VLAN )

  - Disabled ( Receive all frames )

Search result
No more search results.
There are no topics that match your search query.