# Presets

## 1. Function Overview

This product allows you to easily configure optimal settings for AVoIP networks on which to transmit audio and video traffic such as Dante and NDI by using just a single DIP switch.
Simple presets are available to suit each network environment, and you can configure and switch settings without having to log in to the product.

- Presets

  - Dante / Dante AV

  - NDI

  - SDVoE

  - ADECIA

  - Extron NAV

  - IPMX

  - SMPTE ST 2110

- DIP switch on the back of this product

### 1.1. DIP switch settings

The function assignment of the DIP switch is as shown below. Set the switch according to your network environment.

- Function assignment of DIP switch

  DIP switch | Function | Factory default setting
  --- | --- | ---
  #1 | Preset type | OFF
  #2 | OFF
  #3 | OFF
  #4 | OFF
  #5 | - | OFF
  #6 | - | OFF
  #7 | Enable/disable the L2MS function | ON
  #8 | LED on/off | ON

- DIP switch #1 to #4 settings
  Specifies the preset type.
  If you do not need settings specific to the AVoIP network environment, specify Normal, which applies the basic settings of the switch.

  DIP switch | Preset type | Content
  --- | --- | ---
  #1 | #2 | #3 | #4
  OFF | OFF | OFF | OFF | Normal | Basic settings of the switch
  ON | OFF | OFF | OFF | Dante type A | Dante optimal settings (Basic settings)
  OFF | ON | OFF | OFF | Dante type B | Dante optimal settings (Basic settings + Trunk port)
  ON | ON | OFF | OFF | Dante type C | Dante optimal settings (Basic settings + L2MS/BPDU filter)
  OFF | OFF | ON | OFF | ADECIA | Settings for ADECIA linkage
  ON | OFF | ON | OFF | NDI | NDI optimal settings
  OFF | ON | ON | OFF | SDVoE | SDVoE optimal settings
  ON | ON | ON | OFF | IPMX | IPMX optimal settings
  OFF | OFF | OFF | ON | SMPTE ST 2110 (PTP TC) | SMPTE ST 2110 (PTP TC) optimal settings
  ON | OFF | OFF | ON | Extron NAV | Extron NAV optimal settings

In addition to the above presets, you can also use the DIP switch to select the operations of the L2MS function and LED illumination.

- DIP switch #7 setting
  Enables or disables the L2MS function. This setting will be reflected when a preset other than Normal is applied.

  DIP switch #7 | Function
  --- | ---
  ON | Enables the L2MS function
  OFF | Disables the L2MS function

- DIP switch #8 setting
  Specifies whether to turn on or off the LED. This setting will be reflected when a preset other than Normal is applied.

  DIP switch #8 | Function
  --- | ---
  ON | Turns on the LED
  OFF | Turns off the LED

## 2. Definition of Terms Used

- Dante
  Dante is a professional audio networking solution developed by Audinate, Inc.
  A single LAN cable can be used to carry out bidirectional communication of all the information required for a digital audio system, such as multi-channel audio transmission, clock synchronization signals, and control signals.
  Dante AV is a solution that expands Dante technology to video signals, enabling video and audio to be transmitted synchronously over the same network.
  This enables flexible system construction using AV over IP.

- NDI
  NDI is a new protocol developed by Newtek, Inc. to support live video production workflows over IP.
  It enables real-time interactive transmission of video, audio, meta data, and other information within typical Gigabit Ethernet environments.

- SDVoE
  SDVoE (Software Defined Video over Ethernet) is an international standard for the professional audio/video (ProAV) market that can transmit 4K high-definition video and audio over 10 Gigabit communication.
  By combining SDVoE encoders/decoders and controllers with a 10 Gigabit switch, video walls and multi-view systems can be configured.

- ADECIA
  ADECIA is Yamaha’s one-stop sound solution for teleconferences, and is a sound system that includes a complete set of microphones and speakers, ideal for rooms and classrooms where teleconferences and lessons are held.

- IPMX
  IPMX is an AV over IP open standard for the ProAV market, proposed by AIMS (Alliance for IP Media Solutions).
  It is based on SMPTE ST 2110 used in broadcasting industry and incorporate necessary functions for AV equipment such as HDMI, EDID and HDCP. Its aim is to increase interoperability and simplified implementation.
  It can transmit uncompressed or lightly compressed video, audio or control signal with low delay within standard 1GbE or 10GbE network.

- SMPTE ST 2110
  SMTE ST 2110 is an IP-based broadcast media transmission standard developed by SMPTE (Society of Motion Picture and Television Engineers).
  By IP packetizing and transmitting video (ST 2110-20), audio (ST 2110-30), and ancillary data (ST 2110-40) separately, it allows for flexible handling and synchronization on the network.
  It has achieved high quality uncompressed transmission and extremely low delay process, so it has become industry standard in studio equipment transition to IP based.

## 3. Preset setting and switching

### 3.1. About preset setting and switching

For setting or switching the preset, the system checks the DIP switch status at startup and selects the appropriate preset.
Note that you can only switch the preset when starting up the product in the factory default state (without saving any settings). If any settings are saved on the device unit, the unit will start up with the saved settings.
Before switching the preset, be sure to reset this product to its factory default settings. For instructions on how to reset the product to the factory default settings, refer to How to reset to the factory default settings.

### 3.2. Example of preset switching procedure

1. Turn off this product

2. Change the DIP switch to the preset you want to use

3. Turn on this product while holding down the initialization button on the back of the product
   Initialization will begin by holding down the initialization button for approximately 10 seconds.
   During initialization, the port LED on the front of the product will illuminate orange. Then, the product will start up with the selected preset.

## 4. Preset Details

### 4.1. Dante preset

The Dante preset is a setting optimized for Dante, and it applies the following commands.

- List of commands applied by the Dante preset

  Object of setting | Function | Commands
  --- | --- | ---
  Entire system | Disable flow control | flowcontrol disable
  Enable QoS | qos enable
  Optimize transmission queue by DSCP value | qos dscp-queue 8 2
  qos dscp-queue 26 3
  qos dscp-queue 34 4
  qos dscp-queue 46 5
  qos dscp-queue 48 5
  qos dscp-queue 56 7
  qos dscp-queue [not indicated above] 0
  Always forward linked local multicasts | l2-unknown-mcast forward link-local
  Enable LLDP | lldp run
  Enable PTP | ptp enable
  VLAN interface | Set an IP address (*VLAN1 only) | ip address dhcp auto-ip enable
  Flood unknown multicasts | l2-unknown-mcast flood
  Always forward PTP packets | l2-mcast flood 224.0.1.129
  l2-mcast flood 224.0.1.130
  l2-mcast flood 224.0.1.131
  l2-mcast flood 224.0.1.132
  l2-mcast flood 239.254.3.3
  Enable IGMP snooping | ip igmp snooping enable
  Set IGMP snooping version | ip igmp snooping version 3
  Enable IGMP snooping fast-leave function | ip igmp snooping fast-leave auto-assignment
  Enable IGMP query transmission function | ip igmp snooping querier
  Set IGMP query transmission interval | ip igmp snooping query-interval 30
  Disable IGMP report-suppression function | ip igmp snooping report-suppression disable
  Enable IGMP report forwarding function | ip igmp snooping report-forward enable
  Disable IGMP packet TTL value checking function | ip igmp snooping check ttl disable
  Disable IGMP packet RA checking function | ip igmp snooping check ra disable
  Disable IGMP packet ToS checking function | ip igmp snooping check tos disable
  Enable data transfer suppression function for multicast router ports | ip igmp snooping mrouter-port data-suppression enable
  LAN/SFP port | Disable flow control | flowcontrol disable
  Set the MRU | mru 1522
  Set QoS trust mode to DSCP | qos trust dscp
  Set L2MS filter | l2ms filter disable / enable
  Set BPDU filter | spanning-tree bpdu-filter disable / enable
  Disable EEE | eee disable
  Enable LLDP transmission and reception | set lldp enable txrx
  Send LLDP basic management TLVs | tlv-select basic-mgmt
  Enable PTP | ptp enable

- LAN/SFP port settings by type

  Port | Dante type A | Dante type B | Dante type C
  --- | --- | --- | ---
  Access / Trunk | VLAN | L2MS/BPDU filter | Access / Trunk | VLAN | L2MS/BPDU filter | Access / Trunk | VLAN | L2MS/BPDU filter
  1,3,5,7,9,11,13,15,17,19,21,23 | Access | 1 | disable | Access | 1 | disable | Access | 1 | disable
  2,4,6,8,10,12,14,16,18,20,22,24 | Access | 1 | disable | Access | 2 | disable | Access | 2 | enable
  25,27,29 | Access | 1 | disable | Trunk | 1 (untag) , 2 (tag) | disable | Access | 1 | disable
  26,28,30 | Access | 1 | disable | Trunk | 1 (untag) , 2 (tag) | disable | Access | 2 | enable

### 4.2. ADECIA preset

The ADECIA preset is a setting optimized for ADECIA linkage, and it applies the following commands.

- List of commands applied by the ADECIA preset

  Object of setting | Function | Commands
  --- | --- | ---
  Entire system | Disable flow control | flowcontrol disable
  Enable QoS | qos enable
  Optimize transmission queue by DSCP value | qos dscp-queue 8 2
  qos dscp-queue 26 3
  qos dscp-queue 34 4
  qos dscp-queue 46 5
  qos dscp-queue 48 5
  qos dscp-queue 56 7
  qos dscp-queue [not indicated above] 0
  Always forward linked local multicasts | l2-unknown-mcast forward link-local
  Enable LLDP | lldp run
  Disable PTP | ptp disable
  Enable the Y-UNOS function | y-unos enable
  Generate a root certificate authority for the local RADIUS server | crypto pki generate ca
  VLAN interface | Set an IP address (*VLAN1 only) | ip address dhcp auto-ip enable
  Flood unknown multicasts | l2-unknown-mcast flood
  Always forward PTP packets | l2-mcast flood 224.0.1.129
  l2-mcast flood 224.0.1.130
  l2-mcast flood 224.0.1.131
  l2-mcast flood 224.0.1.132
  l2-mcast flood 239.254.3.3
  Forward control frames for the Y-UNOS function | l2-mcast flood 239.192.128.250
  Enable IGMP snooping | ip igmp snooping enable
  Set IGMP snooping version | ip igmp snooping version 3
  Enable IGMP snooping fast-leave function | ip igmp snooping fast-leave auto-assignment
  Enable IGMP query transmission function | ip igmp snooping querier
  Set IGMP query transmission interval | ip igmp snooping query-interval 30
  Disable IGMP report-suppression function | ip igmp snooping report-suppression disable
  Enable IGMP report forwarding function | ip igmp snooping report-forward enable
  Disable IGMP packet TTL value checking function | ip igmp snooping check ttl disable
  Disable IGMP packet RA checking function | ip igmp snooping check ra disable
  Disable IGMP packet ToS checking function | ip igmp snooping check tos disable
  Enable data transfer suppression function for multicast router ports | ip igmp snooping mrouter-port data-suppression enable
  LAN/SFP port | Disable flow control | flowcontrol disable
  Set the MRU | mru 1522
  Set QoS trust mode to DSCP | qos trust dscp
  Disable L2MS filter | l2ms filter disable
  Disable BPDU filter | spanning-tree bpdu-filter disable
  Disable EEE | eee disable
  Enable LLDP transmission and reception | set lldp enable txrx
  Send LLDP basic management TLVs | tlv-select basic-mgmt
  Send LLDP IEEE-802.3 TLVs | tlv-select ieee-8023-org-specific
  Disable PTP | ptp disable

### 4.3. NDI preset

The NDI preset is a setting optimized for NDI, and it applies the following commands.

- List of commands applied by the NDI preset

  Object of setting | Function | Commands
  --- | --- | ---
  Entire system | Enable flow control | flowcontrol enable
  Disable QoS | qos disable
  Always forward linked local multicasts | l2-unknown-mcast forward link-local
  Enable LLDP | lldp run
  Disable PTP | ptp disable
  VLAN interface | Set an IP address | ip address dhcp auto-ip enable
  Flood unknown multicasts | l2-unknown-mcast flood
  Enable IGMP snooping | ip igmp snooping enable
  Set IGMP snooping version | ip igmp snooping version 2
  Enable IGMP snooping fast-leave function | ip igmp snooping fast-leave auto-assignment
  Enable IGMP query transmission function | ip igmp snooping querier
  Set IGMP query transmission interval | ip igmp snooping query-interval 125
  Disable IGMP report-suppression function | ip igmp snooping report-suppression disable
  Enable IGMP report forwarding function | ip igmp snooping report-forward enable
  Disable IGMP packet TTL value checking function | ip igmp snooping check ttl disable
  Disable IGMP packet RA checking function | ip igmp snooping check ra disable
  Disable IGMP packet ToS checking function | ip igmp snooping check tos disable
  Enable data transfer suppression function for multicast router ports | ip igmp snooping mrouter-port data-suppression enable
  LAN/SFP port | Enable flow control | flowcontrol both
  Set the MRU | mru 1522
  Disable L2MS filter | l2ms filter disable
  Disable BPDU filter | spanning-tree bpdu-filter disable
  Disable EEE | eee disable
  Enable LLDP transmission and reception | set lldp enable txrx
  Send LLDP basic management TLVs | tlv-select basic-mgmt
  Disable PTP | ptp disable

### 4.4. SDVoE preset

The SDVoE preset is a setting optimized for SDVoE, and it applies the following commands.

- List of commands applied by the SDVoE preset

  Object of setting | Function | Commands
  --- | --- | ---
  Entire system | Disable flow control | flowcontrol disable
  Disable QoS | qos disable
  Always forward linked local multicasts | l2-unknown-mcast forward link-local
  Enable LLDP | lldp run
  Disable PTP | ptp disable
  VLAN interface | Set an IP address | ip address dhcp auto-ip enable
  Discard unknown multicasts | l2-unknown-mcast discard
  Enable IGMP snooping | ip igmp snooping enable
  Set IGMP snooping version | ip igmp snooping version 2
  Enable IGMP snooping fast-leave function | ip igmp snooping fast-leave auto-assignment
  Enable IGMP query transmission function | ip igmp snooping querier
  Set IGMP query transmission interval | ip igmp snooping query-interval 60
  Disable IGMP report-suppression function | ip igmp snooping report-suppression disable
  Enable IGMP report forwarding function | ip igmp snooping report-forward enable
  Disable IGMP packet TTL value checking function | ip igmp snooping check ttl disable
  Disable IGMP packet RA checking function | ip igmp snooping check ra disable
  Disable IGMP packet ToS checking function | ip igmp snooping check tos disable
  Enable data transfer suppression function for multicast router ports | ip igmp snooping mrouter-port data-suppression enable
  LAN/SFP port | Disable flow control | flowcontrol disable
  Set the MRU | mru 9216
  Disable L2MS filter | l2ms filter disable
  Disable BPDU filter | spanning-tree bpdu-filter disable
  Disable EEE | eee disable
  Enable LLDP transmission and reception | set lldp enable txrx
  Send LLDP basic management TLVs | tlv-select basic-mgmt
  Disable PTP | ptp disable

### 4.5. IPMX preset

The IPMX preset is a setting optimized for IPMX, and it applies the following commands.

- List of commands applied by the IPMX preset

  Object of setting | Function | Commands
  --- | --- | ---
  Entire system | Disable flow control | flowcontrol disable
  Disable QoS | qos disable
  Always forward linked local multicasts | l2-unknown-mcast forward link-local
  Enable LLDP | lldp run
  Enable PTP | ptp enable
  VLAN interface | Set an IP address | ip address dhcp auto-ip enable
  Flood unknown multicasts | l2-unknown-mcast flood
  Enable IGMP snooping | ip igmp snooping enable
  Set IGMP snooping version | ip igmp snooping version 3
  Enable IGMP snooping fast-leave function | ip igmp snooping fast-leave auto-assignment
  Enable IGMP query transmission function | ip igmp snooping querier
  Set IGMP query transmission interval | ip igmp snooping query-interval 125
  Disable IGMP report-suppression function | ip igmp snooping report-suppression disable
  Enable IGMP report forwarding function | ip igmp snooping report-forward enable
  Disable IGMP packet TTL value checking function | ip igmp snooping check ttl disable
  Disable IGMP packet RA checking function | ip igmp snooping check ra disable
  Disable IGMP packet ToS checking function | ip igmp snooping check tos disable
  Enable data transfer suppression function for multicast router ports | ip igmp snooping mrouter-port data-suppression enable
  LAN/SFP port | Disable flow control | flowcontrol disable
  Set the MRU | mru 1522
  Disable L2MS filter | l2ms filter disable
  Disable BPDU filter | spanning-tree bpdu-filter disable
  Disable EEE | eee disable
  Enable LLDP transmission and reception | set lldp enable txrx
  Send LLDP basic management TLVs | tlv-select basic-mgmt
  Enable PTP | ptp enable

### 4.6. SMPTE ST 2110 preset

The SMPTE ST 2110 preset is a setting optimized for SMPTE ST 2110 (PTP TC), and it applies the following commands.

- List of commands applied by the SMPTE ST 2110 preset

  Object of setting | Function | Commands
  --- | --- | ---
  Entire system | Disable flow control | flowcontrol disable
  Disable QoS | qos disable
  Always forward linked local multicasts | l2-unknown-mcast forward link-local
  Enable LLDP | lldp run
  Enable PTP | ptp enable
  VLAN interface | Set an IP address | ip address dhcp auto-ip enable
  Discard unknown multicasts | l2-unknown-mcast discard
  Enable IGMP snooping | ip igmp snooping enable
  Set IGMP snooping version | ip igmp snooping version 3
  Enable IGMP snooping fast-leave function | ip igmp snooping fast-leave auto-assignment
  Enable IGMP query transmission function | ip igmp snooping querier
  Set IGMP query transmission interval | ip igmp snooping query-interval 125
  Disable IGMP report-suppression function | ip igmp snooping report-suppression disable
  Enable IGMP report forwarding function | ip igmp snooping report-forward enable
  Disable IGMP packet TTL value checking function | ip igmp snooping check ttl disable
  Disable IGMP packet RA checking function | ip igmp snooping check ra disable
  Disable IGMP packet ToS checking function | ip igmp snooping check tos disable
  Enable data transfer suppression function for multicast router ports | ip igmp snooping mrouter-port data-suppression enable
  LAN/SFP port | Disable flow control | flowcontrol disable
  Set the MRU | mru 1522
  Disable L2MS filter | l2ms filter disable
  Disable BPDU filter | spanning-tree bpdu-filter disable
  Disable EEE | eee disable
  Enable LLDP transmission and reception | set lldp enable txrx
  Send LLDP basic management TLVs | tlv-select basic-mgmt
  Enable PTP | ptp enable

### 4.7. Extron NAV preset

The Extron NAV preset is a setting optimized for Extron NAV, and it applies the following commands.

- List of commands applied by the Extron NAV preset

  Object of setting | Function | Commands
  --- | --- | ---
  Entire system | Disable flow control | flowcontrol disable
  Disable QoS | qos disable
  Always forward linked local multicasts | l2-unknown-mcast forward link-local
  Enable LLDP | lldp run
  Disable PTP | ptp disable
  VLAN interface | Set an IP address | ip address dhcp auto-ip enable
  Discard unknown multicasts | l2-unknown-mcast discard
  Always forward PTP packets | l2-mcast flood 224.0.1.129
  l2-mcast flood 224.0.1.130
  l2-mcast flood 224.0.1.131
  l2-mcast flood 224.0.1.132
  l2-mcast flood 239.254.3.3
  Enable IGMP snooping | ip igmp snooping enable
  Set IGMP snooping version | ip igmp snooping version 2
  Enable IGMP snooping fast-leave function | ip igmp snooping fast-leave auto-assignment
  Enable IGMP query transmission function | ip igmp snooping querier
  Set IGMP query transmission interval | ip igmp snooping query-interval 125
  Disable IGMP report-suppression function | ip igmp snooping report-suppression disable
  Enable IGMP report forwarding function | ip igmp snooping report-forward enable
  Disable IGMP packet TTL value checking function | ip igmp snooping check ttl disable
  Disable IGMP packet RA checking function | ip igmp snooping check ra disable
  Disable IGMP packet ToS checking function | ip igmp snooping check tos disable
  Enable data transfer suppression function for multicast router ports | ip igmp snooping mrouter-port data-suppression enable
  LAN/SFP port | Disable flow control | flowcontrol disable
  Set the MRU | mru 1522
  Disable L2MS filter | l2ms filter disable
  Disable BPDU filter | spanning-tree bpdu-filter disable
  Disable EEE | eee disable
  Enable LLDP transmission and reception | set lldp enable txrx
  Send LLDP basic management TLVs | tlv-select basic-mgmt
  Disable PTP | ptp disable

## 5. Checking the Status of the DIP Switch

To check the current status of the DIP switch, you can use the show dipsw command, or you can check the status on the WebGUI dashboard screen.
If you log in to this product via the console or WebGUI, some settings will automatically be saved and will no longer be in the factory default settings.

- Example of executing the show dipsw command

      Yamaha>show dipsw
      [Startup status]
         DIPSW  |   1   2   3   4   5   6   7   8
      --------------------------------------------
         Status | OFF OFF OFF OFF OFF OFF  ON  ON
      --------------------------------------------
           Preset type : Normal
           L2MS        : ON
           LED         : ON

      [Current status]
         DIPSW  |   1   2   3   4   5   6   7   8
      --------------------------------------------
         Status | OFF OFF OFF OFF OFF OFF  ON  ON
      --------------------------------------------
           Preset type : Normal
           L2MS        : ON
           LED         : ON

## 6. Related Commands

Related commands are indicated below.
For details, refer to the Command Reference.

Operations | Operating commands
--- | ---
Show the status of the DIP switch | show dipsw

## 7. Points of Caution

- The presets are intended for use when this product is used as a switch dedicated to the AVoIP network.
  The presets provided are merely simplified settings and cannot be changed. To change the settings, you must log in to this product via the console or WebGUI, and configure the settings appropriately.

- To apply the presets, this product must be in the factory default settings.

- If you log in to the this product via the console or WebGUI, the settings will automatically be saved by changing the login password or other actions, and the product will no longer be in the factory default settings.

- If the password for the default administrative user is the default value, there are some access restrictions. For details, refer to Login Security and User Account Management.

- The preset is applied according to the status of the DIP switch at startup. Therefore, the preset will not switch even if the DIP switch is changed after startup.

- The presets cannot be used when the stack function is enabled.

## 8. Related Documentation

- ProAV Settings

- Login Security

- User Account Management

## 9. Trademarks and Trade Names

- Dante™ is a registered trademark of Audinate Pty Ltd.

- NDI® is a registered trademark of Vizrt NDI AB.

- SDVoE™ and the SDVoE logo are trademarks of the SDVoE Alliance.

- Extron is a registered trademark of RGB Systems, Inc.

- IPMX™ is a trademark of the AIMS Alliance (Alliance for IP Media Solutions).

- SMPTE® ST 2110 is a standard and trademark of the SMPTE (Society of Motion Picture and Television Engineers).

Search result
No more search results.
There are no topics that match your search query.