# Server settings

## 1. Summary

This page is for performing operations related to the certificate authority and RADIUS server.

## 2. Top page

This is the top page for the RADIUS server.

### 2.1. Certificate authority management

- Press the “Next” button to the right of “Create certificate authority” to begin the process of creating a certificate authority.

- Press the “Next” button to the right of “Delete certificate authority” to begin the process of deleting the certificate authority.

- Press the “Next” button to the right of “Backup/restoration files and settings related to certificate authority” to begin the process of backing up or restoring.

### 2.2. RADIUS server settings

- Displays the settings for the RADIUS server.

- The table items are explained below.

  - RADIUS server usage

    - Displays whether a RADIUS server is to be used or not.

    - If a RADIUS server is to be used, the port number will be displayed.

  - Interfaces that can access the RADIUS server

    - Displays the interfaces that can access the RADIUS server.

  - Reauthentication interval configured for authenticator

    - Displays the settings for the reauthentication interval configured on the authenticator by the RADIUS server.

  - Authentication method

    - Displays the authentication method settings used by the RADIUS server.

### 2.3. RADIUS client list

- Displays the RADIUS client settings.

- The table items are explained below.

  - Check box

    - Select the check box to delete the RADIUS client settings.

  - IP address

    - Displays the RADIUS client address.

- A maximum of 20 items can be displayed for one page. You can move between pages by pressing or , or by entering a number.

- Press the sort switch to sort by each item.

- Press the “New” button to access a page where you can configure the settings for a new RADIUS client.

- Press the “Setting” button to access a page where you can change the selected RADIUS client settings.

- Press the “Delete” button to delete all RADIUS clients whose check boxes are selected.

- On this page, you can configure up to 100 RADIUS clients.

## 3. Certificate authority creation page

This is the certificate authority creation page.
Enter the certificate authority name, and then press the "Confirm" button.
If there are no mistakes in the input content confirmation screen, press the "OK" button.
If a certificate authority already exists, you will not be able to create a certificate authority.

### 3.1. Create a certificate authority

- Name

  - Specifies the certificate authority name.

  - Enter 3 to 32 characters using single-byte alphanumeric characters excluding ‘\’, ‘[’, ‘]’, ‘/’, ‘"’, ‘?’, and spaces

  - You cannot set the name as DEFAULT.

  - If this is omitted, the name swx-radius will be automatically set.

## 4. Certificate authority deletion page

This is the certificate authority deletion page.
Press the "OK" button to delete the certificate authority.
Deleting the certificate authority will delete all RADIUS-related settings, certificates and so on.

## 5. Backup / Restoration page

This page is for backup/restoration of settings related to certificate authorities.
Enter the contents, and then press the "Confirm" button.
If there are no mistakes in the input content confirmation screen, press the "OK" button.
The following files and settings will be backed up and restored.

- Certificate authority

- Various certificates

- RADIUS client settings

- RADIUS user settings

### 5.1. Backup / Restoration

- Content to execute

  - Select below whether a content to execute.

    - Backup

    - Restoration

    - Import the backup file of a Yamaha wireless AP

- File to restore

  - Press the "Select a file" button to specify the file to restore.

  - When "Import the backup file of a Yamaha wireless AP" is selected, specify the file backed up on WLX402 or WLX313.

- zip file password

  - Enter up to 32 single-byte alphanumeric characters/symbols, with the following exceptions: # & ^ \ ; | ` { }

  - When backing up, enter the password set for the backup file.

  - When restoring or importing the backup file of a Yamaha wireless AP, enter the password set for the backup file when it was backed up.

    - When using a file without a password, restore or import successfully with or without input of password.

## 6. RADIUS server settings page

In this page you can configure the settings for a RADIUS server.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

### 6.1. RADIUS server settings

- RADIUS server usage

  - Select below whether a RADIUS server will be used.

    - Use

    - Don’t use

  - When Use is selected, specify the port number.

  - Input a port number from 1024 to 65535.

  - When Use is selected, a certificate authority is created when the settings are made, if one does not already exist.

- Interfaces that can access the RADIUS server

  - Press the "Select" button to display the "VLAN interface list" dialog box.

  - You can select the port check box in the "VLAN interface list" dialog box and press the "OK" button to select the associated interface.

  - Up to 7 VLAN interfaces can be selected.

- Reauthentication interval configured for authenticator

  - Select the reauthentication interval configured on the authenticator from the options below.

    - 3600 Seconds

    - 43200 Seconds

    - 86400 Seconds

    - 604800 Seconds

- Authentication method

  - Select the authentication method used by the RADIUS server from the methods below.

    - PAP

    - PEAP

    - EAP-MD5

    - EAP-TLS

    - EAP-TTLS

## 7. RADIUS client settings page

This page is for configuring the RADIUS client settings.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

### 7.1. RADIUS client settings

- IP address

  - Specifies the RADIUS client address.

  - Enter IPv4 addresses using the XXX.XXX.XXX.XXX format.

  - Enter IPv6 addresses using the XXXX:XXXX::XXXX.XXXX format.

  - When the settings are changed, the IP address of the selected RADIUS client will be displayed as text.

- Secret text string

  - Specifies the secret text string of the RADIUS client.

  - \ [ ] " ? Enter up to 128 single-byte alphanumeric characters/symbols, with the following exceptions: space

Search result
No more search results.
There are no topics that match your search query.