# PTP statistics

## 1. Summary

This page is for checking the PTP statistics.

You can check the PTP role for each port and the transmission and reception rate of various messages.

You can check the information only when the PTP operation mode is boundary clock.

## 2. Top page

This is the top page for the PTP statistics.

### 2.1. Statistics

- Displays the PTP statistics of this unit.

- Displays the following information when the PTP operation mode is boundary clock.

  - Port

    - Displays the interface name.

  - PTP function

    - Displays whether the PTP function for each port is enabled.

  - Role

    - Displays the PTP role (such as timeTransmitter or timeReceiver) for each port.

  - Announce (TX/RX)

    - Displays the transmission and reception rate of the Announce message.

  - Sync (TX/RX)

    - Displays the transmission and reception rate of the Sync message.

  - Follow Up (TX/RX)

    - Displays the transmission and reception rate of the Follow Up message.

  - Delay Request (TX/RX)

    - Displays the transmission and reception rate of the Delay Request message.

  - Delay Response (TX/RX)

    - Displays the transmission and reception rate of the Delay Response message.

  - Signaling (TX/RX)

    - Displays the transmission and reception rate of the Signaling message.

  - Management (TX/RX)

    - Displays the transmission and reception rate of the Management message.

  - Total (TX/RX)

    - Displays the total transmission and reception rate of each PTP message.

- Pressing the button will refresh the displayed content.

- This information is not displayed when the PTP operation mode is transparent clock or the PTP function is disabled.

Search result
No more search results.
There are no topics that match your search query.