# Routing

## 1. Summary

This page is for configuring the routing settings.

## 2. Top page

This is the top page for routing.

### 2.1. Routing function basic settings

- The current settings for the routing function are shown.

- When you press the "Setting" button, a page where you can change the routing function settings will appear.

### 2.2. Routing table

- Displays the routing table details.

- The table items are explained below.

  - Check box

    - Select the check box to delete static route information.

  - Enabled route

    - For the route used in actual communications, Enabled will be displayed.

    - For the routes not used for actual communications, Disabled will be displayed.

  - Type

    - Displays one of the following route information types.

      - static

      - connected

  - Destination

    - Displays the destination network address for the route information.

    - If the destination is a default gateway, default will be displayed.

  - Gateway

    - Displays the route information gateway.

    - Null is displayed for settings to discard packets.

  - Priority

    - Displays the administrative distance for route information.

- Press the "New" button to display a page where you can create new settings for static route information.

- Press the "Setting" button to display a page where you can change the settings for the selected static route information.

- If you press the "Delete" button, all static route information for which the check boxes are selected will be deleted.

- A check box and "Settings" button are displayed for the static route information entry.

- Up to 1024 static route information entries can be displayed.

  - When 1024 static route information entries are displayed, the "New" button is disabled.

## 3. Routing function basic setting page

In this page you can specify whether the routing function is used.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

### 3.1. Routing function basic settings

- Routing function

  Select the routing function from the following items.

  - Use routing function

  - Don’t use routing function

## 4. Static route information settings page

This page is for configuring the static route information settings.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

### 4.1. Set static route information

- Destination network

  - When configuring new settings

    - Select a destination network from the following networks.

      - Specifying a network address

        - Input the destination network address.

      - Default gateway

  - When changing settings

    - The destination network address is displayed.

- Gateway

  - Select from one of the following gateways.

    - Specifying an IP address

      - Input the gateway IP address.

    - Discarding a packet without forwarding

- Priority

  - Input the priority.

  - The input range is 1 - 255.

Search result
No more search results.
There are no topics that match your search query.