# Device list

### 1. Summary

In the device list you can view a list of the terminals and agentesmanaged in the LAN map, and use the terminal DB to centrally manageterminal information.

### 2. Terminal list

The terminal list page is explained here.

#### 2.1. Summary

The terminal list page shows a list of the terminals that are managed by the LAN map. You can use the list to check the time that a terminalwas detected or the time that it was lost. You can also edit terminalinformation in the list, or register it to the terminal DB.

#### 2.2. About the buttons

- "Delete" button

  Delete information of the selected lost terminal from the terminal list.

- "Refresh display" button

  Refresh the terminal list page.

- "Save as CSV" button

  Save the terminal list as a CSV file.

- "Edit" button

  Edit terminal information. Edited information is registered in the terminal DB.

#### 2.3. Checking terminal information

In the list you can check the terminal information that is managed by the LAN map. You can press each item’s Sort switch to sort the list. The initial screen is sorted in order of route. Lost terminals are shown highlighted in gray.

The VLAN ID item shows (A) for an access VLAN or (T) for a trunk VLAN.

If the port is being used as a port for a private VLAN, the VLAN ID is not shown, and (P) is shown.

If the port is being used as a port for a voice VLAN, the VLAN ID is not shown, and (V) is shown.

#### 2.4. Editing terminal information and registering it to the terminal DB

You can edit the information for the terminals that are managed bythe LAN map. Edited information is registered in the terminal DB. Pressthe "Edit" button of the terminal information that you want to edit, and then edit the information. You can edit the following items.

- Type

  Select the type from the selection menu.

  * This is shown as an icon in the map page and multiple VLAN page "Connected device view".

- Manufacturer

  Enter the manufacturer name.

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- Model name

  Enter the model name.

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- Device name

  Enter the device name.

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- OS

  Enter the OS name.

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- Comment

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- Snapshot

  Select whether the terminal is or is not included in monitoring for the snapshot function.

* Terminal information that has been registered can also be edited from the terminal DB page..

Note: When inputting """ or "," for parameters where text is inputted, the maximum number of allowable characters will be less than 128.

#### 2.5. Deleting a lost terminal

You can delete information of a lost terminal from the terminal list. Select the lost terminal information that you want to delete, and press the "Delete" button. The lost terminal information that you selected is deleted.

#### 2.6. Saving a list to a CSV file

You can save the terminal list as a CSV file. Press the "Save as CSV" button. The terminal list is saved as a CSV file.

### 3. Terminal DB

The terminal DB page is explained here.

#### 3.1. Summary

The terminal DB page shows a list of the terminals that areregistered in the terminal DB. You can newly register, edit, or deleteterminal information, and import or export terminal DB settings.

#### 3.2. About the buttons

- "Delete" button

  Delete the selected terminal information from the terminal DB.

- "Register new" button

  Newly register terminal information in the terminal DB.

- "Refresh display" button

  Refresh the terminal DB page display.

- "Import" button

  Apply the terminal DB saved on the PC to the manager.

- "Export" button

  Save the terminal DB as a CSV file.

- "Edit" button

  You can edit the terminal information that has been registered in the terminal DB.

#### 3.3. Checking terminal information

You can identify the terminal DB in the list. You can press each item’s Sort switch to sort the list. The initial screen is sorted in order of MAC address.

#### 3.4. Registering new terminal information

You can newly register terminal information in the terminal DB. Press the "Register new" button, and enter the content to be registered. You can register the following items.

- MAC address

  Enter the MAC address of the terminal.

  Enter single-byte characters delimited by a ":" (example: 00:a0:de:00:00:00).

- Type

  Select the type from the selection menu.

  * This is shown as an icon in the map page and multiple VLAN page "Connected device view".

- Manufacturer

  Enter the manufacturer name.

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- Model name

  Enter the model name.

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- Device name

  Enter the device name.

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- OS

  Enter the OS name.

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- Comment

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- Snapshot

  Select whether the terminal is or is not included in monitoring for the snapshot function.

#### 3.5. Editing terminal information

You can edit the terminal information that has been registered in the terminal DB. Press the "Edit" button of the terminal information that you want to edit, and then edit the information. You can edit the following items.

- Type

  Select the type from the selection menu.

  * This is shown as an icon in the map page and multiple VLAN page "Connected device view".

- Manufacturer

  Enter the manufacturer name.

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- Model name

  Enter the model name.

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- Device name

  Enter the device name.

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- OS

  Enter the OS name.

  Enter up to 128 single-byte alphanumeric characters or single-byte symbols.

- Comment

- Snapshot

  Select whether the terminal is or is not included in monitoring for the snapshot function.

#### 3.6. Deleting terminal information

You can delete the selected terminal information from the terminalDB. Select the terminal that you want to delete, and press the "Delete" button. The selected terminal information is deleted.

#### 3.7. Importing a terminal DB

Apply the terminal DB saved on the PC to the manager. Press the "Import" button, and use the "Select a file" button to select the terminal DB. The selected terminal DB is applied to the manager.

When directly editing the terminal DB, use no more than 128 single-byte alphanumeric or symbol characters for each item.

A character string that includes multi-byte characters is detected as an empty character string, and a character string that exceeds 128characters is truncated at 128 characters.

#### 3.8. Exporting a terminal DB

You can save the terminal DB as a CSV file. Press the "Export" button. The terminal DB is saved as a CSV file.

### 4. Agent list

The agent list page is explained here.

#### 4.1. Summary

The agent list page shows a list of the agentes that are managed bythe LAN map. You can use the list to check the time that a agent wasdetected or the time that it was lost. You can also change the settingsof a agent in the list.

#### 4.2. About the buttons

- "Delete" button

  Delete information of the selected lost agent from the agent list.

- "Refresh display" button

  Refresh the agent list page display.

- "Save as CSV" button

  Save the agent list as a CSV file.

- "Settings" button

  Make agent settings.

#### 4.3. Checking a agent

In the list you can check the agent information that is managed by the LAN map. You can press each item’s Sort switch to sort the list. The initial screen is sorted in order of route. Lost agentes are shown highlighted in gray.

#### 4.4. Making agent settings

You can edit the settings for the agentes that are managed by the LAN map. Settings can be changed on some Yamaha switches. Press the "Settings" button of the agent whose settings you want to change, and then change the settings. You can set the following items.

- Device name

  Specify the device name of the agent.

  - When "Default device name" is selected, the default names that are predetermined for each device will be set. Normally, this is textthat shows the model name and serial number.

  - When "Manual settings" is selected, the device name that wasinputted in the input box right afterwards will be set. Input a devicename of up to 32 single-byte characters. The characters that can beinput will differ depending on the target agent. See "6-2. Setting and maintaining switches" in "Map" fordetails.

#### 4.5. Deleting a lost agent

You can delete information of a lost agent from the agent list.Select the lost agent information that you want to delete, and press the "Delete" button. The lost agent information that you selected is deleted.

#### 4.6. Saving a list to a CSV file

You can save the agent list as a CSV file. Press the "Save as CSV" button. The agent list is saved as a CSV file.

Search result
No more search results.
There are no topics that match your search query.