# Basic settings

### 1. Summary

This page is for configuring the basic settings.

### 2. Top page

This is the top page for the basic settings.

#### 2.1. IPv4 settings

- Shows the IPv4 settings.

- The table items are explained below.

  - IPv4 address

    - Displays the IPv4 address setting.

  - IPv4 default gateway

    - Displays the IPv4 default gateway setting.

- Press the “Setting” button to show the page for IPv4 settings.

#### 2.2. IPv6 settings

- Shows the IPv6 settings.

- The table items are explained below.

  - IPv6 address

    - Displays the IPv6 address setting.

  - IPv6 default gateway

    - Displays the IPv6 default gateway settings.

- Press the “Setting” button to show the page for IPv6 settings.

### 3. IPv4 settings page

This page is for configuring IPv4 settings.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 3.1. IPv4 settings

- VLAN ID

  - From the list, select the VLAN to assign IPv4 address.

  - However, the VLAN for which frame forwarding is invalid cannot be selected.

- IPv4 address

  Select the IP address from the following items. Only a VLAN for which frame forwarding is valid can be specified for this item.
  Only one VLAN interfaces can be configured for an IPv4 address.

  - Obtain automatically using DHCP

    - When auto-acquire does not work, the link local address is automatically configured by the Auto IP function.

  - Specify a fixed IP address

    - Enter the IP address and subnet mask.

- IPv4 default gateway

  - Specify an IP address for the IPv4 default gateway.

  - If omitted when DHCP is used, the default gateway obtained by DHCP is used.

### 4. IPv6 settings page

This page is for configuring IPv6 settings.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 4.1. IPv6 settings

- VLAN ID

  - From the list, select the VLAN to assign IPv6 address.

  - However, the VLAN for which frame forwarding is invalid cannot be selected.

- IPv6 address

  Only one VLAN interfaces can be configured for an IPv6 address.

  - Select whether the IPv6 address will be enabled or disabled from the following items.

    - Disable IPv6

    - Enable IPv6

  - For global addresses, select from the following items.

    - Not set

    - Obtain automatically using RA

    - Specify a fixed IP address

      - Enter the IP address and subnet mask.

  - Set the link local address.

- IPv6 default gateway

  - Specify an IPv6 address for the IPv6 default gateway.

  - If omitted when RA is used, the default gateway obtained by RA is used.

Search result
No more search results.
There are no topics that match your search query.