# L2MS settings

### 1. Summary

This page is for changing the L2MS settings.
L2MS ( Layer2 Management Service ) is a function for managing Yamaha network devices at the layer 2 level.
These settings can be used to enable/disable L2MS units or specify frame input permission settings using L2MS filters.

### 2. Top page

This is the top page for the L2MS settings.

#### 2.1. L2MS settings

- The current settings of the L2MS are show.

- Press the "Setting" button to access a page where you can change the settings.

#### 2.2. L2MS filter settings

- The current settings for the L2MS filter are shown for each interface.

- The table items are explained below.

  - Check box

    - Select the check box for bulk settings or to initialize the settings.

  - Port

    - Displays the interface name.

  - Rejection of L2MS frame

    - Displays the filter setting for blocking L2MS frames.

  - Rejection of Non-L2MS frame

    - Displays the filter settings for blocking non-L2MS frames.

- Press the "Setting" button to display the page where you can change the settings of the selected interface.

- If you press the "Specify all" button, the settings can be changed for all interfaces whose check box is selected.

  - The default settings will be applied to the settings on the L2MS filter settings page.

- If you press the "Return to defaults" button, the settings will be initialized on all interfaces whose check boxes are selected.

  - Each of the default settings are shown below.

    - Rejection of L2MS frame : Disabled

    - Rejection of Non-L2MS frame : Disabled

### 3. L2MS settings page

In this page you can enable/disable L2MS.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 3.1. L2MS settings

- L2MS

  - Enabled

    - L2MS will be enabled.

    - This device functions as an L2MS agent and can be controlled by the L2MS manager.

  - Disabled

    - L2MS will be disabled.

    - L2MS frames can be transmitted in the same manner as non-L2MS frames, but cannot be controlled by the L2MS manager.

### 4. L2MS filter settings page

This page is for L2MS filter settings.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 4.1. L2MS filter settings

- Port

  - Displays the name of the interface for which settings will be made.

- Rejection of L2MS frame

  - Select the operation for the filter for blocking L2MS frames from the following options.

    - Disabled

    - Enabled

- Rejection of Non-L2MS frame

  - Select the operation for the filter for blocking non-L2MS frames from the following options.

    - Disabled

    - Enabled

- If both filters are enabled, all frames are rejected at the interface.

- Be aware that it will no longer be possible to access the GUI form a port where the non-L2MS filter is enabled.

Search result
No more search results.
There are no topics that match your search query.