# SNMP MIB Reference

### 1. SNMP MIB List

The SNMP MIBs that are supported by this product are shown below.

#### 1.1. MIB tree

The MIB tree for MIB groups that are supported by this product are shown below.

       iso(1)
       |
       +--std(0)
       ||
       |+--iso8802(8802)
       ||
       |+--ieee802dot1(1)
       ||
       |+--ieee802dot1mibs(1)
       ||
       |+--ieee8021paeMIB(1)           (port authentication information)
       ||
       |+--lldpMIB(2)
       ||
       |+--lldpObjects(1)           (LLDP information)
       |
       +--member-body(2)
       ||
       |+--us(840)
       ||
       |+--802dot3(10006)
       ||
       |+--snmpmibs(300)
       ||
       |+--lagMIB(43)         (LACP link aggregation information)
       |
       +--org(3)
          |
          +--dod(6)
          ||
          |+--internet(1)
          ||
          |+--mgmt(2)
          |||
          ||+--mib-2(1)
          |||
          ||+--system(1)             (system information)
          |||
          ||+--interfaces(2)         (interface information)
          |||
          ||+--at(3)                 (mapping information for network addresses and physical addresses)
          |||
          ||+--rmon(16)              (RMON information)
          |||
          ||+--dot1dBridge(17)       (dot1dBridge information)
          |||
          ||+--ifMIB(31)             (additional information for interface)
          |||
          ||+--entityMIB(47)         (entity information)
          |||
          ||+--powerEthernetMIB(105) (PoE information)
          ||
          |+--private(4)
          ||
          |+--enterprises(1)
          ||
          |+--yamaha(1182)
          ||
          |+--yamahaSW(3)                  (private MIB Yamaha switch information)
          ||
          |+--yamahaSWHardware(1)       (hardware information)
          ||
          |+--yamahaSWFirmware(2)       (firmware information)
          ||
          |+--yamahaSWL2ms(5)           (L2MS information)
          ||
          |+--yamahaSWErrDisable(6)     (error detection function information)
          ||
          |+--yamahaSWRmon(7)           (RMON information)
          ||
          |+--yamahaSWTermMon(8)        (terminal monitoring information)
          ||
          |+--yamahaSWBridge(9)         (dot1dBridge information)
          ||
          |+--yamahaSWPowerEthernet(10) (PoE information)
          ||
          |+--yamahaSWLoopDetect(11)    (Loop detection information)
          |
          +--ieee(111)
             |
             +--standards-association-numbers-series-standards(2)
                |
                +--lan-man-stds(802)
                   |
                   +--ieee802dot1(1)
                      |
                      +--ieee802dot1mibs(1)
                         |
                         +--lldpV2MIB(13)            (LLDP information)

#### 1.2. Standard MIB list

The standard MIBs that are supported are shown below.

MIB group | Summary
--- | ---
ieee8021paeMIB group | Port authentication information
lldpMIB group | LLDP information
lagMIB group | LACP link aggregation information
system group | System information
interface group | Interface information
at group | Mapping information for physical addresses and network addresses
rmon group | RMON information
dot1dBridge group | dot1dBridge information
ifMIB group | Additional information for interface
entityMIB group | Entity information
powerEthernetMIB group | PoE information

#### 1.3. Private MIB list

Private MIBs that are supported are shown below.
All of this information is related to Yamaha switches.

MIB group | Summary
--- | ---
yamahaSWHardware group | Hardware information
yamahaSWFirmware group | Firmware information
yamahaSWL2ms group | L2MS information
yamahaSWErrDisable group | Error detection function information
yamahaSWRmon group | RMON information
yamahaSWTermMon group | Terminal monitoring information
yamahaSWBridge group | dot1dBridge information
yamahaSWPowerEthernet group | PoE information
yamahaSWLoopDetect group | Loop detection information

#### 1.4. Standard MIB trap list

The standard MIB traps that are supported are shown below.

Trap | Summary
--- | ---
coldStart | Power OFF/ON notification
warmStart | Reload notification
linkDown | Linkdown notification
linkUp | Linkup notification
authenticationFailure | Notification of failed authentication
risingAlarm | Notification that RMON upper threshold value has been exceeded
fallingAlarm | Notification that RMON lower threshold value has been exceeded
newRoot | Notification that new root for bridge has been detected
topologyChange | Notification when a change in topology has been detected
pethPsePortOnOffNotification | PoE port status change notification
pethMainPowerUsageOnNotification | Notification that the power consumption has exceeded the threshold value
pethMainPowerUsageOffNotification | Notification that the power consumption has fallen below the threshold value

#### 1.5. Private MIB trap list

Private MIBs traps that are supported are shown below.

Trap | Summary
--- | ---
yshTemperatureStatusNormalTrap | Normal temperature status notification
yshTemperatureStatusWarningTrap | Warning temperature status notification
yshTemperatureStatusErrorTrap | Error temperature status notification
yshFanStoppedTrap | Fan stopped notification
yshFanSpeedUpTrap | Increased fan RPM notification
yshFanSpeedDownTrap | Decreased fan RPM notification
yshTemperatureSensorInvalidTrap | Notification that a thermal sensor abnormality has occurred
ysl2msFindAgent | Notification that L2MS agent was detected
ysl2msDetectDown | Notification that L2MS agent was lost
ysedTrap | Notification of detect/cancel for error detection function
ystmIfTermTrap | Notification of terminal monitoring (port) detection
ystmIpTermTrap | Notification of terminal monitoring (IP address) detection
yspeSupplyPortTrap | Power supply start notification
yspeTerminatePortTrap | Power supply stop notification
yspeGuardBandStateTrap | Guard band status change notification
yspePortErrorTrap | PoE port error detection/removal notification
yspeUnitFailureTrap | PoE unit power supply abnormality notification
ysldPortDetectLoopTrap | Loop detection notification (port)
ysldPortResolveLoopTrap | Loop detection cancellation notification (port)
ysldLagDetectLoopTrap | Loop detection notification (logical interface)
ysldLagResolveLoopTrap | Loop detection cancellation notification (logical interface)

### 2. Definition of Terms Used

MIB access classification

The MIB access type used in subsequent explanations is described below.

- MIB access classification

  Access name | Description
  --- | ---
  R/O | Access to the MIB is read-only
  R/W | Access to the MIB is read-write
  R/NW | Although the access to the MIB is read-write as per the standards, it is read-only on this product
  R/C | Access to the MIB is read-create
  R/NC | Although the access to the MIB is read-create as per the standards, it is read-only on this product
  N/A | The MIB cannot be retrieved Note: May be used as additional information for traps (variable-bindings)

ifIndex

This is the ID number linked to the interface. For information about ifIndex assignments, refer to the following technical reference.

- Basic Interface Functions

### 3. Obtaining a Private MIB

Private MIB files may be acquired from here.

### 4. Standard MIBs

Standard MIBs that are supported by this product are shown below.

#### 4.1. ieee8021paeMIB group

This MIB is related to port authentication information.
The syntax defined for the ieee8021paeMIB group is shown below.

- Syntax defined in the ieee8021paeMIB group

  Syntax | Definition
  --- | ---
  PaeControlledDirections | INTEGER * both(0) * in(1)
  PaeControlledPortStatus | INTEGER * authorized(1) * unauthorized(2)
  PaeControlledPortControl | INTEGER * forceUnauthorized(1) * auto(2) * forceAuthorized(3)

The ieee8021paeMIB group is divided into subgroups such as those shown below.

       ieee8021paeMIB(1)
         |
         +--paeMIBObjects(1)
            |
            +--dot1xPaeSystem(1)
            |
            +--dot1xPaeAuthenticator(2)

- dot1xPaeSystem group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  dot1xPaeSystemAuthControl | 1.0.8802.1.1.1.1.1.1 | R/NW | INTEGER * enabled(1) * disabled(2) | Setting value for authentication function at the system level
  dot1xPaePortTable | 1.0.8802.1.1.1.1.1.2 | N/A |  | System-level information table
  | dot1xPaePortEntry | 1.0.8802.1.1.1.1.1.2.1 | N/A |  | INDEX * dot1xPaePortNumber
  dot1xPaePortNumber | 1.0.8802.1.1.1.1.1.2.1.1 | N/A | InterfaceIndex | Port numbers for which the authentication function is enabled | dot1xPaePortProtocolVersion
  1.0.8802.1.1.1.1.1.2.1.2 | R/O | Unsigned32 | Protocol version (2, fixed) | dot1xPaePortCapabilities
  1.0.8802.1.1.1.1.1.2.1.3 | R/O | BITS | PAE functions supported by the port (0, fixed) | dot1xPaePortInitialize
  1.0.8802.1.1.1.1.1.2.1.4 | R/NW | TruthValue | Initialization control for ports (2, fixed) | dot1xPaePortReauthenticate

- dot1xPaeAuthenticator group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  dot1xAuthConfigTable | 1.0.8802.1.1.1.1.2.1 | N/A |  | Structural object table for Authenticator PAE for each port
  | dot1xAuthConfigEntry | 1.0.8802.1.1.1.1.2.1.1 | N/A |  | INDEX * dot1xPaePortNumber
  | Dot1xAuthAdminControlledDirections | 1.0.8802.1.1.1.1.2.1.1.3 | R/NW | PaeControlledDirections | Packet forwarding operation in an unauthenticated state, controlled by management
  dot1xAuthOperControlledDirections | 1.0.8802.1.1.1.1.2.1.1.4 | R/O | PaeControlledDirections | Packet forwarding operation in an unauthenticated state, controlled by operation
  dot1xAuthAuthControlledPortStatus | 1.0.8802.1.1.1.1.2.1.1.5 | R/O | PaeControlledPortStatus | Port authentication status
  dot1xAuthAuthControlledPortControl | 1.0.8802.1.1.1.1.2.1.1.6 | R/NW | PaeControlledPortControl | Setting value for 802.1X authentication operating mode
  dot1xAuthQuietPeriod | 1.0.8802.1.1.1.1.2.1.1.7 | R/NW | Unsigned32 | Setting value for authentication restriction period
  dot1xAuthSuppTimeout | 1.0.8802.1.1.1.1.2.1.1.9 | R/NW | Unsigned32 | Response wait time setting value for the supplicant
  dot1xAuthServerTimeout | 1.0.8802.1.1.1.1.2.1.1.10 | R/NW | Unsigned32 | Setting value for server response wait time
  dot1xAuthMaxReq | 1.0.8802.1.1.1.1.2.1.1.11 | R/NW | Unsigned32 | Setting value for number of times EAPOL packets are retransmitted
  dot1xAuthReAuthPeriod | 1.0.8802.1.1.1.1.2.1.1.12 | R/NW | Unsigned32 | Setting value for re-authentication interval
  dot1xAuthReAuthEnabled | 1.0.8802.1.1.1.1.2.1.1.13 | R/NW | TruthValue | Setting value for reauthentication function
  dot1xAuthKeyTxEnabled | 1.0.8802.1.1.1.1.2.1.1.14 | R/NW | TruthValue | Constant value (2, fixed) used by Authenticator PAE state machine
  dot1xAuthStatsTable | 1.0.8802.1.1.1.1.2.2 | N/A |  | Statistical data object table for Authenticator PAE associated with each port
  | dot1xAuthStatsEntry | 1.0.8802.1.1.1.1.2.2.1 | N/A |  | INDEX * dot1xPaePortNumber
  | dot1xAuthEapolFramesRx | 1.0.8802.1.1.1.1.2.2.1.1 | R/O | Counter32 | No. of EAPOL frames that are received, all valid types
  dot1xAuthEapolFramesTx | 1.0.8802.1.1.1.1.2.2.1.2 | R/O | Counter32 | No. of EAPOL frames that are transmitted, all types
  dot1xAuthEapolStartFramesRx | 1.0.8802.1.1.1.1.2.2.1.3 | R/O | Counter32 | No. of EAPOL Start frames received
  dot1xAuthEapolLogoffFramesRx | 1.0.8802.1.1.1.1.2.2.1.4 | R/O | Counter32 | No. of EAPOL Logoff frames received
  dot1xAuthEapolRespIdFramesRx | 1.0.8802.1.1.1.1.2.2.1.5 | R/O | Counter32 | No. of EAP Response/Identity frames received
  dot1xAuthEapolRespFramesRx | 1.0.8802.1.1.1.1.2.2.1.6 | R/O | Counter32 | No. of valid EAP Response frames, excepting EAP Response/Identity frames received
  dot1xAuthEapolReqIdFramesTx | 1.0.8802.1.1.1.1.2.2.1.7 | R/O | Counter32 | No. of EAP Request/Identity frames transmitted
  dot1xAuthEapolReqFramesTx | 1.0.8802.1.1.1.1.2.2.1.8 | R/O | Counter32 | No. of EAP Request frames, excepting EAP Request/Identity frames transmitted
  dot1xAuthInvalidEapolFramesRx | 1.0.8802.1.1.1.1.2.2.1.9 | R/O | Counter32 | No. of frames within received EAPOL frames, for which frame type has not been approved
  dot1xAuthEapLengthErrorFramesRx | 1.0.8802.1.1.1.1.2.2.1.10 | R/O | Counter32 | No. of received EAPOL frames, for which the packet body length is invalid
  dot1xAuthLastEapolFrameVersion | 1.0.8802.1.1.1.1.2.2.1.11 | R/O | Unsigned32 | Protocol version numbers for most recently received EAPOL frames
  dot1xAuthLastEapolFrameSource | 1.0.8802.1.1.1.1.2.2.1.12 | R/O | MacAddress | Source MAC address of EAPOL frames most recently received

#### 4.2. lldpMIB group

This MIB is related to LLDP information.
This product handles the following two MIB groups involved in the LLDP.

- lldpMIB group (MIB defined in IEEE Std 802.1AB-2005)

- lldpV2MIB group (MIB defined in IEEE Std 802.1AB-2009)

Though both MIBs handle the LLDP in the same way, both are supported to provide compatibility with other models.
Some MIBs refer to the same value.

The syntax defined for the lldpMIB group is shown below.

- Syntax defined in the lldpMIB group

  Syntax | Definition
  --- | ---
  LldpChassisIdSubtype | INTEGER * chassisComponent(1) * interfaceAlias(2) * portComponent(3) * macAddress(4) * networkAddress(5) * interfaceName(6) * local(7)
  LldpChassisId | OCTET STRING (SIZE (1..255))
  LldpPortIdSubtype | INTEGER * interfaceAlias(1) * portComponent(2) * macAddress(3) * networkAddress(4) * interfaceName(5) * agentCircuitId(6) * local(7)
  LldpPortId | OCTET STRING (SIZE (1..255))
  LldpSystemCapabilitiesMap | BITS * other(0) * repeater(1) * bridge(2) * wlanAccessPoint(3) * router(4) * telephone(5) * docsisCableDevice(6) * stationOnly(7)
  LldpPortNumber | INTEGER32 (1..4096)
  LldpPowerPortClass | INTEGER * pClassPSE(1) * pClassPD(2)
  LldpXMedDeviceClass | INTEGER * notDefined(0) * endpointClass1(1) * endpointClass2(2) * endpointClass3(3) * networkConnectivity(4)
  LldpXMedCapabilities | INTEGER * capabilities(0) * networkPolicy(1) * location(2) * extendedPSE(3) * extendedPD(4) * inventory(5)
  LldpManAddress | OCTET STRING (SIZE (1..31))
  LldpManAddrIfSubtype | INTEGER * unknown(1) * ifIndex(2) * systemPortNumber(3)

The lldpMIB group is divided into subgroups, such as shown below.

       lldpObjects(1)
         |
         +--lldpConfiguration(1)
         |
         +--lldpStatistics(2)
         |
         +--lldpLocalSystemData(3)
         |
         +--lldpRemoteSystemsData(4)
         |
         +--lldpExtensions(5)
            |
            +--lldpXdot3MIB(4623)
            ||
            |+--lldpXdot3Objects(1)
            ||
            |+--lldpXdot3Config(1)
            ||
            |+--lldpXdot3LocalData(2)
            ||
            |+--lldpXdot3RemoteData(3)
            |
            +--lldpXMedMIB(4795)
               |
               +--lldpXMedObjects(1)
                  |
                  +--lldpXMedConfig(1)
                  |
                  +--lldpXMedLocalData(2)
                  |
                  +--lldpXMedRemoteData(3)

- lldpConfiguration group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpPortConfigTable | 1.0.8802.1.1.2.1.1.6 | N/A |  | Table of information for each port
  | lldpPortConfigEntry | 1.0.8802.1.1.2.1.1.6.1 | N/A |  | INDEX * lldpPortConfigPortNum
  | lldpPortConfigAdminStatus | 1.0.8802.1.1.2.1.1.6.1.2 | R/NW | INTEGER * txOnly(1) * rxOnly(2) * txAndRx(3) * disabled(4) | LLDP transmission/reception status
  lldpPortConfigNotificationEnable | 1.0.8802.1.1.2.1.1.6.1.3 | R/NW | TruthVal | LLDP notification status
  lldpPortConfigTLVsTxEnable | 1.0.8802.1.1.2.1.1.6.1.4 | R/NW | BITS * portDesc(0) * sysName(1) * sysDesc(2) * sysCap(3) | Basic management TLV transmission item

- lldpStatistics group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpStatsRemTablesLastChangeTime | 1.0.8802.1.1.2.1.2.1 | R/O | TimeTicks | Time from system initialization until remote data update
  lldpStatsRemTablesInserts | 1.0.8802.1.1.2.1.2.2 | R/O | INTEGER (0..4294967295) | Total number of entries added to the remote device management table
  lldpStatsRemTablesDeletes | 1.0.8802.1.1.2.1.2.3 | R/O | INTEGER (0..4294967295) | Total number of entries deleted from the remote device management table
  lldpStatsRemTablesDrops | 1.0.8802.1.1.2.1.2.4 | R/O | INTEGER (0..4294967295) | Total number of entries that could not be specified in the remote device management table
  lldpStatsRemTablesAgeouts | 1.0.8802.1.1.2.1.2.5 | R/O | INTEGER (0..4294967295) | Total number of entries that exceeded the TTL time (aged out) and were deleted from the remote device management table
  lldpStatsTxPortTable | 1.0.8802.1.1.2.1.2.6 | N/A |  | Table of information for each port
  | lldpStatsTxPortEntry | 1.0.8802.1.1.2.1.2.6.1 | N/A |  | INDEX * lldpStatsTxPortNum
  | lldpStatsTxPortNum | 1.0.8802.1.1.2.1.2.6.1.1 | N/A | LldpPortNumber |
  lldpStatsTxPortFramesTotal | 1.0.8802.1.1.2.1.2.6.1.2 | R/O | INTEGER (0..4294967295) | Total number of LLDP frames transmitted
  lldpStatsRxPortTable | 1.0.8802.1.1.2.1.2.7 | N/A |  | Table of information for each port
  | lldpStatsRxPortEntry | 1.0.8802.1.1.2.1.2.7.1 | N/A |  | INDEX * lldpStatsRxPortNum
  | lldpStatsRxPortNum | 1.0.8802.1.1.2.1.2.7.1.1 | N/A | LldpPortNumber |
  lldpStatsRxPortFramesDiscardedTotal | 1.0.8802.1.1.2.1.2.7.1.2 | R/O | INTEGER (0..4294967295) | Number of LLDP frames discarded
  lldpStatsRxPortFramesErrors | 1.0.8802.1.1.2.1.2.7.1.3 | R/O | INTEGER (0..4294967295) | Number of error frames received
  lldpStatsRxPortFramesTotal | 1.0.8802.1.1.2.1.2.7.1.4 | R/O | INTEGER (0..4294967295) | Number of LLDP frames received
  lldpStatsRxPortTLVsDiscardedTotal | 1.0.8802.1.1.2.1.2.7.1.5 | R/O | INTEGER (0..4294967295) | Number of TLVs discarded
  lldpStatsRxPortTLVsUnrecognizedTotal | 1.0.8802.1.1.2.1.2.7.1.6 | R/O | INTEGER (0..4294967295) | Number of unrecognized TLVs received
  lldpStatsRxPortAgeoutsTotal | 1.0.8802.1.1.2.1.2.7.1.7 | R/O | INTEGER (0..4294967295) | Number of entries that aged-out

- lldpLocalSystemData group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpLocChassisIdSubtype | 1.0.8802.1.1.2.1.3.1 | R/O | LldpChassisIdSubtype | Subtype of chassis ID
  lldpLocChassisId | 1.0.8802.1.1.2.1.3.2 | R/O | LldpChassisId | Chassis ID
  lldpLocSysName | 1.0.8802.1.1.2.1.3.3 | R/O | SnmpAdminString (SIZE (0..255)) | System name
  lldpLocSysDesc | 1.0.8802.1.1.2.1.3.4 | R/O | SnmpAdminString (SIZE (0..255)) | System description
  lldpLocSysCapSupported | 1.0.8802.1.1.2.1.3.5 | R/O | LldpSystemCapabilitiesMap | Functions supported by the system
  lldpLocSysCapEnabled | 1.0.8802.1.1.2.1.3.6 | R/O | LldpSystemCapabilitiesMap | Functions enabled by the system
  lldpLocPortTable | 1.0.8802.1.1.2.1.3.7 | N/A |  | Table of information for each port
  | lldpLocPortEntry | 1.0.8802.1.1.2.1.3.7.1 | N/A |  | INDEX * lldpLocPortNum
  | lldpLocPortNum | 1.0.8802.1.1.2.1.3.7.1.1 | N/A | LldpPortNumber |
  lldpLocPortIdSubtype | 1.0.8802.1.1.2.1.3.7.1.2 | R/O | LldpPortIdSubtype | Subtype of port ID
  lldpLocPortId | 1.0.8802.1.1.2.1.3.7.1.3 | R/O | OCTET STRING (SIZE (1..255)) | Port ID
  lldpLocPortDesc | 1.0.8802.1.1.2.1.3.7.1.4 | R/O | SnmpAdminString (SIZE (0..255)) | Port description
  lldpLocManAddrTable | 1.0.8802.1.1.2.1.3.8 | N/A |  | Table of local system management addresses
  | lldpLocManAddrEntry | 1.0.8802.1.1.2.1.3.8.1 | N/A |  | INDEX * lldpV2LocManAddrSubtype * lldpLocManAddr
  | lldpLocManAddrSubtype | 1.0.8802.1.1.2.1.3.8.1.1 | N/A | AddressFamilyNumbers | Sub-type for management address
  lldpLocManAddr | 1.0.8802.1.1.2.1.3.8.1.2 | N/A | LldpManAddress | Management address
  lldpLocManAddrLen | 1.0.8802.1.1.2.1.3.8.1.3 | R/O | Integer32 | Management address length
  lldpLocManAddrIfSubtype | 1.0.8802.1.1.2.1.3.8.1.4 | R/O | LldpManAddrIfSubtype | Interface sub-type
  lldpLocManAddrIfId | 1.0.8802.1.1.2.1.3.8.1.5 | R/O | Integer32 | Interface ID

- lldpRemoteSystemsData group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpRemTable | 1.0.8802.1.1.2.1.4.1 | N/A |  | Table of information for each port
  | lldpRemEntry | 1.0.8802.1.1.2.1.4.1.1 | N/A |  | INDEX * lldpRemTimeMark * lldpRemLocalPortNum * lldpRemIndex
  | lldpRemTimeMark | 1.0.8802.1.1.2.1.4.1.1.1 | N/A | TimeFilter |
  lldpRemLocalPortNum | 1.0.8802.1.1.2.1.4.1.1.2 | N/A | LldpPortNumber |
  lldpRemIndex | 1.0.8802.1.1.2.1.4.1.1.3 | N/A | INTEGER32 (1..2147483647) |
  lldpRemChassisIdSubtype | 1.0.8802.1.1.2.1.4.1.1.4 | R/O | LldpChassisIdSubtype | Subtype of the remote device chassis ID
  lldpRemChassisId | 1.0.8802.1.1.2.1.4.1.1.5 | R/O | SnmpAdminString (SIZE (0..255)) | Chassis ID of remote device
  lldpRemPortIdSubtype | 1.0.8802.1.1.2.1.4.1.1.6 | R/O | LldpPortIdSubtype | Subtype of the remote device port ID
  lldpRemPortId | 1.0.8802.1.1.2.1.4.1.1.7 | R/O | OCTET STRING (SIZE (1..255)) | Port ID of remote device
  lldpRemPortDesc | 1.0.8802.1.1.2.1.4.1.1.8 | R/O | SnmpAdminString (SIZE (0..255)) | Description of remote device port
  lldpRemSysName | 1.0.8802.1.1.2.1.4.1.1.9 | R/O | SnmpAdminString (SIZE (0..255)) | System name of remote device
  lldpRemSysDesc | 1.0.8802.1.1.2.1.4.1.1.10 | R/O | SnmpAdminString (SIZE (0..255)) | System description of remote device
  lldpRemSysCapSupported | 1.0.8802.1.1.2.1.4.1.1.11 | R/O | LldpSystemCapabilitiesMap | Functionality supported by the remote device system
  lldpRemSysCapEnabled | 1.0.8802.1.1.2.1.4.1.1.12 | R/O | LldpSystemCapabilitiesMap | Functionality enabled in the remote device system
  lldpRemManAddrTable | 1.0.8802.1.1.2.1.4.2 | N/A |  |
  | lldpRemManAddrEntry | 1.0.8802.1.1.2.1.4.2.1 | N/A |  | INDEX * lldpRemTimeMark * lldpRemLocalPortNum * lldpRemIndex * lldpRemManAddrSubtype * lldpRemManAddr
  | lldpRemManAddrSubtype | 1.0.8802.1.1.2.1.4.2.1.1 | N/A | LldpPortNumber |
  lldpRemManAddr | 1.0.8802.1.1.2.1.4.2.1.2 | N/A |  |
  lldpRemManAddrIfSubtype | 1.0.8802.1.1.2.1.4.2.1.3 | R/O | INTEGER * unknown(1) * ifIndex(2) * systemPortNumber(3) | Subtype of remote device interface
  lldpRemManAddrIfId | 1.0.8802.1.1.2.1.4.2.1.4 | R/O | Integer32 | Interface ID of remote device
  lldpRemManAddrOID | 1.0.8802.1.1.2.1.4.2.1.5 | R/O | OBJECT IDENTIFIER | OID of the remote device management address
  lldpRemUnknownTLVTable | 1.0.8802.1.1.2.1.4.3 | N/A |  |
  | lldpRemUnknownTLVEntry | 1.0.8802.1.1.2.1.4.3.1 | N/A |  | INDEX * lldpRemTimeMark * lldpRemLocalPortNum * lldpRemIndex * lldpRemUnknownTLVType
  | lldpRemUnknownTLVType | 1.0.8802.1.1.2.1.4.3.1.1 | N/A | LldpPortNumber |
  lldpRemUnknownTLVInfo | 1.0.8802.1.1.2.1.4.3.1.2 | R/O | LldpPortNumber | Latest undefined TLV information for remote device
  lldpRemOrgDefInfoTable | 1.0.8802.1.1.2.1.4.4 | N/A |  |
  | lldpRemOrgDefInfoEntry | 1.0.8802.1.1.2.1.4.4.1 | N/A |  | INDEX * lldpRemTimeMark * lldpRemLocalPortNum * lldpRemIndex * lldpRemOrgDefInfoOUI * lldpRemOrgDefInfoSubtype * lldpRemOrgDefInfoIndex
  | lldpRemOrgDefInfoOUI | 1.0.8802.1.1.2.1.4.4.1.1 | N/A |  |
  lldpRemOrgDefInfoSubtype | 1.0.8802.1.1.2.1.4.4.1.2 | N/A |  |
  lldpRemOrgDefInfoIndex | 1.0.8802.1.1.2.1.4.4.1.3 | N/A |  |
  lldpRemOrgDefInfo | 1.0.8802.1.1.2.1.4.4.1.4 | R/O | OCTET STRING (SIZE (0..507)) | Index of undefined TLV information for remote device (Limited to IEEE802.1 and IEEE802.3)

- lldpXdot3LocalData group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpXdot3LocPowerTable | 1.0.8802.1.1.2.1.5.4623.1.2.2 | N/A |  | Table of information for each port
  | lldpXdot3LocPowerEntry | 1.0.8802.1.1.2.1.5.4623.1.2.2.1 | N/A |  | INDEX * lldpLocPortNum
  | lldpXdot3LocPowerPortClass | 1.0.8802.1.1.2.1.5.4623.1.2.2.1.1 | R/O | LldpPowerPortClass | PSE or PD status
  lldpXdot3LocPowerMDISupported | 1.0.8802.1.1.2.1.5.4623.1.2.2.1.2 | R/O | TruthValue | Power supply capability support
  lldpXdot3LocPowerMDIEnabled | 1.0.8802.1.1.2.1.5.4623.1.2.2.1.3 | R/O | TruthValue | Enables/disables the power supply capability
  lldpXdot3LocPowerPairControlable | 1.0.8802.1.1.2.1.5.4623.1.2.2.1.4 | R/O | TruthValue | Ability to select the signal line to be used for power supply
  lldpXdot3LocPowerPairs | 1.0.8802.1.1.2.1.5.4623.1.2.2.1.5 | R/O | INTEGER32 (1|2) * signal(1) * spare(2) | Signal line to be used for power supply
  lldpXdot3LocPowerClass | 1.0.8802.1.1.2.1.5.4623.1.2.2.1.6 | R/O | INTEGER32 (1|2|3|4|5) * class0(1) * class1(2) * class2(3) * class3(4) * class4(5) | Port power class

- lldpXdot3RemoteData group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpXdot3RemPowerTable | 1.0.8802.1.1.2.1.5.4623.1.3.2 | N/A |  | Table of information for each port
  | lldpXdot3RemPowerEntry | 1.0.8802.1.1.2.1.5.4623.1.3.2.1 | N/A |  | INDEX * lldpRemTimeMark * lldpRemLocalPortNum * lldpRemIndex
  | lldpXdot3RemPowerPortClass | 1.0.8802.1.1.2.1.5.4623.1.3.2.1.1 | R/O | LldpPowerPortClass | Remote device status whether it is PSE or PD
  lldpXdot3RemPowerMDISupported | 1.0.8802.1.1.2.1.5.4623.1.3.2.1.2 | R/O | TruthValue | Remote device power supply capability support
  lldpXdot3RemPowerMDIEnabled | 1.0.8802.1.1.2.1.5.4623.1.3.2.1.3 | R/O | TruthValue | Enables/disables the remote device power supply capability
  lldpXdot3RemPowerPairControlable | 1.0.8802.1.1.2.1.5.4623.1.3.2.1.4 | R/O | TruthValue | Ability to select the signal line to be used for power supply of remote device
  lldpXdot3RemPowerPairs | 1.0.8802.1.1.2.1.5.4623.1.3.2.1.5 | R/O | INTEGER32 (1|2) * signal(1) * spare(2) | Signal line to be used for power supply of remote device
  lldpXdot3RemPowerClass | 1.0.8802.1.1.2.1.5.4623.1.3.2.1.6 | R/O | INTEGER32 (1|2|3|4|5) * class0(1) * class1(2) * class2(3) * class3(4) * class4(5) | Remote device port power class

- lldpXMedConfig group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpXMedLocDeviceClass | 1.0.8802.1.1.2.1.5.4795.1.1.1 | R/O | LldpXMedDeviceClass | Local device class
  lldpXMedPortConfigTable | 1.0.8802.1.1.2.1.5.4795.1.1.2 | N/A |  | Table of information for each port
  | lldpXMedPortConfigEntry | 1.0.8802.1.1.2.1.5.4795.1.1.2.1 | N/A |  | INDEX * Port number
  | lldpXMedPortCapSupported | 1.0.8802.1.1.2.1.5.4795.1.1.2.1.1 | R/O | LldpXMedCapabilities | TLV transmission items supported by LLDP-MED
  lldpXMedPortConfigTLVsTxEnable | 1.0.8802.1.1.2.1.5.4795.1.1.2.1.2 | R/NW | LldpXMedCapabilities | TLV items sent as LLDP-MED
  lldpXMedPortConfigNotifEnable | 1.0.8802.1.1.2.1.5.4795.1.1.2.1.3 | R/NW | TruthValue | LLDP-MED notification status
  lldpXMedFastStartRepeatCount | 1.0.8802.1.1.2.1.5.4795.1.1.3 | R/NW | Unsigned32 (1..10) | LLDP-MED fast transmission count

- lldpXMedLocalData group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpXMedLocXPoEDeviceType | 1.0.8802.1.1.2.1.5.4795.1.2.10 | R/O | INTEGER * unknown(1) * pseDevice(2) * pdDevice(3) * none(4) | PSE or PD status
  lldpXMedLocXPoEPSEPortTable | 1.0.8802.1.1.2.1.5.4795.1.2.11 | N/A |  | PSE information table for each port
  | lldpXMedLocXPoEPSEPortEntry | 1.0.8802.1.1.2.1.5.4795.1.2.11.1 | N/A |  | INDEX * lldpLocPortNum
  | lldpXMedLocXPoEPSEPortPowerAv | 1.0.8802.1.1.2.1.5.4795.1.2.11.1.1 | R/O | Gauge32 (0..1023) | Power supply from the port (in units of 0.1 W)
  lldpXMedLocXPoEPSEPortPDPriority | 1.0.8802.1.1.2.1.5.4795.1.2.11.1.2 | R/O | INTEGER * unknown(1) * critical(2) * high(3) * low(4) | Port power supply priority order
  lldpXMedLocXPoEPSEPowerSource | 1.0.8802.1.1.2.1.5.4795.1.2.12 | R/O | INTEGER * unknown(1) * primary(2) * backup(3) | Own power source
  lldpXMedLocXPoEPDPowerReq | 1.0.8802.1.1.2.1.5.4795.1.2.13 | R/O | INTEGER32 (0..1023) | Power requirement for PSE (in units of 0.1 W)
  lldpXMedLocXPoEPDPowerSource | 1.0.8802.1.1.2.1.5.4795.1.2.14 | R/O | INTEGER * unknown(1) * fromPSE(2) * local * localAndPSE(4) | Type of own power source notified to the PSE
  lldpXMedLocXPoEPDPowerPriority | 1.0.8802.1.1.2.1.5.4795.1.2.15 | R/O | INTEGER * unknown(1) * critical(2) * high(3) * low(4) | Power supply priority requirement of the own device notified to the PSE

- lldpXMedRemoteData group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpXMedRemXPoETable | 1.0.8802.1.1.2.1.5.4795.1.3.5 | N/A |  | Remote device information table
  | lldpXMedRemXPoEEntry | 1.0.8802.1.1.2.1.5.4795.1.3.5.1 | N/A |  | INDEX * lldpRemTimeMark * lldpRemLocalPortNum * lldpRemIndex
  | lldpXMedRemXPoEDeviceType | 1.0.8802.1.1.2.1.5.4795.1.3.5.1.1 | R/O | INTEGER * unknown(1) * pseDevice(2) * pdDevice(3) * none(4) | Indicates whether the remote device is PSE or PD
  lldpXMedRemXPoEPSETable | 1.0.8802.1.1.2.1.5.4795.1.3.6 | N/A |  | PSE information table for remote device
  | lldpXMedRemXPoEPSEEntry | 1.0.8802.1.1.2.1.5.4795.1.3.6.1 | N/A |  | INDEX * lldpRemTimeMark * lldpRemLocalPortNum * lldpRemIndex
  | lldpXMedRemXPoEPSEPowerAv | 1.0.8802.1.1.2.1.5.4795.1.3.6.1.1 | R/O | Integer(0..1023) | Power requirement of remote device (in units of 0.1 W)
  lldpXMedRemXPoEPSEPowerSource | 1.0.8802.1.1.2.1.5.4795.1.3.6.1.2 | R/O | INTEGER * unknown(1) * fromPSE(2) * local(3) * localAndPSE(4) | Power supply type of remote device
  lldpXMedRemXPoEPDPowerPriority | 1.0.8802.1.1.2.1.5.4795.1.3.6.1.3 | R/O | INTEGER * unknown(1) * critical(2) * high(3) * low(4) | Power supply priority of remote device
  lldpXMedRemXPoEPDTable | 1.0.8802.1.1.2.1.5.4795.1.3.7 | N/A |  | PSE information table for remote device
  | lldpXMedRemXPoEPDEntry | 1.0.8802.1.1.2.1.5.4795.1.3.7.1 | N/A |  | INDEX * lldpRemTimeMark * lldpRemLocalPortNum * lldpRemIndex
  | lldpXMedRemXPoEPDPowerReq | 1.0.8802.1.1.2.1.5.4795.1.3.7.1.1 | R/O | Integer(0..1023) | Power requirement of remote device (in units of 0.1 W)
  lldpXMedRemXPoEPDPowerSource | 1.0.8802.1.1.2.1.5.4795.1.3.7.1.2 | R/O | INTEGER * unknown(1) * fromPSE(2) * local(3) * localAndPSE(4) | Power supply type of remote device
  lldpXMedRemXPoEPDPowerPriority | 1.0.8802.1.1.2.1.5.4795.1.3.7.1.3 | R/O | INTEGER * unknown(1) * critical(2) * high(3) * low(4) | Power supply priority of remote device

The lldpV2MIB group is divided into subgroups, such as shown below.

       lldpV2MIB(13)
         |
         +--lldpV2Objects(1)
            |
            +--lldpV2Configuration(1)
            |
            +--lldpV2Statistics(2)
            |
            +--lldpV2LocalSystemData(3)
            |
            +--lldpV2RemoteSystemsData(4)
            |
            +--lldpV2Extensions(5)
               |
               +--lldpV2Xdot3MIB(4623)
                  |
                  +--lldpV2Xdot3Objects(1)
                     |
                     +--lldpV2Xdot3LocalData(2)
                     |
                     +--lldpV2Xdot3RemoteData(3)

- lldpV2Configuration group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpV2PortConfigTable | 1.3.111.2.802.1.1.13.1.1.8 | N/A |  | Table for managing transmitted information for each port
  | lldpV2PortConfigEntry | 1.3.111.2.802.1.1.13.1.1.8.1 | N/A |  | INDEX * lldpV2PortConfigIfIndex * lldpV2PortConfigDestAddressIndex
  | lldpV2PortConfigIfIndex | 1.3.111.2.802.1.1.13.1.1.8.1.1 | N/A | InterfaceIndex | Index for each port
  lldpV2PortConfigDestAddressIndex | 1.3.111.2.802.1.1.13.1.1.8.1.2 | N/A | LldpV2DestAddressTableIndex | Destination MAC address index
  lldpV2PortConfigAdminStatus | 1.3.111.2.802.1.1.13.1.1.8.1.3 | R/O | INTEGER * txOnly(1) * rxOnly(2) * txAndRx(3) * disabled(4) | LLDP transmission/reception status
  lldpV2PortConfigNotificationEnable | 1.3.111.2.802.1.1.13.1.1.8.1.4 | R/O | TruthValue | LLDP notification status
  lldpV2PortConfigTLVsTxEnable | 1.3.111.2.802.1.1.13.1.1.8.1.5 | R/O | BITS * portDesc(0) * sysName(1) * sysDesc(2) * sysCap(3) | Basic management TLV transmission item
  lldpV2DestAddressTable | 1.3.111.2.802.1.1.13.1.1.9 | N/A |  | Table of MAC addresses used by LLDP
  | lldpV2DestAddressTableEntry | 1.3.111.2.802.1.1.13.1.1.9.1 | N/A |  | INDEX * lldpV2AddressTableIndex
  | lldpV2AddressTableIndex | 1.3.111.2.802.1.1.13.1.1.9.1.1 | N/A | LldpV2DestAddressTableIndex | Destination MAC address index
  lldpV2DestMacAddress | 1.3.111.2.802.1.1.13.1.1.9.1.2 | R/O | MacAddress | MAC address used for LLDP transmission

- lldpV2Statistics group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpV2StatsRemTablesLastChangeTime | 1.3.111.2.802.1.1.13.1.2.1 | R/O | TimeStamp | Time from system initialization until remote data update
  lldpV2StatsRemTablesInserts | 1.3.111.2.802.1.1.13.1.2.2 | R/O | ZeroBasedCounter32 | Total number of entries added to device management table
  lldpV2StatsRemTablesDeletes | 1.3.111.2.802.1.1.13.1.2.3 | R/O | ZeroBasedCounter32 | Total number of entries deleted from device management table
  lldpV2StatsRemTablesDrops | 1.3.111.2.802.1.1.13.1.2.4 | R/O | ZeroBasedCounter32 | Total number of entries that could not be set to device management table
  lldpV2StatsRemTablesAgeouts | 1.3.111.2.802.1.1.13.1.2.5 | R/O | ZeroBasedCounter32 | Total number of entries that exceeded TTL time (aged out) and were deleted from device management table
  lldpV2StatsTxPortTable | 1.3.111.2.802.1.1.13.1.2.6 | N/A |  | Table of statistical information for LLDP transmission
  | lldpV2StatsTxPortEntry | 1.3.111.2.802.1.1.13.1.2.6.1 | N/A |  | INDEX * lldpV2StatsTxIfInde * lldpV2StatsTxDestMACAddress
  | lldpV2StatsTxIfIndex | 1.3.111.2.802.1.1.13.1.2.6.1.1 | N/A | InterfaceIndex | Port index
  lldpV2StatsTxDestMACAddress | 1.3.111.2.802.1.1.13.1.2.6.1.2 | N/A | LldpV2DestAddressTableIndex | Destination MAC address index
  lldpV2StatsTxPortFramesTotal | 1.3.111.2.802.1.1.13.1.2.6.1.3 | R/O | Counter32 | Total number of LLDP frames transmitted
  lldpV2StatsTxLLDPDULengthErrors | 1.3.111.2.802.1.1.13.1.2.6.1.4 | R/O | Counter32 | Total no. of LLDP frame length errors
  lldpV2StatsRxPortTable | 1.3.111.2.802.1.1.13.1.2.7 | N/A |  | Table of statistical information for LLDP reception
  | lldpV2StatsRxPortEntry | 1.3.111.2.802.1.1.13.1.2.7.1 | N/A |  | INDEX * lldpV2StatsRxDestIfIndex * lldpV2StatsRxDestMACAddress
  | LldpV2StatsRxDestIfIndex | 1.3.111.2.802.1.1.13.1.2.7.1.1 | N/A | InterfaceIndex | Port index
  lldpV2StatsRxDestMACAddress | 1.3.111.2.802.1.1.13.1.2.7.1.2 | N/A | LldpV2DestAddressTableIndex | Destination MAC address index
  lldpV2StatsRxPortFramesDiscardedTotal | 1.3.111.2.802.1.1.13.1.2.7.1.3 | R/O | Counter32 | Number of LLDP frames discarded
  lldpV2StatsRxPortFramesErrors | 1.3.111.2.802.1.1.13.1.2.7.1.4 | R/O | Counter32 | Number of error frames received
  lldpV2StatsRxPortFramesTotal | 1.3.111.2.802.1.1.13.1.2.7.1.5 | R/O | Counter32 | Number of LLDP frames received
  lldpV2StatsRxPortTLVsDiscardedTotal | 1.3.111.2.802.1.1.13.1.2.7.1.6 | R/O | Counter32 | Number of LLDP frames discarded
  lldpV2StatsRxPortTLVsUnrecognizedTotal | 1.3.111.2.802.1.1.13.1.2.7.1.7 | R/O | Counter32 | Number of unrecognized TLVs received
  lldpV2StatsRxPortAgeoutsTotal | 1.3.111.2.802.1.1.13.1.2.7.1.8 | R/O | ZeroBasedCounter32 | Number of entries that aged-out

- lldpV2LocalSystemData group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpV2LocChassisIdSubtype | 1.3.111.2.802.1.1.13.1.3.1 | R/O | LldpV2ChassisIdSubtype | Subtype of chassis ID
  lldpV2LocChassisId | 1.3.111.2.802.1.1.13.1.3.2 | R/O | LldpV2ChassisId | Chassis ID
  lldpV2LocSysName | 1.3.111.2.802.1.1.13.1.3.3 | R/O | SnmpAdminString (SIZE (0..255)) | System name
  lldpV2LocSysDesc | 1.3.111.2.802.1.1.13.1.3.4 | R/O | SnmpAdminString (SIZE (0..255)) | System description
  lldpV2LocSysCapSupported | 1.3.111.2.802.1.1.13.1.3.5 | R/O | LldpV2SystemCapabilitiesMap | Functions supported by the system
  lldpV2LocSysCapEnabled | 1.3.111.2.802.1.1.13.1.3.6 | R/O | LldpV2SystemCapabilitiesMap | Functions enabled by the system
  lldpV2LocPortTable | 1.3.111.2.802.1.1.13.1.3.7 | N/A |  | Table of local port information
  | lldpV2LocPortEntry | 1.3.111.2.802.1.1.13.1.3.7.1 | N/A |  | INDEX * lldpV2LocPortIfIndex
  | lldpV2LocPortIfIndex | 1.3.111.2.802.1.1.13.1.3.7.1.1 | N/A | InterfaceIndex | Port index
  lldpV2LocPortIdSubtype | 1.3.111.2.802.1.1.13.1.3.7.1.2 | R/O | LldpV2PortIdSubtype | Subtype of port ID
  lldpV2LocPortId | 1.3.111.2.802.1.1.13.1.3.7.1.3 | R/O | LldpV2PortId | Port ID
  lldpV2LocPortDesc | 1.3.111.2.802.1.1.13.1.3.7.1.4 | R/O | SnmpAdminString (SIZE (0..255)) | Port description
  lldpV2LocManAddrTable | 1.3.111.2.802.1.1.13.1.3.8 | N/A |  | Table of local system management addresses
  | lldpV2LocManAddrEntry | 1.3.111.2.802.1.1.13.1.3.8.1 | N/A |  | INDEX * lldpV2LocManAddrSubtype * lldpV2LocManAddr
  | lldpV2LocManAddrSubtype | 1.3.111.2.802.1.1.13.1.3.8.1.1 | N/A | AddressFamilyNumbers | Sub-type for management address
  lldpV2LocManAddr | 1.3.111.2.802.1.1.13.1.3.8.1.2 | N/A | LldpV2ManAddress | Management address
  lldpV2LocManAddrLen | 1.3.111.2.802.1.1.13.1.3.8.1.3 | R/O | Unsigned32 | Management address length
  lldpV2LocManAddrIfSubtype | 1.3.111.2.802.1.1.13.1.3.8.1.4 | R/O | LldpV2ManAddrIfSubtype | Interface sub-type
  lldpV2LocManAddrIfId | 1.3.111.2.802.1.1.13.1.3.8.1.5 | R/O | Unsigned32 | Interface ID

- lldpV2RemoteSystemsData group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpV2RemTable | 1.3.111.2.802.1.1.13.1.4.1 | N/A |  | Table of information for connected remote devices
  | lldpV2RemEntry | 1.3.111.2.802.1.1.13.1.4.1.1 | N/A |  | INDEX * lldpV2RemTimeMark * lldpV2RemLocalIfIndex * lldpV2RemLocalDestMACAddress * lldpV2RemIndex
  | lldpV2RemTimeMark | 1.3.111.2.802.1.1.13.1.4.1.1.1 | N/A | TimeFilter | Time filter for lldpV2RemEntry
  lldpV2RemLocalIfIndex | 1.3.111.2.802.1.1.13.1.4.1.1.2 | N/A | InterfaceIndex | Port index
  lldpV2RemLocalDestMACAddress | 1.3.111.2.802.1.1.13.1.4.1.1.3 | N/A | LldpV2DestAddressTableIndex | Destination MAC address
  lldpV2RemIndex | 1.3.111.2.802.1.1.13.1.4.1.1.4 | N/A | Unsigned32(1..2147483647) | Remote system index
  lldpV2RemChassisIdSubtype | 1.3.111.2.802.1.1.13.1.4.1.1.5 | R/O | LldpV2ChassisIdSubtype | Subtype of chassis ID
  lldpV2RemChassisId | 1.3.111.2.802.1.1.13.1.4.1.1.6 | R/O | LldpV2ChassisId | Chassis ID
  lldpV2RemPortIdSubtype | 1.3.111.2.802.1.1.13.1.4.1.1.7 | R/O | LldpV2PortIdSubtype | Subtype of port ID
  lldpV2RemPortId | 1.3.111.2.802.1.1.13.1.4.1.1.8 | R/O | LldpV2PortId | Port ID
  lldpV2RemPortDesc | 1.3.111.2.802.1.1.13.1.4.1.1.9 | R/O | SnmpAdminString (SIZE (0..255)) | Port description
  lldpV2RemSysName | 1.3.111.2.802.1.1.13.1.4.1.1.10 | R/O | SnmpAdminString (SIZE (0..255)) | System name
  lldpV2RemSysDesc | 1.3.111.2.802.1.1.13.1.4.1.1.11 | R/O | SnmpAdminString (SIZE (0..255)) | System description
  lldpV2RemSysCapSupported | 1.3.111.2.802.1.1.13.1.4.1.1.12 | R/O | LldpV2SystemCapabilitiesMap | Functions supported by the system
  lldpV2RemSysCapEnabled | 1.3.111.2.802.1.1.13.1.4.1.1.13 | R/O | LldpV2SystemCapabilitiesMap | Functions enabled on the system
  lldpV2RemRemoteChanges | 1.3.111.2.802.1.1.13.1.4.1.1.14 | R/O | TruthValue | Flag indicating that a change in the MIB occurred on the remote device
  lldpV2RemTooManyNeighbors | 1.3.111.2.802.1.1.13.1.4.1.1.15 | R/O | TruthValue | Flag indicating that the number of connected remote devices exceeded the limit of the management table
  lldpV2RemManAddrTable | 1.3.111.2.802.1.1.13.1.4.2 | N/A |  | Table of remote system management addresses
  | lldpV2RemManAddrEntry | 1.3.111.2.802.1.1.13.1.4.2.1 | N/A |  | INDEX * lldpV2RemTimeMark * lldpV2RemLocalIfIndex * lldpV2RemLocalDestMACAddress * lldpV2RemIndex * lldpV2RemManAddrSubtype * lldpV2RemManAddr
  | lldpV2RemManAddrSubtype | 1.3.111.2.802.1.1.13.1.4.2.1.1 | N/A | AddressFamilyNumbers | Sub-type for management address
  lldpV2RemManAddr | 1.3.111.2.802.1.1.13.1.4.2.1.2 | N/A | LldpV2ManAddress | Remote system management addresses
  lldpV2RemManAddrIfSubtype | 1.3.111.2.802.1.1.13.1.4.2.1.3 | R/O | LldpV2ManAddrIfSubtype | Interface sub-type
  lldpV2RemManAddrIfId | 1.3.111.2.802.1.1.13.1.4.2.1.4 | R/O | Unsigned32 | Interface ID
  lldpV2RemManAddrOID | 1.3.111.2.802.1.1.13.1.4.2.1.5 | R/O | OBJECT IDENTIFIER | OID of management address
  lldpV2RemUnknownTLVTable | 1.3.111.2.802.1.1.13.1.4.3 | N/A |  | Table of undefined TLV information
  | lldpV2RemUnknownTLVEntry | 1.3.111.2.802.1.1.13.1.4.3.1 | N/A |  | INDEX * lldpV2RemTimeMark * lldpV2RemLocalIfIndex * lldpV2RemLocalDestMACAddress * lldpV2RemIndex * lldpV2RemUnknownTLVType
  | lldpV2RemUnknownTLVType | 1.3.111.2.802.1.1.13.1.4.3.1.1 | N/A | Unsigned32(9..126) | Undefined TLV types
  lldpV2RemUnknownTLVInfo | 1.3.111.2.802.1.1.13.1.4.3.1.2 | R/O | OCTET STRING (SIZE (0..511)) | Information for undefined TLVs
  lldpV2RemOrgDefInfoTable | 1.3.111.2.802.1.1.13.1.4.4 | N/A |  | Table for OUI information
  | lldpV2RemOrgDefInfoEntry | 1.3.111.2.802.1.1.13.1.4.4.1 | N/A |  | INDEX * lldpV2RemTimeMark * lldpV2RemLocalIfIndex * lldpV2RemLocalDestMACAddress * lldpV2RemIndex * lldpV2RemOrgDefInfoOUI * lldpV2RemOrgDefInfoSubtype * lldpV2RemOrgDefInfoIndex
  | lldpV2RemOrgDefInfoOUI | 1.3.111.2.802.1.1.13.1.4.4.1.1 | N/A | OCTET STRING (SIZE (3)) | OUI information for remote system
  lldpV2RemOrgDefInfoSubtype | 1.3.111.2.802.1.1.13.1.4.4.1.2 | N/A | Unsigned32(1..255) | OUI information sub-type for remote system
  lldpV2RemOrgDefInfoIndex | 1.3.111.2.802.1.1.13.1.4.4.1.3 | N/A | Unsigned32(1..2147483647) | Index for OUI information and OUI information sub-types
  lldpV2RemOrgDefInfo | 1.3.111.2.802.1.1.13.1.4.4.1.4 | R/O | OCTET STRING (SIZE (0..507)) | Information defined for each organization

- lldpV2Xdot3LocalData group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpV2Xdot3LocPowerTable | 1.3.111.2.802.1.1.13.1.5.4623.1.2.2 | N/A |  | POE information table for each port
  | lldpV2Xdot3LocPowerEntry | 1.3.111.2.802.1.1.13.1.5.4623.1.2.2.1 | N/A |  | INDEX * lldpV2LocPortIfIndex
  | lldpV2Xdot3LocPowerPortClass | 1.3.111.2.802.1.1.13.1.5.4623.1.2.2.1.1 | R/O | LldpV2PowerPortClass | PSE or PD status
  lldpV2Xdot3LocPowerMDISupported | 1.3.111.2.802.1.1.13.1.5.4623.1.2.2.1.2 | R/O | TruthValue | Power supply capability support status
  lldpV2Xdot3LocPowerMDIEnabled | 1.3.111.2.802.1.1.13.1.5.4623.1.2.2.1.3 | R/O | TruthValue | Enables/disables the power supply capability
  lldpV2Xdot3LocPowerPairControlable | 1.3.111.2.802.1.1.13.1.5.4623.1.2.2.1.4 | R/O | TruthValue | Ability to select wiring to be used for power supply
  lldpV2Xdot3LocPowerPairs | 1.3.111.2.802.1.1.13.1.5.4623.1.2.2.1.5 | R/O | Unsigned32(1|2) | Selection of wiring to be used for power supply
  lldpV2Xdot3LocPowerClass | 1.3.111.2.802.1.1.13.1.5.4623.1.2.2.1.6 | R/O | Unsigned32(1|2|3|4|5) | Power class

- lldpV2Xdot3RemoteData group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  lldpV2Xdot3RemPowerTable | 1.3.111.2.802.1.1.13.1.5.4623.1.3.2 | N/A |  | POE information for remote system
  | lldpV2Xdot3RemPowerEntry | 1.3.111.2.802.1.1.13.1.5.4623.1.3.2.1 | N/A |  | INDEX * lldpV2RemTimeMark * lldpV2RemLocalIfIndex * lldpV2RemLocalDestMACAddress * lldpV2RemIndex
  | lldpV2Xdot3RemPowerPortClass | 1.3.111.2.802.1.1.13.1.5.4623.1.3.2.1.1 | R/O | LldpV2PowerPortClass | PSE or PD status
  lldpV2Xdot3RemPowerMDISupported | 1.3.111.2.802.1.1.13.1.5.4623.1.3.2.1.2 | R/O | TruthValue | Power supply capability support
  lldpV2Xdot3RemPowerMDIEnabled | 1.3.111.2.802.1.1.13.1.5.4623.1.3.2.1.3 | R/O | TruthValue | Enables/disables the power supply capability
  lldpV2Xdot3RemPowerPairControlable | 1.3.111.2.802.1.1.13.1.5.4623.1.3.2.1.4 | R/O | TruthValue | Ability to select the signal line to be used for power supply
  lldpV2Xdot3RemPowerPairs | 1.3.111.2.802.1.1.13.1.5.4623.1.3.2.1.5 | R/O | Unsigned32(1|2) | Signal line to be used for power supply
  lldpV2Xdot3RemPowerClass | 1.3.111.2.802.1.1.13.1.5.4623.1.3.2.1.6 | R/O | Unsigned32(1|2|3|4|5) | Port power class

#### 4.3. lagMIB group

This MIB is related to LACP link aggregation information.
The syntax defined for the lagMIB group is shown below.

- Syntax defined in the lagMIB group

  Syntax | Definition
  --- | ---
  LacpKey | INTEGER (1..127) Note: Although this is INTEGER (0..65535) as per the standards, on this product it is in the range of INTEGER (1..127)
  LacpState | BITS * lacpActivity(0) * lacpTimeout(1) * aggregation(2) * synchronization(3) * collecting(4) * distributing(5) * defaulted(6) * expired(7)
  ChurnState | INTEGER * noChurn(1) * churn(2) * churnMonitor(3)

The lagMIB group is divided into subgroups such as those shown below.

       lagMIB(43)
         |
         +--lagMIBObjects(1)
             |
             +--dot3adAgg(1)
             |
             +--dot3adAggPort(2)
             |
             +--dot3adTablesLastChanged(3)

- dot3adAgg group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  dot3adAggTable | 1.2.840.10006.300.43.1.1.1 | N/A |  | LACP information table for system
  | dot3adAggEntry | 1.2.840.10006.300.43.1.1.1.1 | N/A |  | INDEX * dot3adAggIndex
  | dot3adAggIndex | 1.2.840.10006.300.43.1.1.1.1.1 | N/A | InterfaceIndex | LACP logical interface number
  dot3adAggMACAddress | 1.2.840.10006.300.43.1.1.1.1.2 | R/O | MacAddress | MAC address for LACP logical interface
  dot3adAggActorSystemPriority | 1.2.840.10006.300.43.1.1.1.1.3 | R/NW | INTEGER (1..65535) Note: Although this is INTEGER (0..65535) as per the standards, on this product it is in the range of INTEGER (1..65535) Same applies to other priority-related lagMIB | LACP system priority for this device
  dot3adAggActorSystemID | 1.2.840.10006.300.43.1.1.1.1.4 | R/NW | MacAddress | LACP system ID for the device itself
  dot3adAggAggregateOrIndividual | 1.2.840.10006.300.43.1.1.1.1.5 | R/O | TruthValue | Whether operating as Aggregate (true) or as individual links (alternate waiting ports) (false)
  dot3adAggActorAdminKey | 1.2.840.10006.300.43.1.1.1.1.6 | R/NW | LacpKey | ADMIN Key (identifier ID for the LACP logical interface) used in managing this device + “Used in managing” means the setting values for ADMIN properties or the config value. Same applies to other lagMIB
  dot3adAggActorOperKey | 1.2.840.10006.300.43.1.1.1.1.7 | R/O | LacpKey | ADMIN Key (identifier ID for the LACP logical interface) used in operation, for this device + “Used in operating” means the current values of the current operation, which are exchanged by the LACP protocol. Same applies to other lagMIB
  dot3adAggPartnerSystemID | 1.2.840.10006.300.43.1.1.1.1.8 | R/O | MacAddress | LACP system ID of the opposing device
  dot3adAggPartnerSystemPriority | 1.2.840.10006.300.43.1.1.1.1.9 | R/O | INTEGER (1..65535) | LACP system priority for the opposing device
  dot3adAggPartnerOperKey | 1.2.840.10006.300.43.1.1.1.1.10 | R/O | LacpKey | ADMIN Key (identifier ID for the LACP logical interface) used in operation, for the opposing device
  dot3adAggCollectorMaxDelay | 1.2.840.10006.300.43.1.1.1.1.11 | R/NW | INTEGER (0..65535) | Delay time from when the LACP packet is received to the time it is reflected in operation
  dot3adAggPortListTable | 1.2.840.10006.300.43.1.1.2 | N/A |  | LACP port list table for the system
  | dot3adAggPortListEntry | 1.2.840.10006.300.43.1.1.2.1 | N/A |  | INDEX * dot3adAggIndex
  | dot3adAggPortListPorts | 1.2.840.10006.300.43.1.1.2.1.1 | R/O | PortList | List of ports used by the LACP. Shown as an interface (port) bitmap. Bits are assigned in the following order starting from the most significant bit: port1.1 …​ port1.51, port1.52, port2.1 …​ port2.51, port2.52 For example, if port1.4 and port2.4 are used, the following value in hexadecimal will be indicated. 10 00 00 00 00 00 01 00 00 00 00 00 00

- dot3adAggPort group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  dot3adAggPortTable | 1.2.840.10006.300.43.1.2.1 | N/A |  | Table of information for ports used by the LACP
  | dot3adAggPortEntry | 1.2.840.10006.300.43.1.2.1.1 | N/A |  | INDEX * dot3adAggPortIndex
  | dot3adAggPortIndex | 1.2.840.10006.300.43.1.2.1.1.1 | N/A | InterfaceIndex | Port interface number
  dot3adAggPortActorSystemPriority | 1.2.840.10006.300.43.1.2.1.1.2 | R/NW | INTEGER (1..65535) | LACP system priority for this device
  dot3adAggPortActorSystemID | 1.2.840.10006.300.43.1.2.1.1.3 | R/O | MacAddress | LACP system ID for the device itself
  dot3adAggPortActorAdminKey | 1.2.840.10006.300.43.1.2.1.1.4 | R/NW | LacpKey | ADMIN Key (identifier ID for the LACP logical interface) used in managing this device
  dot3adAggPortActorOperKey | 1.2.840.10006.300.43.1.2.1.1.5 | R/NW | LacpKey | ADMIN Key (identifier ID for the LACP logical interface) used in operation, for this device
  dot3adAggPortPartnerAdminSystemPriority | 1.2.840.10006.300.43.1.2.1.1.6 | R/NW | INTEGER (1..65535) | LACP system priority used in management, for the opposing device
  dot3adAggPortPartnerOperSystemPriority | 1.2.840.10006.300.43.1.2.1.1.7 | R/O | INTEGER (1..65535) | LACP system priority used in operation, for the opposing device
  dot3adAggPortPartnerAdminSystemID | 1.2.840.10006.300.43.1.2.1.1.8 | R/NW | MacAddress | LACP system ID used in management, for the opposing device
  dot3adAggPortPartnerOperSystemID | 1.2.840.10006.300.43.1.2.1.1.9 | R/O | MacAddress | LACP system ID used in operation, for the opposing device
  dot3adAggPortPartnerAdminKey | 1.2.840.10006.300.43.1.2.1.1.10 | R/NW | LacpKey | ADMIN Key (identifier ID for the LACP logical interface) used in management, for the opposing device
  dot3adAggPortPartnerOperKey | 1.2.840.10006.300.43.1.2.1.1.11 | R/O | LacpKey | ADMIN Key (identifier ID for the LACP logical interface) used in operation, for the opposing device
  dot3adAggPortSelectedAggID | 1.2.840.10006.300.43.1.2.1.1.12 | R/O | InterfaceIndex | Logical interface number selected by the port
  dot3adAggPortAttachedAggID | 1.2.840.10006.300.43.1.2.1.1.13 | R/O | InterfaceIndex | Logical interface number connected to the port
  dot3adAggPortActorPort | 1.2.840.10006.300.43.1.2.1.1.14 | R/O | INTEGER (0..65535) | Physical interface number of this device
  dot3adAggPortActorPortPriority | 1.2.840.10006.300.43.1.2.1.1.15 | R/NW | INTEGER (0..65535) | Port priority for physical interface of this device
  dot3adAggPortPartnerAdminPort | 1.2.840.10006.300.43.1.2.1.1.16 | R/NW | INTEGER (0..65535) | Physical interface number used in management, for the opposing device
  dot3adAggPortPartnerOperPort | 1.2.840.10006.300.43.1.2.1.1.17 | R/O | INTEGER (0..65535) | Physical interface number used in operation, for the opposing device
  dot3adAggPortPartnerAdminPortPriority | 1.2.840.10006.300.43.1.2.1.1.18 | R/NW | INTEGER (1..65535) | Port priority of physical interface used in management, for the opposing device
  dot3adAggPortPartnerOperPortPriority | 1.2.840.10006.300.43.1.2.1.1.19 | R/O | INTEGER (1..65535) | Port priority for physical interface used in operation, for the opposing device
  dot3adAggPortActorAdminState | 1.2.840.10006.300.43.1.2.1.1.20 | R/NW | LacpState | Actor_State used in management, for this device + Actor_State is a status variable that shows internal transitions
  dot3adAggPortActorOperState | 1.2.840.10006.300.43.1.2.1.1.21 | R/O | LacpState | Actor_State used in operation, for this device
  dot3adAggPortPartnerAdminState | 1.2.840.10006.300.43.1.2.1.1.22 | R/NW | LacpState | Actor_State used in management, for the opposing device
  dot3adAggPortPartnerOperState | 1.2.840.10006.300.43.1.2.1.1.23 | R/O | LacpState | Actor_State used in operation, for the opposing device
  dot3adAggPortAggregateOrIndividual | 1.2.840.10006.300.43.1.2.1.1.24 | R/O | TruthValue | Whether Aggregate (true), or individual physical interfaces (alternate waiting ports) (false)
  dot3adAggPortStatsTable | 1.2.840.10006.300.43.1.2.2 | N/A |  | Table of statistical information for ports used by the LACP
  | dot3adAggPortStatsEntry | 1.2.840.10006.300.43.1.2.2.1 | N/A |  | INDEX * dot3adAggPortIndex
  | dot3adAggPortStatsLACPDUsRx | 1.2.840.10006.300.43.1.2.2.1.1 | R/O | Counter32 | No. of correct LACPDU received by the physical interface
  dot3adAggPortStatsMarkerPDUsRx | 1.2.840.10006.300.43.1.2.2.1.2 | R/O | Counter32 | No. of correct marker frames received by the physical interface
  dot3adAggPortStatsMarkerResponsePDUsRx | 1.2.840.10006.300.43.1.2.2.1.3 | R/O | Counter32 | No. of correct marker response frames received by the physical interface
  dot3adAggPortStatsUnknownRx | 1.2.840.10006.300.43.1.2.2.1.4 | R/O | Counter32 | No. of unknown frames received by the physical interface
  dot3adAggPortStatsIllegalRx | 1.2.840.10006.300.43.1.2.2.1.5 | R/O | Counter32 | No. of frames received by the physical interface on which the EtherType was 0x8809 but the PDU was invalid
  dot3adAggPortStatsLACPDUsTx | 1.2.840.10006.300.43.1.2.2.1.6 | R/O | Counter32 | No. of LACPDU transmitted from physical interface
  dot3adAggPortStatsMarkerPDUsTx | 1.2.840.10006.300.43.1.2.2.1.7 | R/O | Counter32 | No. of marker frames transmitted from physical interface
  dot3adAggPortStatsMarkerResponsePDUsTx | 1.2.840.10006.300.43.1.2.2.1.8 | R/O | Counter32 | No. of marker response frames transmitted from physical interface
  dot3adAggPortDebugTable | 1.2.840.10006.300.43.1.2.3 | N/A |  | Debug information table for ports used by the LACP
  | dot3adAggPortDebugEntry | 1.2.840.10006.300.43.1.2.3.1 | N/A |  | INDEX * dot3adAggPortIndex
  | dot3adAggPortDebugRxState | 1.2.840.10006.300.43.1.2.3.1.1 | R/O | INTEGER * current(1) * expired(2) * defaulted(3) * initialize(4) * lacpDisabled(5) * portDisabled(6) | Status of LACP protocol “Receive machine” transition variable
  dot3adAggPortDebugLastRxTime | 1.2.840.10006.300.43.1.2.3.1.2 | R/O | TimeTicks | Internal time when logical interface last received data
  dot3adAggPortDebugMuxState | 1.2.840.10006.300.43.1.2.3.1.3 | R/O | INTEGER * detached(1) * waiting(2) * attached(3) * collecting(4) * distributing(5) * collecting_distributing(6) | Status of LACP protocol “Mux machine” transition variable
  dot3adAggPortDebugMuxReason | 1.2.840.10006.300.43.1.2.3.1.4 | R/O | DisplayString | Reason why most recent LACP protocol “Mux machine” transition variable was changed
  dot3adAggPortDebugActorChurnState | 1.2.840.10006.300.43.1.2.3.1.5 | R/O | ChurnState | Status of “Churn Detection” transition variable for LACP protocol of this device
  dot3adAggPortDebugPartnerChurnState | 1.2.840.10006.300.43.1.2.3.1.6 | R/O | ChurnState | Status of LACP protocol “Churn Detection” transition variable for the opposing device
  dot3adAggPortDebugActorChurnCount | 1.2.840.10006.300.43.1.2.3.1.7 | R/O | Counter32 | No. of times that the LACP protocol “Churn Detection” status variable changed to ACTOR_CHURN status
  dot3adAggPortDebugPartnerChurnCount | 1.2.840.10006.300.43.1.2.3.1.8 | R/O | Counter32 | No. of times that LACP protocol “Churn Detection” status variable changed to PARTNER_CHURN status
  dot3adAggPortDebugActorSyncTransitionCount | 1.2.840.10006.300.43.1.2.3.1.9 | R/O | Counter32 | No. of times that LACP protocol “Mux machine” status variable of this device changed to IN_SYNC status
  dot3adAggPortDebugPartnerSyncTransitionCount | 1.2.840.10006.300.43.1.2.3.1.10 | R/O | Counter32 | No. of times that the LACP protocol “Mux machine” status variable of the opposing device changed to IN_SYNC status
  dot3adAggPortDebugActorChangeCount | 1.2.840.10006.300.43.1.2.3.1.11 | R/O | Counter32 | No. of times that the LAG ID of this device was changed
  dot3adAggPortDebugPartnerChangeCount | 1.2.840.10006.300.43.1.2.3.1.12 | R/O | Counter32 | No. of times that the LAG ID of the opposing device was changed

- dot3adTablesLastChanged group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  dot3adTablesLastChanged | 1.2.840.10006.300.43.1.3 | R/O | TimeTicks | Most recent time in which Dot3adAggTable, dot3adAggPortListTable, or dot3adAggPortTable was changed Note: This is always “0” on this product

#### 4.4. system group

This MIB is related to system information.

- system group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  sysDescr | 1.3.6.1.2.1.1.1 | R/O | DisplayString (SIZE (0..255)) | The description of the device. Device name and firmware revision
  sysObjectID | 1.3.6.1.2.1.1.2 | R/O | OBJECT IDENTIFIER | Device OID that is defined by Yamaha’s private MIB
  sysUpTimeInstance | 1.3.6.1.2.1.1.3 | R/O | TimeTicks | Elapsed time from boot
  sysContact | 1.3.6.1.2.1.1.4 | R/W | DisplayString (SIZE (0..255)) | Administrator contact information Setting value for snmp-server contact command
  sysName | 1.3.6.1.2.1.1.5 | R/W | DisplayString (SIZE (0..255)) | Administrative name Setting value for hostname command
  sysLocation | 1.3.6.1.2.1.1.6 | R/W | DisplayString (SIZE (0..255)) | Device location Setting value for snmp-server location command
  sysServices | 1.3.6.1.2.1.1.7 | R/O | INTEGER (0..127) | Value that indicates services the device supports

#### 4.5. interface group

This MIB is related to interface information.

- interface group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  ifNumber | 1.3.6.1.2.1.2.1 | R/O | Integer32 | No. of interfaces
  ifTable | 1.3.6.1.2.1.2.2 | N/A |  | Table of interface information Counters with a VLAN ifIndex value count the total traffic of all physical ports associated to the VLAN
  | ifEntry | 1.3.6.1.2.1.2.2.1 | N/A |  | INDEX * ifIndex
  | ifIndex | 1.3.6.1.2.1.2.2.1.1 | R/O | InterfaceIndex | Interface ID number
  ifDescr | 1.3.6.1.2.1.2.2.1.2 | R/O | DisplayString (SIZE (0..255)) | Description of the interface. Interface name
  ifType | 1.3.6.1.2.1.2.2.1.3 | R/O | IANAifType * ethernetCsmacd(6) * l3ipvlan(136), etc. | Types of interfaces
  ifMtu | 1.3.6.1.2.1.2.2.1.4 | R/O | Integer32 | Maximum frame size that can be transmitted/received
  ifSpeed | 1.3.6.1.2.1.2.2.1.5 | R/O | Gauge32 | Interface speed
  ifPhysAddress | 1.3.6.1.2.1.2.2.1.6 | R/O | PhysAddress | MAC address
  ifAdminStatus | 1.3.6.1.2.1.2.2.1.7 | R/W | INTEGER * up(1) * down(2) | Desirable interface status
  ifOperStatus | 1.3.6.1.2.1.2.2.1.8 | R/O | INTEGER * up(1) * down(2) | Current status of interface
  ifLastChange | 1.3.6.1.2.1.2.2.1.9 | R/O | TimeTicks | Time when the interface changed to the current status (elapsed time from boot)
  ifInOctets | 1.3.6.1.2.1.2.2.1.10 | R/O | Counter32 | Total no. of octets received
  ifInUcastPkts | 1.3.6.1.2.1.2.2.1.11 | R/O | Counter32 | No. of unicast packets notified to higher protocol
  ifInNUcastPkts | 1.3.6.1.2.1.2.2.1.12 | R/O | Counter32 | Number of non-unicast packets notified to higher protocol
  ifInDiscards | 1.3.6.1.2.1.2.2.1.13 | R/O | Counter32 | No. of packets that were discarded, despite no errors detected
  ifInErrors | 1.3.6.1.2.1.2.2.1.14 | R/O | Counter32 | No. of packets not notified to higher protocol due to errors
  ifInUnknownProtos | 1.3.6.1.2.1.2.2.1.15 | R/O | Counter32 | No. of discarded packets, due to an unsupported protocol
  ifOutOctets | 1.3.6.1.2.1.2.2.1.16 | R/O | Counter32 | Total no. of octets transmitted
  ifOutUcastPkts | 1.3.6.1.2.1.2.2.1.17 | R/O | Counter32 | No. of unicast packets requested for transmission by a higher protocol
  ifOutNUcastPkts | 1.3.6.1.2.1.2.2.1.18 | R/O | Counter32 | No. of non-unicast packets requested for transmission by a higher protocol
  ifOutDiscards | 1.3.6.1.2.1.2.2.1.19 | R/O | Counter32 | No. of packets that were discarded for transmission, despite no errors detected
  ifOutErrors | 1.3.6.1.2.1.2.2.1.20 | R/O | Counter32 | No. of packets not transmitted due to errors
  ifSpecific | 1.3.6.1.2.1.2.2.1.22 | R/O | OBJECT IDENTIFIER | Reference to MIB that defines interface media characteristics + If no reference exists, this will be 0.0

#### 4.6. at group

This MIB is related to mapping information for physical addresses and network addresses.

- at group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  atTable | 1.3.6.1.2.1.3.1 | N/A |  | Table of mapping information for physical addresses and network addresses
  | atEntry | 1.3.6.1.2.1.3.1.1 | N/A |  | INDEX * atIfIndex * atNetAddress
  | atIfIndex | 1.3.6.1.2.1.3.1.1.1 | R/NW | INTEGER | ifIndex for the corresponding interface
  atPhysAddress | 1.3.6.1.2.1.3.1.1.2 | R/NW | PhysAddress | Physical address
  atNetAddress | 1.3.6.1.2.1.3.1.1.3 | R/NW | NetworkAddress | IP address corresponding to the physical address

#### 4.7. rmon group

This MIB is related to RMON information.
The syntax defined for the rmon group is shown below.

- Syntax defined in the rmon group

  Syntax | Definition
  --- | ---
  OwnerString | OCTET STRING (SIZE (0..127))
  EntryStatus | INTEGER * valid(1) * createRequest(2) * underCreation(3) * invalid(4)

The rmon group is divided into subgroups such as those shown below.

       rmon(16)
          |
          +--statistics(1)
          |
          +--history(2)
          |
          +--alarm(3)
          |
          +--event(9)

- statistics group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  etherStatsTable | 1.3.6.1.2.1.16.1.1 | N/A |  | Table of statistical information for Ethernet
  | etherStatsEntry | 1.3.6.1.2.1.16.1.1.1 | N/A |  | INDEX * etherStatsIndex
  | etherStatsIndex | 1.3.6.1.2.1.16.1.1.1.1 | R/O | Integer32 (1..65535) | Index of entries
  etherStatsDataSource | 1.3.6.1.2.1.16.1.1.1.2 | R/C | OBJECT IDENTIFIER | Interface being monitored
  etherStatsDropEvents | 1.3.6.1.2.1.16.1.1.1.3 | R/O | Counter32 | Number of drop packets
  etherStatsOctets | 1.3.6.1.2.1.16.1.1.1.4 | R/O | Counter32 | Number of octets received
  etherStatsPkts | 1.3.6.1.2.1.16.1.1.1.5 | R/O | Counter32 | Number of received packets
  etherStatsBroadcastPkts | 1.3.6.1.2.1.16.1.1.1.6 | R/O | Counter32 | Number of broadcast packets received
  etherStatsMulticastPkts | 1.3.6.1.2.1.16.1.1.1.7 | R/O | Counter32 | Number of multicast packets received
  etherStatsCRCAlignErrors | 1.3.6.1.2.1.16.1.1.1.8 | R/O | Counter32 | Number of FCS error packets received
  etherStatsUndersizePkts | 1.3.6.1.2.1.16.1.1.1.9 | R/O | Counter32 | Number of undersize packets received (packets smaller than 64 octets)
  etherStatsOversizePkts | 1.3.6.1.2.1.16.1.1.1.10 | R/O | Counter32 | Number of oversize packets received (packets larger than 1518 octets)
  etherStatsFragments | 1.3.6.1.2.1.16.1.1.1.11 | R/O | Counter32 | Number of fragment packets received (packets smaller than 64 octets with abnormal FCS)
  etherStatsJabbers | 1.3.6.1.2.1.16.1.1.1.12 | R/O | Counter32 | Number of jabber packets received (packets larger than 1518 octets with abnormal FCS)
  etherStatsCollisions | 1.3.6.1.2.1.16.1.1.1.13 | R/O | Counter32 | Number of collisions
  etherStatsOwner | 1.3.6.1.2.1.16.1.1.1.20 | R/C | OwnerString | Owner name
  etherStatsStatus | 1.3.6.1.2.1.16.1.1.1.21 | R/C | EntryStatus | Status of statistical group

- history group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  historyControlTable | 1.3.6.1.2.1.16.2.1 | N/A |  | Table of control information for the history group
  | historyControlEntry | 1.3.6.1.2.1.16.2.1.1 | N/A |  | INDEX * historyControlIndex
  | historyControlIndex | 1.3.6.1.2.1.16.2.1.1.1 | R/O | Integer32 (1..65535) | Index of entries
  historyControlDataSource | 1.3.6.1.2.1.16.2.1.1.2 | R/C | OBJECT IDENTIFIER | Interface being monitored
  historyControlBucketsRequested | 1.3.6.1.2.1.16.2.1.1.3 | R/C | Integer32 (1..65535) | Number of history group history saves requested
  historyControlBucketsGranted | 1.3.6.1.2.1.16.2.1.1.4 | R/O | Integer32 (1..65535) | Number of history group histories saved
  historyControlInterval | 1.3.6.1.2.1.16.2.1.1.5 | R/C | Integer32 (1..3600) | Interval at which history group histories are saved
  historyControlOwner | 1.3.6.1.2.1.16.2.1.1.6 | R/C | OwnerString | Owner name
  historyControlStatus | 1.3.6.1.2.1.16.2.1.1.7 | R/C | EntryStatus | History group status
  etherHistoryTable | 1.3.6.1.2.1.16.2.2 | N/A |  | Table of history information
  | etherHistoryEntry | 1.3.6.1.2.1.16.2.2.1 | N/A |  | INDEX * etherHistoryIndex * etherHistorySampleIndex
  | etherHistoryIndex | 1.3.6.1.2.1.16.2.2.1.1 | R/O | Integer32 (1..65535) | Same value as the index value of historyControlIndex
  etherHistorySampleIndex | 1.3.6.1.2.1.16.2.2.1.2 | R/O | Integer32 (1..2147483647) | Index of history entries
  etherHistoryIntervalStart | 1.3.6.1.2.1.16.2.2.1.3 | R/O | TimeTicks | Interval at which history group histories are saved
  etherHistoryDropEvents | 1.3.6.1.2.1.16.2.2.1.4 | R/O | Counter32 | Number of drop packets
  etherHistoryOctets | 1.3.6.1.2.1.16.2.2.1.5 | R/O | Counter32 | Number of octets received
  etherHistoryPkts | 1.3.6.1.2.1.16.2.2.1.6 | R/O | Counter32 | Number of received packets
  etherHistoryBroadcastPkts | 1.3.6.1.2.1.16.2.2.1.7 | R/O | Counter32 | Number of broadcast packets received
  etherHistoryMulticastPkts | 1.3.6.1.2.1.16.2.2.1.8 | R/O | Counter32 | Number of multicast packets received
  etherHistoryCRCAlignErrors | 1.3.6.1.2.1.16.2.2.1.9 | R/O | Counter32 | Number of FCS error packets received
  etherHistoryUndersizePkts | 1.3.6.1.2.1.16.2.2.1.10 | R/O | Counter32 | Number of undersize packets received (packets smaller than 64 octets)
  etherHistoryOversizePkts | 1.3.6.1.2.1.16.2.2.1.11 | R/O | Counter32 | Number of oversize packets received (packets larger than 1518 octets)
  etherHistoryFragments | 1.3.6.1.2.1.16.2.2.1.12 | R/O | Counter32 | Number of fragment packets received (packets smaller than 64 octets with abnormal FCS)
  etherHistoryJabbers | 1.3.6.1.2.1.16.2.2.1.13 | R/O | Counter32 | Number of jabber packets received (packets larger than 1518 octets with abnormal FCS)
  etherHistoryCollisions | 1.3.6.1.2.1.16.2.2.1.14 | R/O | Counter32 | Number of collisions
  etherHistoryUtilization | 1.3.6.1.2.1.16.2.2.1.15 | R/O | Integer32 (0..10000) | Estimated value of network usage ratio

- alarm group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  alarmTable | 1.3.6.1.2.1.16.3.1 | N/A |  | Table of information for the alarm group
  | alarmEntry | 1.3.6.1.2.1.16.3.1.1 | N/A |  | INDEX * alarmIndex
  | alarmIndex | 1.3.6.1.2.1.16.3.1.1.1 | R/O | Integer32 (1..65535) | Index of entries
  alarmInterval | 1.3.6.1.2.1.16.3.1.1.2 | R/C | Integer32 | Sampling interval
  alarmVariable | 1.3.6.1.2.1.16.3.1.1.3 | R/C | OBJECT IDENTIFIER | MIB object to be monitored
  alarmSampleType | 1.3.6.1.2.1.16.3.1.1.4 | R/C | INTEGER * absoluteValue(1) * deltaValue(2) | Sampling type
  alarmValue | 1.3.6.1.2.1.16.3.1.1.5 | R/O | Integer32 | Estimated value
  alarmStartupAlarm | 1.3.6.1.2.1.16.3.1.1.6 | R/C | INTEGER * risingAlarm(1) * fallingAlarm(2) * risingOrFallingAlarm(3) | Threshold value used for first alarm determination
  alarmRisingThreshold | 1.3.6.1.2.1.16.3.1.1.7 | R/C | Integer32 | Upper threshold value
  alarmFallingThreshold | 1.3.6.1.2.1.16.3.1.1.8 | R/C | Integer32 | Lower threshold value
  alarmRisingEventIndex | 1.3.6.1.2.1.16.3.1.1.9 | R/C | Integer32 (0..65535) | Event index when crossing upper limit
  alarmFallingEventIndex | 1.3.6.1.2.1.16.3.1.1.10 | R/C | Integer32 (0..65535) | Event index when crossing lower limit
  alarmOwner | 1.3.6.1.2.1.16.3.1.1.11 | R/C | OwnerString | Owner name
  alarmStatus | 1.3.6.1.2.1.16.3.1.1.12 | R/C | EntryStatus | Alarm group status

- event group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  eventTable | 1.3.6.1.2.1.16.9.1 | N/A |  | Table of information for event group
  | eventEntry | 1.3.6.1.2.1.16.9.1.1 | N/A |  | INDEX * eventIndex
  | eventIndex | 1.3.6.1.2.1.16.9.1.1.1 | R/O | Integer32 (1..65535) | Index of entries
  eventDescription | 1.3.6.1.2.1.16.9.1.1.2 | R/C | DisplayString (SIZE (0..127)) | Event description
  eventType | 1.3.6.1.2.1.16.9.1.1.3 | R/C | INTEGER * none(1) * log(2) * snmptrap(3) * logandtrap(4) | Event type
  eventCommunity | 1.3.6.1.2.1.16.9.1.1.4 | R/C | OCTET STRING (SIZE (0..127)) | Community name
  eventLastTimeSent | 1.3.6.1.2.1.16.9.1.1.5 | R/O | TimeTicks | Event execution time
  eventOwner | 1.3.6.1.2.1.16.9.1.1.6 | R/C | OwnerString | Owner name
  eventStatus | 1.3.6.1.2.1.16.9.1.1.7 | R/C | EntryStatus | Event group status

#### 4.8. dot1dBridge group

This MIB is related to dot1dBridge information.
The syntax defined in the dot1dBridge group is shown below.

- Syntax defined in the dot1dBridge group

  Syntax | Definition
  --- | ---
  BridgeId | OCTET STRING (SIZE (8))
  Timeout | Integer32
  PortList | OCTET STRING
  VlanIndex | Unsigned32
  VlanId | Integer32 (1..4094)

The dot1dBridge group is divided into subgroups such as those shown below.

       dot1dBridge(17)
          |
          +--dot1dBase(1)
          |
          +--dot1dStp(2)
          |
          +--dot1dTp(4)
          |
          +--dot1dStatic(5)
          |
          +--qBridgeMIB(7)
             |
             +--qBridgeMIBObjects(1)
                |
                +--dot1qBase(1)
                |
                +--dot1qTp(2)
                |
                +--dot1qVlan(4)

- dot1dBase group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  dot1dBaseBridgeAddress | 1.3.6.1.2.1.17.1.1 | R/O | MacAddress | MAC address of bridge
  dot1dBaseNumPorts | 1.3.6.1.2.1.17.1.2 | R/O | Integer32 | No. of ports for bridge
  dot1dBaseType | 1.3.6.1.2.1.17.1.3 | R/O | INTEGER * unknown(1) * transparent-only(2) * sourceroute-only(3) * srt(4) | Type of bridging executable by the bridge
  dot1dBasePortTable | 1.3.6.1.2.1.17.1.4 | N/A |  | Table of port information for bridge
  | dot1dBasePortEntry | 1.3.6.1.2.1.17.1.4.1 | N/A |  | INDEX * dot1dBasePort
  | dot1dBasePort | 1.3.6.1.2.1.17.1.4.1.1 | R/O | Integer32 (1..65535) | Port number
  dot1dBasePortIfIndex | 1.3.6.1.2.1.17.1.4.1.2 | R/O | InterfaceIndex | Instance value for ifIndex, defined by the IF-MIB of the interface corresponding to the port
  dot1dBasePortCircuit | 1.3.6.1.2.1.17.1.4.1.3 | R/O | OBJECT IDENTIFIER | Identifier used when the value of dot1dBasePortIfIndex is the same port in the bridge
  dot1dBasePortDelayExceededDiscards | 1.3.6.1.2.1.17.1.4.1.4 | R/O | Counter32 | No. of frames discarded at the port due to a bridge forwarding delay Note: This is always “0” on this product
  dot1dBasePortMtuExceededDiscards | 1.3.6.1.2.1.17.1.4.1.5 | R/O | Counter32 | No. of frames discarded at the port due to excessive size Note: This is always “0” on this product

- dot1dStp group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  dot1dStpProtocolSpecification | 1.3.6.1.2.1.17.2.1 | R/O | INTEGER * unknown(1) * decLb100(2) * ieee8021d(3) | Spanning tree protocol version
  dot1dStpPriority | 1.3.6.1.2.1.17.2.2 | R/NW | Integer32 (0..65535) | Bridge priority value
  dot1dStpTimeSinceTopologyChange | 1.3.6.1.2.1.17.2.3 | R/O | TimeTicks | Time elapsed since detecting a change in topology
  dot1dStpTopChanges | 1.3.6.1.2.1.17.2.4 | R/O | Counter32 | No. of times a change in topology has been detected
  dot1dStpDesignatedRoot | 1.3.6.1.2.1.17.2.5 | R/O | BridgeId | Root bridge identifier of spanning tree
  dot1dStpRootCost | 1.3.6.1.2.1.17.2.6 | R/O | Integer32 | Path cost to root bridge
  dot1dStpRootPort | 1.3.6.1.2.1.17.2.7 | R/O | Integer32 | Port number with the lowest cost from bridge to root bridge
  dot1dStpMaxAge | 1.3.6.1.2.1.17.2.8 | R/O | Timeout | Maximum time elapsed for spanning tree protocol information (in units of 1/100 sec.)
  dot1dStpHelloTime | 1.3.6.1.2.1.17.2.9 | R/O | Timeout | BPDU transmission interval (in units of 1/100 sec.)
  dot1dStpHoldTime | 1.3.6.1.2.1.17.2.10 | R/O | Integer32 | Minimum transmission interval for Configuration BPDU (in units of 1/100 sec.)
  dot1dStpForwardDelay | 1.3.6.1.2.1.17.2.11 | R/O | Timeout | Forward delay time (in units of 1/100 sec.)
  dot1dStpBridgeMaxAge | 1.3.6.1.2.1.17.2.12 | R/NW | Timeout (600..4000) | Setting value for maximum elapsed time
  dot1dStpBridgeHelloTime | 1.3.6.1.2.1.17.2.13 | R/NW | Timeout (100..1000) | Setting value for BPDU transmission interval
  dot1dStpBridgeForwardDelay | 1.3.6.1.2.1.17.2.14 | R/NW | Timeout (400..3000) | Setting value for forward delay time
  dot1dStpPortTable | 1.3.6.1.2.1.17.2.15 | N/A |  | Table of port information for spanning tree protocol
  | dot1dStpPortEntry | 1.3.6.1.2.1.17.2.15.1 | N/A |  | INDEX * dot1dStpPort
  | dot1dStpPort | 1.3.6.1.2.1.17.2.15.1.1 | R/O | Integer32 (1..65535) | Port number for spanning tree protocol
  dot1dStpPortPriority | 1.3.6.1.2.1.17.2.15.1.2 | R/NW | Integer32 (0..255) | Port priority value
  dot1dStpPortState | 1.3.6.1.2.1.17.2.15.1.3 | R/O | INTEGER * disabled(1) * blocking(2) * listening(3) * learning(4) * forwarding(5) * broken(6) | Port status
  dot1dStpPortEnable | 1.3.6.1.2.1.17.2.15.1.4 | R/NW | INTEGER * enabled(1) * disabled(2) | Port enabled/disabled status
  dot1dStpPortPathCost | 1.3.6.1.2.1.17.2.15.1.5 | R/NW | Integer32 (1..65535) | Path cost value for port
  dot1dStpPortDesignatedRoot | 1.3.6.1.2.1.17.2.15.1.6 | R/O | BridgeId | Root bridge identifier of configuration BPDU
  dot1dStpPortDesignatedCost | 1.3.6.1.2.1.17.2.15.1.7 | R/O | Integer32 | Path cost value for specified port
  dot1dStpPortDesignatedBridge | 1.3.6.1.2.1.17.2.15.1.8 | R/O | BridgeId | Specified bridge identifier
  dot1dStpPortDesignatedPort | 1.3.6.1.2.1.17.2.15.1.9 | R/O | OCTET STRING (SIZE (2)) | Port identifier for specified bridge
  dot1dStpPortForwardTransitions | 1.3.6.1.2.1.17.2.15.1.10 | R/O | Counter32 | No. of times that port switched from acquisition status to forwarding status
  dot1dStpPortPathCost32 | 1.3.6.1.2.1.17.2.15.1.11 | R/NW | Integer32 (1..200000000) | Path cost value for ports complying with IEEE 802.1t
  dot1dStpVersion | 1.3.6.1.2.1.17.2.16 | R/NW | INTEGER * stpCompatible(0) * rstp(2) | Spanning tree protocol version
  dot1dStpTxHoldCount | 1.3.6.1.2.1.17.2.17 | R/NW | Integer32 (1..10) | Forward hold count value
  dot1dStpExtPortTable | 1.3.6.1.2.1.17.2.19 | N/A |  | Table of port information for RSTP
  | dot1dStpExtPortEntry | 1.3.6.1.2.1.17.2.19.1 | N/A |  | AUGMENTS * dot1dStpPortEntry
  | dot1dStpPortProtocolMigration | 1.3.6.1.2.1.17.2.19.1.1 | R/NW | TruthValue | Writing “true(1)” to this object will cause the BPDU of the port to be forcibly transmitted Note: This is always “false(2)” when read
  dot1dStpPortAdminEdgePort | 1.3.6.1.2.1.17.2.19.1.2 | R/NW | TruthValue | Setting value for edge port
  dot1dStpPortOperEdgePort | 1.3.6.1.2.1.17.2.19.1.3 | R/O | TruthValue | Current value for edge port
  dot1dStpPortAdminPointToPoint | 1.3.6.1.2.1.17.2.19.1.4 | R/NW | INTEGER * forceTrue(0) * forceFalse(1) * auto(2) | Setting value for point-to-point of the port
  dot1dStpPortOperPointToPoint | 1.3.6.1.2.1.17.2.19.1.5 | R/O | TruthValue | Current value for point-to-point of the port
  dot1dStpPortAdminPathCost | 1.3.6.1.2.1.17.2.19.1.6 | R/NW | Integer32 (0..200000000) | Setting value for path cost of port

- dot1dTp group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  dot1dTpLearnedEntryDiscards | 1.3.6.1.2.1.17.4.1 | R/O | Counter32 | Amount of forwarding information that was discarded due to having exceeded the upper save limit of the forwarding database
  dot1dTpAgingTime | 1.3.6.1.2.1.17.4.2 | R/NW | Integer32 (10..1000000) | Timeout duration for aging out forwarding information that was actively acquired
  dot1dTpFdbTable | 1.3.6.1.2.1.17.4.3 | N/A |  | Table of unicast entries that have forwarding or filtering information
  | dot1dTpFdbEntry | 1.3.6.1.2.1.17.4.3.1 | N/A |  | INDEX * dot1dTpFdbAddress
  | dot1dTpFdbAddress | 1.3.6.1.2.1.17.4.3.1.1 | R/O | MacAddress | Unicast MAC addresses that have forwarding or filtering information
  dot1dTpFdbPort | 1.3.6.1.2.1.17.4.3.1.2 | R/O | Integer32 | Port number of port that transmitted a frame with a source address that is the same as the instance value, corresponding to the dot1dTpFdbAddress
  dot1dTpFdbStatus | 1.3.6.1.2.1.17.4.3.1.3 | R/O | INTEGER * other(1) * invalid(2) * learned(3) * self(4) * mgmt(5) | MAC address table status
  dot1dTpPortTable | 1.3.6.1.2.1.17.4.4 | N/A |  | Table for all port information that is associated with a transparent bridge
  | dot1dTpPortEntry | 1.3.6.1.2.1.17.4.4.1 | N/A |  | INDEX * dot1dTpPort
  | dot1dTpPort | 1.3.6.1.2.1.17.4.4.1.1 | R/O | Integer32 (1..65535) | Port numbers that include transparent bridge management information
  dot1dTpPortMaxInfo | 1.3.6.1.2.1.17.4.4.1.2 | R/O | Integer32 | Maximum size of information fields transmitted/received by a port
  dot1dTpPortInFrames | 1.3.6.1.2.1.17.4.4.1.3 | R/O | Counter32 | No. of frames received by a port
  dot1dTpPortOutFrames | 1.3.6.1.2.1.17.4.4.1.4 | R/O | Counter32 | No. of frames transmitted by a port
  dot1dTpPortInDiscards | 1.3.6.1.2.1.17.4.4.1.5 | R/O | Counter32 | No. of frames that are valid for reception, which were discarded during forwarding

- dot1dStatic group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  dot1dStaticTable | 1.3.6.1.2.1.17.5.1 | N/A |  | Table of filtering information that was registered statically
  | dot1dStaticEntry | 1.3.6.1.2.1.17.5.1.1 | N/A |  | INDEX * dot1dStaticAddress * dot1dStaticReceivePort
  | dot1dStaticAddress | 1.3.6.1.2.1.17.5.1.1.1 | R/NC | MacAddress | Destination MAC address for which filtering information is applied
  dot1dStaticReceivePort | 1.3.6.1.2.1.17.5.1.1.2 | R/NC | Integer32 (0..65535) | Reception port no. on which filtering information is applied
  dot1dStaticAllowedToGoTo | 1.3.6.1.2.1.17.5.1.1.3 | R/NC | OCTET STRING (SIZE (0..512)) | Set of ports on which to transmit frames to which filtering information was applied
  dot1dStaticStatus | 1.3.6.1.2.1.17.5.1.1.4 | R/NC | INTEGER * other(1) * invalid(2) * permanent(3) * deleteOnReset(4) * deleteOnTimeout(5) | Application status for filtering information

- dot1qBase group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  dot1qVlanVersionNumber | 1.3.6.1.2.1.17.7.1.1.1 | R/O | INTEGER * version1(1) | IEEE 802.1Q version information
  dot1qMaxVlanId | 1.3.6.1.2.1.17.7.1.1.2 | R/O | VlanId | Maximum no. of IEEE 802.1Q VLAN IDs
  dot1qMaxSupportedVlans | 1.3.6.1.2.1.17.7.1.1.3 | R/O | Unsigned32 | Maximum no. of IEEE 802.1Q VLANs
  dot1qNumVlans | 1.3.6.1.2.1.17.7.1.1.4 | R/O | Unsigned32 | No. of IEEE 802.1Q VLANs used

- dot1qTp group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  dot1qFdbTable | 1.3.6.1.2.1.17.7.1.2.1 | N/A |  | Filtering table
  | dot1qFdbEntry | 1.3.6.1.2.1.17.7.1.2.1.1 | N/A |  | INDEX * dot1qFdbId
  | dot1qFdbId | 1.3.6.1.2.1.17.7.1.2.1.1.1 | N/A | Unsigned32 | Identifier for filtering database
  dot1qFdbDynamicCount | 1.3.6.1.2.1.17.7.1.2.1.1.2 | R/O | Counter32 | No. of active entries in filtering database
  dot1qTpFdbTable | 1.3.6.1.2.1.17.7.1.2.2 | N/A |  | Table of information for unicast entries that have transparent bridge forwarding or filtering information
  | dot1qTpFdbEntry | 1.3.6.1.2.1.17.7.1.2.2.1 | N/A |  | INDEX * dot1qFdbId * dot1qTpFdbAddress
  | dot1qTpFdbAddress | 1.3.6.1.2.1.17.7.1.2.2.1.1 | N/A | MacAddress | Unicast MAC addresses that have transparent bridge forwarding or filtering information
  dot1qTpFdbPort | 1.3.6.1.2.1.17.7.1.2.2.1.2 | R/O | Integer32 (0..65535) | Port number of port that transmitted a frame with a source address that is the same as the instance value, corresponding to the transparent bridge dot1qTpFdbAddress
  dot1qTpFdbStatus | 1.3.6.1.2.1.17.7.1.2.2.1.3 | R/O | INTEGER * other(1) * invalid(2) * learned(3) * self(4) * mgmt(5) | Transparent bridge MAC address table status

- dot1qVlan group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  dot1qVlanNumDeletes | 1.3.6.1.2.1.17.7.1.4.1 | R/O | Counter32 | No. of VLAN entries that were deleted
  dot1qVlanCurrentTable | 1.3.6.1.2.1.17.7.1.4.2 | N/A |  | Table of VLAN entry information
  | dot1qVlanCurrentEntry | 1.3.6.1.2.1.17.7.1.4.2.1 | N/A |  | INDEX * dot1qVlanTimeMark * dot1qVlanIndex
  | dot1qVlanTimeMark | 1.3.6.1.2.1.17.7.1.4.2.1.1 | N/A | TimeFilter | Time filter for VLAN entries
  dot1qVlanIndex | 1.3.6.1.2.1.17.7.1.4.2.1.2 | N/A | VlanIndex | VLAN ID
  dot1qVlanFdbId | 1.3.6.1.2.1.17.7.1.4.2.1.3 | R/O | Unsigned32 | Filtering database used by VLAN
  dot1qVlanCurrentEgressPorts | 1.3.6.1.2.1.17.7.1.4.2.1.4 | R/O | PortList | Set of ports that output VLAN traffic as untagged or tagged frames
  dot1qVlanCurrentUntaggedPorts | 1.3.6.1.2.1.17.7.1.4.2.1.5 | R/O | PortList | Set of ports that transmit VLAN traffic as untagged frames
  dot1qVlanStatus | 1.3.6.1.2.1.17.7.1.4.2.1.6 | R/O | INTEGER * other(1) * permanent(2) * dynamicGvrp(3) | VLAN status
  dot1qVlanCreationTime | 1.3.6.1.2.1.17.7.1.4.2.1.7 | R/O | TimeTicks | sysUpTime value when creating VLAN
  dot1qVlanStaticTable | 1.3.6.1.2.1.17.7.1.4.3 | N/A |  | Table of VLAN static setting information
  | dot1qVlanStaticEntry | 1.3.6.1.2.1.17.7.1.4.3.1 | N/A |  | INDEX * dot1qVlanIndex
  | dot1qVlanStaticName | 1.3.6.1.2.1.17.7.1.4.3.1.1 | R/NC | SnmpAdminString (SIZE (0..32)) | Name assigned to VLAN
  dot1qVlanStaticEgressPorts | 1.3.6.1.2.1.17.7.1.4.3.1.2 | R/NC | PortList | Set of ports assigned to VLAN output list
  dot1qVlanForbiddenEgressPorts | 1.3.6.1.2.1.17.7.1.4.3.1.3 | R/NC | PortList | Set of ports prohibited from being included in the VLAN output list
  dot1qVlanStaticUntaggedPorts | 1.3.6.1.2.1.17.7.1.4.3.1.4 | R/NC | PortList | Set of ports that transmit VLAN output traffic as untagged frames
  dot1qVlanStaticRowStatus | 1.3.6.1.2.1.17.7.1.4.3.1.5 | R/NC | RowStatus | VLAN entry status
  dot1qNextFreeLocalVlanIndex | 1.3.6.1.2.1.17.7.1.4.4 | R/O | Integer32 (0|4096..2147483647) | Next VLAN ID that can be used
  dot1qPortVlanTable | 1.3.6.1.2.1.17.7.1.4.5 | N/A |  | Table of VLAN setting information for each port
  | dot1qPortVlanEntry | 1.3.6.1.2.1.17.7.1.4.5.1 | N/A |  | AUGMENTS * dot1dBasePortEntry
  | dot1qPvid | 1.3.6.1.2.1.17.7.1.4.5.1.1 | R/NW | VlanIndex | VLAN IDs assigned to untagged or priority tag frames
  dot1qPortAcceptableFrameTypes | 1.3.6.1.2.1.17.7.1.4.5.1.2 | R/NW | INTEGER * admitAll(1) * admitOnlyVlanTagged(2) | Frame types permitted for reception on the port
  dot1qPortIngressFiltering | 1.3.6.1.2.1.17.7.1.4.5.1.3 | R/NW | TruthValue | Filtering of received frames on a port

#### 4.9. ifMIB group

This MIB is related to additional information for the interface.
The ifMIB group is divided into subgroups such as those shown below.

       ifMIB(31)
          |
          +--ifMIBObjects(1)

- ifMIBObjects group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  ifXTable | 1.3.6.1.2.1.31.1.1 | N/A |  | Table of additional interface information Counters with a VLAN ifIndex value count the total traffic of all physical ports associated to the VLAN
  | ifXEntry | 1.3.6.1.2.1.31.1.1.1 | N/A |  | AUGMENTS * ifEntry
  | ifName | 1.3.6.1.2.1.31.1.1.1.1 | R/O | DisplayString | Interface name
  ifInMulticastPkts | 1.3.6.1.2.1.31.1.1.1.2 | R/O | Counter32 | Number of multicast packets notified to higher protocol
  ifInBroadcastPkts | 1.3.6.1.2.1.31.1.1.1.3 | R/O | Counter32 | Number of broadcast packets notified to higher protocol
  ifOutMulticastPkts | 1.3.6.1.2.1.31.1.1.1.4 | R/O | Counter32 | Number of multicast packets requested for transmission by a higher protocol
  ifOutBroadcastPkts | 1.3.6.1.2.1.31.1.1.1.5 | R/O | Counter32 | Number of broadcast packets requested for transmission by a higher protocol
  ifHCInOctets | 1.3.6.1.2.1.31.1.1.1.6 | R/O | Counter64 | Total number of octets received 64-bit version of ifInOctets
  ifHCOutOctets | 1.3.6.1.2.1.31.1.1.1.10 | R/O | Counter64 | Total number of octets sent 64-bit version of ifOutOctets
  ifHighSpeed | 1.3.6.1.2.1.31.1.1.1.15 | R/O | Gauge32 | The speed of the interface. Mbps
  ifAlias | 1.3.6.1.2.1.31.1.1.1.18 | R/NW | DisplayString (SIZE (0..64)) | Alias name of the interface * If the description command is set for the interface, that value will be used. * If the description command is not set, an empty character string will be set. * If a character string exceeding 64 characters set in the description command, only the first 64 characters are returned.

#### 4.10. entityMIB group

This MIB is related to entity information
The syntax defined in the entityMIB group is shown below.

- Syntax defined in the entityMIB group

  Syntax | Definition
  --- | ---
  PhysicalIndex | Integer32 (1..2147483647)

The entityMIB group is divided into subgroups such as those shown below.

       entityMIB(47)
          |
          +--entityMIBObjects(1)
             |
             +--entityPhysical(1)

- entityPhysical group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  entPhysicalTable | 1.3.6.1.2.1.47.1.1.1 | N/A |  | Table of entity information
  | entPhysicalEntry | 1.3.6.1.2.1.47.1.1.1.1 | N/A |  | INDEX * entPhysicalIndex
  | entPhysicalIndex | 1.3.6.1.2.1.47.1.1.1.1.1 | N/A | PhysicalIndex | Index of entities Stack ID This can be obtained with stack ID 1 if stack was not configured.
  entPhysicalSerialNum | 1.3.6.1.2.1.47.1.1.1.1.11 | R/NW | SnmpAdminString (SIZE (0..32)) | Serial number of device

#### 4.11. powerEthernetMIB group

This MIB is related to PoE information. The powerEthernetMIB group is divided into subgroups such as those shown below.

       powerEthernetMIB(105)
          |
          +--pethObjects(1)
             |
             +--pethMainPseObjects(3)
             |
             +--pethNotificationControl(4)

- pethObjects group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  pethPsePortTable | 1.3.6.1.2.1.105.1.1 | N/A |  | Table of port information for PoE
  | pethPsePortEntry | 1.3.6.1.2.1.105.1.1.1 | N/A |  | INDEX * pethPsePortGroupIndex * pethPsePortIndex
  | pethPsePortGroupIndex | 1.3.6.1.2.1.105.1.1.1.1 | N/A | Integer32 (1..2147483647) | Identifier for power supply device group Stack ID This can be obtained with stack ID 1 if stack was not configured.
  pethPsePortIndex | 1.3.6.1.2.1.105.1.1.1.2 | N/A | Integer32 (1..2147483647) | Identifier of the port in pethPsePortGroupIndex Port number
  pethPsePortAdminEnable | 1.3.6.1.2.1.105.1.1.1.3 | R/W | TruthValue | Enables/disables the power supply function
  pethPsePortPowerPairsControlAbility | 1.3.6.1.2.1.105.1.1.1.4 | R/O | TruthValue | Possible/not possible to switch the power supply target pair (fixed to false(2))
  pethPsePortPowerPairs | 1.3.6.1.2.1.105.1.1.1.5 | R/NW | INTEGER * signal(1) * spare(2) | Type of power supply target pair (fixed to signal(1))
  pethPsePortDetectionStatus | 1.3.6.1.2.1.105.1.1.1.6 | R/O | INTEGER * disabled(1) * searching(2) * deliveringPower(3) * fault(4) * test(5) * otherFault(6) | Power receiving device detection status fault(4) and test(5) are not used
  pethPsePortPowerPriority | 1.3.6.1.2.1.105.1.1.1.7 | R/W | INTEGER * critical(1) * high(2) * low(3) | Port power supply priority order
  pethPsePortType | 1.3.6.1.2.1.105.1.1.1.9 | R/W | SnmpAdminString (SIZE (0..64)) | Description about power supply port Setting value of the power-inline description command
  pethPsePortPowerClassifications | 1.3.6.1.2.1.105.1.1.1.10 | R/O | INTEGER * class0(1) * class1(2) * class2(3) * class3(4) * class4(5) | Information on the power supply class of the connected device * If no PoE device is connected, this value will be class0(1) * If a device of class5 or higher is connected, this value will be class4(5)

- pethMainPseObjects group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  pethMainPseTable | 1.3.6.1.2.1.105.1.3.1 | N/A |  | Table of main power supply unit information for power supply device
  | pethMainPseEntry | 1.3.6.1.2.1.105.1.3.1.1 | N/A |  | INDEX * pethMainPseGroupIndex
  | pethMainPseGroupIndex | 1.3.6.1.2.1.105.1.3.1.1.1 | N/A | Integer32 (1..2147483647) | Identifier for power supply device group Stack ID This can be obtained with stack ID 1 if stack was not configured.
  pethMainPsePower | 1.3.6.1.2.1.105.1.3.1.1.2 | R/O | Gauge32 (1..65535) | Total power of the power supply device (watts)
  pethMainPseOperStatus | 1.3.6.1.2.1.105.1.3.1.1.3 | R/O | INTEGER * on(1) * off(2) * faulty(3) | Power supply device control status
  pethMainPseConsumptionPower | 1.3.6.1.2.1.105.1.3.1.1.4 | R/O | Gauge32 | Power consumption of the power supply device (watts)
  pethMainPseUsageThreshold | 1.3.6.1.2.1.105.1.3.1.1.5 | R/NW | Integer32 (1..99) | Power consumption threshold value (percentage) for alarm notification + This product calculates this MIB value from the guardband value. The relational formula is as follows: pethMainPseUsageThreshold = ROUND (100 * (pethMainPsePower - Guard band value) / pethMainPsePower) The minimum value that can be specified is calculated using the following formula. Minimum = ROUND ((pethMainPsePower - 30) / pethMainPsePower) Note: ROUND indicates rounding off to the nearest whole number. If the calculation result is 100, the value of this MIB will be regarded as 99.

- pethNotificationControl group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  pethNotificationControlTable | 1.3.6.1.2.1.105.1.4.1 | N/A |  | Table of notification information display/control information for power supply devices
  | pethNotificationControlEntry | 1.3.6.1.2.1.105.1.4.1.1 | N/A |  | INDEX * pethNotificationControlGroupIndex
  | pethNotificationControlGroupIndex | 1.3.6.1.2.1.105.1.4.1.1.1 | N/A | Integer32 (1..2147483647) | Identifier for notification information group Stack ID This can be obtained with stack ID 1 if stack was not configured.
  pethNotificationControlEnable | 1.3.6.1.2.1.105.1.4.1.1.2 | R/W | TruthValue | Control of notification function. * true(1): Allows notifications * false(2): Prohibits notifications Corresponds to the powerethernet parameter of the snmp-server enable trap command

### 5. Private MIBs

The private MIBs that are supported by this product are shown below.

#### 5.1. yamahaSWHardware group

This MIB is related to hardware information for Yamaha switches.

- yamahaSWHardware group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  yshMemorySize | 1.3.6.1.4.1.1182.3.1.2 | R/O | INTEGER | Memory size
  yshFlashROMSize | 1.3.6.1.4.1.1182.3.1.3 | R/O | INTEGER | FlashROM size
  yshMemoryUtil | 1.3.6.1.4.1.1182.3.1.4 | R/O | Gauge (0..100) | Memory usage ratio
  yshCpuUtil5sec | 1.3.6.1.4.1.1182.3.1.5 | R/O | Gauge (0..100) | CPU usage ratio (5-second average)
  yshCpuUtil1min | 1.3.6.1.4.1.1182.3.1.6 | R/O | Gauge (0..100) | CPU usage ratio (1-minute average)
  yshCpuUtil5min | 1.3.6.1.4.1.1182.3.1.7 | R/O | Gauge (0..100) | CPU usage ratio (5-minute average)
  yshStackTable | 1.3.6.1.4.1.1182.3.1.19 | N/A |  | Table of hardware information for each member switch + This can only be obtained when a stack is configured.
  | yshStackEntry | 1.3.6.1.4.1.1182.3.1.19.1 | N/A |  | INDEX * yshStackId
  | yshStackId | 1.3.6.1.4.1.1182.3.1.19.1.1 | N/A | INTEGER (1..2147483647) | Stack ID
  yshStackMemorySize | 1.3.6.1.4.1.1182.3.1.19.1.2 | R/O | INTEGER | Memory size
  yshStackFlashROMSize | 1.3.6.1.4.1.1182.3.1.19.1.3 | R/O | INTEGER | FlashROM size
  yshStackMemoryUtil | 1.3.6.1.4.1.1182.3.1.19.1.4 | R/O | Gauge (0..100) | Memory usage ratio
  yshStackCpuUtil5sec | 1.3.6.1.4.1.1182.3.1.19.1.5 | R/O | Gauge (0..100) | CPU usage ratio (5-second average)
  yshStackCpuUtil1min | 1.3.6.1.4.1.1182.3.1.19.1.6 | R/O | Gauge (0..100) | CPU usage ratio (1-minute average)
  yshStackCpuUtil5min | 1.3.6.1.4.1.1182.3.1.19.1.7 | R/O | Gauge (0..100) | CPU usage ratio (5-minute average)
  yshEnableTemperatureTrap | 1.3.6.1.4.1.1182.3.1.20 | R/W | INTEGER * enabled(1) * disabled(2) | Setting value that determines whether SNMP traps based on temperature information are notified
  yshTemperatureTable | 1.3.6.1.4.1.1182.3.1.21 | N/A |  | Temperature information table
  | yshTemperatureEntry | 1.3.6.1.4.1.1182.3.1.21.1 | N/A |  | INDEX * yshTemperatureStackId * yshTemperatureDeviceType * yshTemperatureDeviceIndex
  | yshTemperatureStackId | 1.3.6.1.4.1.1182.3.1.21.1.1 | N/A | INTEGER (1..2147483647) | Stack ID This can be obtained with stack ID 1 if stack was not configured.
  yshTemperatureDeviceType | 1.3.6.1.4.1.1182.3.1.21.1.2 | N/A | INTEGER * cpu(1) * phy(2) * sfp(3) * thermal-sensor(4) * pse(5) * mac(6) | Device type
  yshTemperatureDeviceIndex | 1.3.6.1.4.1.1182.3.1.21.1.3 | N/A | INTEGER (1..2147483647) | Index for each device + For example, index values are 1 and 2 for devices with two CPUs
  yshTemperatureValue | 1.3.6.1.4.1.1182.3.1.21.1.4 | R/O | Gauge | Device temperature + If the device temperature was not measured, this is “0”
  yshTemperatureStatusTable | 1.3.6.1.4.1.1182.3.1.22 | N/A |  | Temperature status table
  | yshTemperatureStatusEntry | 1.3.6.1.4.1.1182.3.1.22.1 | N/A |  | INDEX * yshTemperatureStatusStackId * yshTemperatureStatusDeviceType
  | yshTemperatureStatusStackId | 1.3.6.1.4.1.1182.3.1.22.1.1 | N/A | INTEGER (1..2147483647) | Stack ID This can be obtained with stack ID 1 if stack was not configured.
  yshTemperatureStatusDeviceType | 1.3.6.1.4.1.1182.3.1.22.1.2 | N/A | INTEGER * cpu(1) * phy(2) * sfp(3) * thermal-sensor(4) * pse(5) * mac(6) | Device type
  yshTemperatureStatus | 1.3.6.1.4.1.1182.3.1.22.1.3 | R/O | INTEGER * normal(1) * warning(2) * error(3) | Temperature status * “Normal” when normal * “Warning” indicates temperature over High threshold value * “Error” indicates temperature exceeded alarm temperature
  yshTemperatureStatusNormalThreshold | 1.3.6.1.4.1.1182.3.1.22.1.4 | N/A | Gauge | Threshold value for determining Normal status Note: Only used for trap notifications
  yshTemperatureStatusWarningThreshold | 1.3.6.1.4.1.1182.3.1.22.1.5 | N/A | Gauge | Threshold value for determining Warning status Note: Only used for trap notifications
  yshTemperatureStatusErrorThreshold | 1.3.6.1.4.1.1182.3.1.22.1.6 | N/A | Gauge | Threshold value for determining Error status Note: Only used for trap notifications
  yshEnableFanTrap | 1.3.6.1.4.1.1182.3.1.23 | R/W | INTEGER * enabled(1) * disabled(2) | Setting value for determining whether SNMP traps based on fan information are notified
  yshFanTable | 1.3.6.1.4.1.1182.3.1.24 | N/A |  | Fan information table
  | yshFanEntry | 1.3.6.1.4.1.1182.3.1.24.1 | N/A |  | INDEX * yshFanStackId * yshFanIndex
  | yshFanStackId | 1.3.6.1.4.1.1182.3.1.24.1.1 | N/A | INTEGER (1..2147483647) | Stack ID This can be obtained with stack ID 1 if stack was not configured.
  yshFanIndex | 1.3.6.1.4.1.1182.3.1.24.1.2 | N/A | INTEGER (1..2147483647) | Index for each fan + For example, index values will be 1 and 2 for devices with two fans
  yshFanRpm | 1.3.6.1.4.1.1182.3.1.24.1.3 | R/O | Gauge | Fan RPM
  yshFanStatus | 1.3.6.1.4.1.1182.3.1.24.1.4 | R/O | INTEGER * normal(1) * stopped(2) | Fan status
  yshFanSpeedStatusTable | 1.3.6.1.4.1.1182.3.1.25 | N/A |  | Fan RPM status table
  | yshFanSpeedStatusEntry | 1.3.6.1.4.1.1182.3.1.25.1 | N/A |  | INDEX * yshFanSpeedStatusStackId
  | yshFanSpeedStatusStackId | 1.3.6.1.4.1.1182.3.1.25.1.1 | N/A | INTEGER (1..2147483647) | Stack ID This can be obtained with stack ID 1 if stack was not configured.
  yshFanSpeedStatus | 1.3.6.1.4.1.1182.3.1.25.1.2 | R/O | INTEGER * low(1) * middle(2) * high(3) * max-speed(4) * middle-high(5) * high-alarm(6) | Fan RPM status

#### 5.2. yamahaSWFirmware group

This MIB is related to firmware information for Yamaha switches.

- yamahaSWFirmware group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  ysfConfigFile | 1.3.6.1.4.1.1182.3.2.2 | R/O | DisplayString (SIZE (0..255)) | Startup config
  ysfRevision | 1.3.6.1.4.1.1182.3.2.3 | R/O | DisplayString (SIZE (0..255)) | Firmware version
  ysfUpTime | 1.3.6.1.4.1.1182.3.2.4 | R/O | TimeTicks | Elapsed time from boot
  ysfRestart | 1.3.6.1.4.1.1182.3.2.11 | R/W | INTEGER * nothing(1) * restart(2) | The system will reboot when the “restart” value is written
  ysfStackTable | 1.3.6.1.4.1.1182.3.2.12 | N/A |  | Table of firmware information for each member switch + This can only be obtained when a stack is configured.
  | ysfStackEntry | 1.3.6.1.4.1.1182.3.2.12.1 | N/A |  | INDEX * ysfStackId
  | ysfStackId | 1.3.6.1.4.1.1182.3.2.12.1.1 | N/A | INTEGER (1..2147483647) | Stack ID
  ysfStackUpTime | 1.3.6.1.4.1.1182.3.2.12.1.2 | R/O | TimeTicks | Elapsed time from boot

#### 5.3. yamahaSWL2ms group

This MIB is related to L2MS information for Yamaha network switches.

- yamahaSWL2ms group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  ysl2msNumber | 1.3.6.1.4.1.1182.3.5.1 | N/A | INTEGER | Number of switches that can be recognized Note: Used only with trap notifications
  ysl2msEnableTrap | 1.3.6.1.4.1.1182.3.5.2 | R/W | INTEGER * enabled(1) * disabled(2) | Setting value for determining whether SNMP traps due to L2MS information are notified
  ysl2msTable | 1.3.6.1.4.1.1182.3.5.3 | N/A |  | Table of information for devices connected via L2MS
  | ysl2msEntry | 1.3.6.1.4.1.1182.3.5.3.1 | N/A |  | INDEX * ysl2msIndex
  | ysl2msIndex | 1.3.6.1.4.1.1182.3.5.3.1.1 | N/A | DisplayString (SIZE (0..6)) | MAC address of device Note: Used only with trap notifications
  ysl2msProduct | 1.3.6.1.4.1.1182.3.5.3.1.2 | N/A | INTEGER * generic(1) * swx2200-8g(2) * swx2200-24g(3) * swx2200-8poe(4) | Model of device Note: Used only with trap notifications
  ysl2msPhysAddress | 1.3.6.1.4.1.1182.3.5.3.1.5 | N/A | DisplayString (SIZE (0..6)) | MAC address of device Note: Used only with trap notifications
  ysl2msRoute | 1.3.6.1.4.1.1182.3.5.3.1.11 | N/A | DisplayString (SIZE (0..64)) | Route information to device Note: Used only with trap notifications

#### 5.4. yamahaSWErrDisable group

This MIB is related to error detection function information for Yamaha network switches.

- yamahaSWErrDisable group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  ysedConfigTable | 1.3.6.1.4.1.1182.3.6.1 | N/A |  | Table of setting information for the error detection function
  | ysedConfigEntry | 1.3.6.1.4.1.1182.3.6.1.1 | N/A |  | INDEX * ysedConfigIndex
  | ysedConfigIndex | 1.3.6.1.4.1.1182.3.6.1.1.1 | N/A | INTEGER (1..2147483647) | Table index + Corresponds to the ysedConfigFunction value
  ysedConfigFunction | 1.3.6.1.4.1.1182.3.6.1.1.2 | R/O | INTEGER * bpduguard(1) * loopdetect(2) | Functions that are enabled for error detection
  ysedConfigAutoRecovery | 1.3.6.1.4.1.1182.3.6.1.1.3 | R/W | INTEGER * enabled(1) * disabled(2) | Setting for automatic recovery from Error Disable state
  ysedConfigRecoveryInterval | 1.3.6.1.4.1.1182.3.6.1.1.4 | R/W | INTEGER (10..1000000) | Frequency (seconds) at which to attempt automatic recovery from Error Disable state
  ysedEnableTrap | 1.3.6.1.4.1.1182.3.6.2 | R/W | INTEGER * enabled(1) * disabled(2) | Setting value for determining whether SNMP traps due to error detection functions are notified
  ysedIfTable | 1.3.6.1.4.1.1182.3.6.3 | N/A |  | Table of information for the error detection function
  | ysedIfEntry | 1.3.6.1.4.1.1182.3.6.3.1 | N/A |  | INDEX * ysedIfIndex
  | ysedIfIndex | 1.3.6.1.4.1.1182.3.6.3.1.1 | N/A | INTEGER (1..2147483647) | Interface index
  ysedIfStatus | 1.3.6.1.4.1.1182.3.6.3.1.2 | R/O | INTEGER * normal(1) * bpduguard(2) * loopdetect(3) * portsecurity(4) | Error Disable state of port

#### 5.5. yamahaSWRmon group

This MIB is related to RMON information for Yamaha network switches.

- yamahaSWRmon group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  ysrmonSetting | 1.3.6.1.4.1.1182.3.7.1 | R/W | INTEGER * enabled(1) * disabled(2) | Enabled/disabled setting of RMON function
  ysrmonEnableTrap | 1.3.6.1.4.1.1182.3.7.2 | R/W | INTEGER * enabled(1) * disabled(2) | Setting value for determining whether SNMP traps due to RMON functions are notified

#### 5.6. yamahaSWTermMon group

This MIB is related to terminal monitoring information for Yamaha network switches.

- yamahaSWTermMon group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  ystmEnableTrap | 1.3.6.1.4.1.1182.3.8.1 | R/W | INTEGER * enabled(1) * disabled(2) | Setting value for determining whether SNMP traps due to terminal monitoring functions are notified
  ystmIfTermTable | 1.3.6.1.4.1.1182.3.8.3 | N/A |  | Table of terminal monitoring functions targeted at ports
  | ystmIfTermEntry | 1.3.6.1.4.1.1182.3.8.3.1 | N/A |  | INDEX * ystmIfTermIndex
  | ystmIfTermIndex | 1.3.6.1.4.1.1182.3.8.3.1.1 | N/A | INTEGER (1..2147483647) | ifIndex Note: Used only with trap notifications
  ystmIfTermDescr | 1.3.6.1.4.1.1182.3.8.3.1.2 | N/A | DisplayString (SIZE (0..255)) | Terminal monitoring description Note: Used only with trap notifications
  ystmIfTermStatus | 1.3.6.1.4.1.1182.3.8.3.1.3 | N/A | INTEGER * up(1) * down(2) * idle(3) | Terminal monitoring status Note: Used only with trap notifications
  ystmIpTermTable | 1.3.6.1.4.1.1182.3.8.4 | N/A |  | Table of terminal monitoring functions targeted at IP addresses
  | ystmIpTermEntry | 1.3.6.1.4.1.1182.3.8.4.1 | N/A |  | INDEX ystmIpTermIndex
  | ystmIpTermIndex | 1.3.6.1.4.1.1182.3.8.4.1.1 | N/A | IpAddress | IP address of monitored target Note: Used only with trap notifications
  ystmIpTermDescr | 1.3.6.1.4.1.1182.3.8.4.1.2 | N/A | DisplayString (SIZE (0..255)) | Terminal monitoring description Note: Used only with trap notifications
  ystmIpTermStatus | 1.3.6.1.4.1.1182.3.8.4.1.3 | N/A | INTEGER * up(1) * down(2) * idle(3) | Terminal monitoring status Note: Used only with trap notifications

#### 5.7. yamahaSWBridge group

This MIB is related to dot1dBridge information on Yamaha network switches.

- yamahaSWBridge group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  ysbridgeEnableTrap | 1.3.6.1.4.1.1182.3.9.1 | R/W | INTEGER * enabled(1) * disabled(2) | Setting value for determining whether SNMP traps due to dot1dBridge information are notified

#### 5.8. yamahaSWPowerEthernet group

This MIB is related to PoE information for Yamaha switches.

- yamahaSWPowerEthernet group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  yspeEnableTrap | 1.3.6.1.4.1.1182.3.10.1 | R/W | INTEGER * enabled(1) * disabled(2) | Setting value for determining whether SNMP traps due to PoE information are notified
  yspeUnitSupplySetting | 1.3.6.1.4.1.1182.3.10.2 | R/W | INTEGER * enabled(1) * disabled(2) | Enables/disables the power supply function
  yspeUnitTable | 1.3.6.1.4.1.1182.3.10.3 | N/A |  | Table of device PoE information
  | yspeUnitEntry | 1.3.6.1.4.1.1182.3.10.3.1 | N/A |  | INDEX * yspeUnitStackId
  | yspeUnitStackId | 1.3.6.1.4.1.1182.3.10.3.1.1 | N/A | INTEGER (1..2147483647) | Stack ID This can be obtained with stack ID 1 if stack was not configured.
  yspeUnitSupplyPower | 1.3.6.1.4.1.1182.3.10.3.1.2 | R/O | Gauge32 | Power supply for the entire device
  yspeUnitPowerFailure | 1.3.6.1.4.1.1182.3.10.3.1.3 | R/O | INTEGER * normal(1) * failure(2) | Device power supply error
  yspeUnitGuardBandStatus | 1.3.6.1.4.1.1182.3.10.3.1.4 | R/O | INTEGER * not_operating(1) * operating(2) | Guard band status not_operating(1): Not operating State where the available power supply is greater than the guard band, and the guard band does not limit the power supply operating(2): Operating State where the available power supply is smaller than the guard band, and the guard band limits the power supply
  yspeUnitGuardBandValue | 1.3.6.1.4.1.1182.3.10.3.1.5 | R/W | Gauge32 (0..90000) | Guard band value (mW)
  yspePortTable | 1.3.6.1.4.1.1182.3.10.4 | N/A |  | Table of port information for PoE
  | yspePortEntry | 1.3.6.1.4.1.1182.3.10.4.1 | N/A |  | INDEX * yspePortStackId * yspePortIndex
  | yspePortStackId | 1.3.6.1.4.1.1182.3.10.4.1.1 | N/A | INTEGER (1..2147483647) | Stack ID This can be obtained with stack ID 1 if stack was not configured.
  yspePortIndex | 1.3.6.1.4.1.1182.3.10.4.1.2 | N/A | INTEGER (1..2147483647) | Port index for power supply port. Port numbers are used
  yspePortDescr | 1.3.6.1.4.1.1182.3.10.4.1.3 | R/W | DisplayString (SIZE (0..64)) | Description about power supply port + Setting value of the power-inline description command
  yspePortSupplySetting | 1.3.6.1.4.1.1182.3.10.4.1.4 | R/W | INTEGER * enabled(1) * disabled(2) | Enables/disables the power supply function
  yspePortDetectClass | 1.3.6.1.4.1.1182.3.10.4.1.5 | R/O | INTEGER * na(1) * class0(2) * class1(3) * class2(4) * class3(5) * class4(6) * class5(7) * class6(8) * class7(9) * class8(10) | Power supply class information for connected devices
  yspePortSupplyState | 1.3.6.1.4.1.1182.3.10.4.1.6 | R/O | INTEGER * none(1) * supply-class0(2) * supply-class1(3) * supply-class2(4) * supply-class3(5) * supply-class4(6) * terminate(7) * overcurrent(8) * forced-terminate(9) * over-supply(10) * over-temp(11) * fanlock(12) * power-failure(13) * class-failure(14) * over-guardband(15) * pd-failure(16) * guardband-restrict(17) * supply-class5(18) * supply-class6(19) * supply-class7(20) * supply-class8(21) | Port power supply status * If the power supply function of the port is enabled and no PoE device is connected, this value is terminate(7) * If the power supply function of the port is disabled, this value is none(1)
  yspePortSupplyPower | 1.3.6.1.4.1.1182.3.10.4.1.7 | R/O | Gauge32 | Port power consumption (mW)
  yspePortPowerPriority | 1.3.6.1.4.1.1182.3.10.4.1.8 | R/W | INTEGER * critical(1) * high(2) * low(3) | Port power supply priority order

#### 5.9. yamahaSWLoopDetect group

This MIB is related to loop detection information for Yamaha switches.

- yamahaSWLoopDetect group

  MIB name | OID | Access | Syntax | Description
  --- | --- | --- | --- | ---
  ysldEnableTrap | 1.3.6.1.4.1.1182.3.11.1 | R/W | INTEGER * enabled(1) * disabled(2) | Whether or not trap sends notification
  ysldSystemAdmin | 1.3.6.1.4.1.1182.3.11.2 | R/W | INTEGER * enabled(1) * disabled(2) | Enables/disables loop detection for the entire system
  ysldSystemBlockingRecoveryInterval | 1.3.6.1.4.1.1182.3.11.6 | R/W | INTEGER (0｜10..3600) | Time (seconds) for a blocked interface to be automatically restored after resolving a loop
  ysldSystemStatusReset | 1.3.6.1.4.1.1182.3.11.7 | R/W | INTEGER * nothing(1) * reset(2) | Reset the loop detection status
  ysldPortTable | 1.3.6.1.4.1.1182.3.11.8 | N/A |  | Table of loop detection information for each port
  | ysldPortEntry | 1.3.6.1.4.1.1182.3.11.8.1 | N/A |  | INDEX * ysldPortStackId * ysldPortIndex
  | ysldPortStackId | 1.3.6.1.4.1.1182.3.11.8.1.1 | N/A | INTEGER (1..2147483647) | Stack ID This can be obtained with stack ID 1 if stack was not configured.
  ysldPortIndex | 1.3.6.1.4.1.1182.3.11.8.1.2 | N/A | INTEGER (1..2147483647) | Port number
  ysldPortAdmin | 1.3.6.1.4.1.1182.3.11.8.1.3 | R/W | INTEGER * enabled(1) * disabled(2) | Enables/disables loop detection at ports
  ysldPortStatus | 1.3.6.1.4.1.1182.3.11.8.1.4 | R/O | INTEGER * disabled(1) * normal(2) * detected(3) * blocked(4) * shutdown(5) | Loop detection status * disabled(1): The loop detection function is disabled * normal(2): No loop is detected * detected(3): A loop is detected * blocked(4): A loop is detected and the port is blocked * shutdown(5): A loop is detected, so the port is shut down
  ysldPortBlocking | 1.3.6.1.4.1.1182.3.11.8.1.5 | R/W | INTEGER * enabled(1) * disabled(2) | Sets whether or not to block port if a loop occurs
  ysldLagTable | 1.3.6.1.4.1.1182.3.11.9 | N/A |  | Table of logical interface loop detection information for each link aggregation
  | ysldLagEntry | 1.3.6.1.4.1.1182.3.11.9.1 | N/A |  | INDEX * ysldLagIndex
  | ysldLagIndex | 1.3.6.1.4.1.1182.3.11.9.1.1 | N/A | INTEGER (1..2147483647) | ifIndex for link aggregation logical interface
  ysldLagAdmin | 1.3.6.1.4.1.1182.3.11.9.1.2 | R/W | INTEGER * enabled(1) * disabled(2) | Loop detection for link aggregation logical interface enabled/disabled
  ysldLagStatus | 1.3.6.1.4.1.1182.3.11.9.1.3 | R/O | INTEGER * disabled(1) * normal(2) * detected(3) * blocked(4) * shutdown(5) | Loop detection status * disabled(1): The loop detection function is disabled * normal(2): No loop is detected * detected(3): A loop is detected * blocked(4): A loop is detected and the logical interface is blocked * shutdown(5): A loop is detected and the logical interface is shut down
  ysldLagBlocking | 1.3.6.1.4.1.1182.3.11.9.1.4 | R/W | INTEGER * enabled(1) * disabled(2) | Sets whether or not to block the logical interface if a loop occurs

### 6. Standard MIB Traps

Standard MIB traps that are supported by this product are shown below.

#### 6.1. Traps defined by RFC1157

These are traps defined by RFC1157.

Trap name | OID | Additional information for trap (variable-bindings) | Description
--- | --- | --- | ---
coldStart | 1.3.6.1.6.3.1.1.5.1 | None | Notification on power OFF/ON and during firmware updates
warmStart | 1.3.6.1.6.3.1.1.5.2 | None | Notification while the reload command is being executed
linkDown | 1.3.6.1.6.3.1.1.5.3 | ifIndex ifAdminStatus ifOperStatus | Notification during linkdown
linkUp | 1.3.6.1.6.3.1.1.5.4 | ifIndex ifAdminStatus ifOperStatus | Notification during linkup
authenticationFailure | 1.3.6.1.6.3.1.1.5.5 | None | Notification when receiving an SNMP message that has an incorrect community name

#### 6.2. rmon group trap

This trap is related to RMON information.

Trap name | OID | Additional information for trap (variable-bindings) | Description
--- | --- | --- | ---
risingAlarm | 1.3.6.1.2.1.16.0.1 | alarmIndex alarmVariable alarmSampleType alarmValue alarmRisingThreshold | Notification that upper threshold value has been exceeded
fallingAlarm | 1.3.6.1.2.1.16.0.2 | alarmIndex alarmVariable alarmSampleType alarmValue alarmFallingThreshold | Notification that lower threshold value has been exceeded

#### 6.3. dot1dBridge group trap

This trap is related to dot1dBridge information.

Trap name | OID | Additional information for trap (variable-bindings) | Description
--- | --- | --- | ---
newRoot | 1.3.6.1.2.1.17.0.1 | None | Notification that a new root for bridge has been detected
topologyChange | 1.3.6.1.2.1.17.0.2 | None | Notification that a change in topology has been detected

#### 6.4. powerEthernetMIB group trap

This trap is related to PoE information.

Trap name | OID | Additional information for trap (variable-bindings) | Description
--- | --- | --- | ---
pethPsePortOnOffNotification | 1.3.6.1.2.1.105.0.1 | pethPsePortDetectionStatus | Notification that the PoE port status has changed
pethMainPowerUsageOnNotification | 1.3.6.1.2.1.105.0.2 | pethMainPseConsumptionPower | Notification that the power consumption goes from below the threshold value to on or above the threshold value + pethMainPseUsageThreshold is used as the threshold value
pethMainPowerUsageOffNotification | 1.3.6.1.2.1.105.0.3 | pethMainPseConsumptionPower | Notification that the power consumption goes from on or above the threshold value to below the threshold value + pethMainPseUsageThreshold is used as the threshold value

### 7. Private MIB Traps

The private MIB traps that are supported by this product are shown below.

#### 7.1. yamahaSWHardware group trap

This trap is related to hardware information for Yamaha switches.

Trap name | OID | Additional information for trap (variable-bindings) | Description
--- | --- | --- | ---
yshTemperatureStatusNormalTrap | 1.3.6.1.4.1.1182.3.1.0.5 | yshTemperatureStatusStackId yshTemperatureStatusDeviceType yshTemperatureStatus yshTemperatureStatusNormalThreshold yshTemperatureValue | Notification when temperature status returns to “Normal”
yshTemperatureStatusWarningTrap | 1.3.6.1.4.1.1182.3.1.0.6 | yshTemperatureStatusStackId yshTemperatureStatusDeviceType yshTemperatureStatus yshTemperatureStatusWarningThreshold yshTemperatureValue | Notification when temperature status changes to “Warning”
yshTemperatureStatusErrorTrap | 1.3.6.1.4.1.1182.3.1.0.7 | yshTemperatureStatusStackId yshTemperatureStatusDeviceType yshTemperatureStatus yshTemperatureStatusErrorThreshold yshTemperatureValue | Notification when temperature status changes to “Error”
yshFanStoppedTrap | 1.3.6.1.4.1.1182.3.1.0.8 | yshFanStackId yshFanIndex | Notification when fan stops
yshFanSpeedUpTrap | 1.3.6.1.4.1.1182.3.1.0.9 | yshFanSpeedStatusStackId yshFanSpeedStatus | Notification when fan RPM increases (when RPM reaches the “High” value)
yshFanSpeedDownTrap | 1.3.6.1.4.1.1182.3.1.0.10 | yshFanSpeedStatusStackId yshFanSpeedStatus | Notification when fan RPM decreases (when “High” RPM status is canceled)
yshTemperatureSensorInvalidTrap | 1.3.6.1.4.1.1182.3.1.0.13 | yshTemperatureStatusStackId | Notification that a thermal sensor abnormality has occurred

#### 7.2. yamahaSWL2ms group trap

This trap is related to L2MS information for Yamaha network switches.

Trap name | OID | Additional information for trap (variable-bindings) | Description
--- | --- | --- | ---
ysl2msFindAgent | 1.3.6.1.4.1.1182.3.5.0.1 | ysl2msNumber ysl2msProduct ysl2msPhysAddress ysl2msRoute | Notification sent when L2MS agent is detected
ysl2msDetectDown | 1.3.6.1.4.1.1182.3.5.0.2 | ysl2msNumber ysl2msProduct ysl2msPhysAddress ysl2msRoute | Notification sent when L2MS agent is lost

#### 7.3. yamahaSWErrDisable group trap

This trap is related to error detection function information for Yamaha network switches.

Trap name | OID | Additional information for trap (variable-bindings) | Description
--- | --- | --- | ---
ysedTrap | 1.3.6.1.4.1.1182.3.6.0.1 | ysedIfStatus | Notification when ErrorDisable is detected/cancelled

#### 7.4. yamahaSWTermMon group trap

This trap is related to terminal monitoring information for Yamaha network switches.

Trap name | OID | Additional information for trap (variable-bindings) | Description
--- | --- | --- | ---
ystmIfTermTrap | 1.3.6.1.4.1.1182.3.8.0.1 | ystmIfTermDescr ystmIfTermStatus | Notification when terminal monitoring is detected
ystmIpTermTrap | 1.3.6.1.4.1.1182.3.8.0.2 | ystmIpTermDescr ystmIpTermStatus | Notification when IP address terminal monitoring is detected

#### 7.5. yamahaSWPowerEthernet group trap

This trap is related to PoE information for Yamaha switches.

Trap name | OID | Additional information for trap (variable-bindings) | Description
--- | --- | --- | ---
yspeSupplyPortTrap | 1.3.6.1.4.1.1182.3.10.0.1 | yspePortStackId yspePortIndex yspePortDescr yspePortSupplyState | Notification that the power supply to the PoE device has started
yspeTerminatePortTrap | 1.3.6.1.4.1.1182.3.10.0.2 | yspePortStackId yspePortIndex yspePortDescr yspePortSupplyState | Notification that the power supply to the PoE device has stopped
yspeGuardBandStateTrap | 1.3.6.1.4.1.1182.3.10.0.3 | yspeUnitStackId yspeUnitSupplyPower yspeUnitGuardBandStatus yspeUnitGuardBandValue | Notification when the guard band status changes
yspePortErrorTrap | 1.3.6.1.4.1.1182.3.10.0.4 | yspePortStackId yspePortIndex yspePortDescr yspePortSupplyState | Notification that a PoE port error has been detected or resolved
yspeUnitFailureTrap | 1.3.6.1.4.1.1182.3.10.0.5 | yspeUnitStackId yspeUnitPowerFailure | Notification that a PoE unit power supply abnormality has been detected

#### 7.6. yamahaSWLoopDetect group trap

This trap is related to loop detection information for Yamaha switches.

Trap name | OID | Additional information for trap (variable-bindings) | Description
--- | --- | --- | ---
ysldPortDetectLoopTrap | 1.3.6.1.4.1.1182.3.11.0.1 | ysldPortStackId ysldPortIndex ysldPortStatus | Sends notification when a loop is detected at a port
ysldPortResolveLoopTrap | 1.3.6.1.4.1.1182.3.11.0.2 | ysldPortStackId ysldPortIndex ysldPortStatus | Sends notification when loop is resolved
ysldLagDetectLoopTrap | 1.3.6.1.4.1.1182.3.11.0.3 | ysldLagIndex ysldLagStatus | Sends notification if loop is detected at a link aggregation logical interface
ysldLagResolveLoopTrap | 1.3.6.1.4.1.1182.3.11.0.4 | ysldLagIndex ysldLagStatus | Sends notification when a loop is resolved at a link aggregation logical interface

### 8. Points of Caution

- The 64-bit counter MIB can be read and written by SNMPv2c and SNMPv3 requests.

  - Those MIBs cannot be read or written by SNMPv1 requests.

Search result
No more search results.
There are no topics that match your search query.