# PoE

### 1. Summary

This page is for changing the PoE control settings.

### 2. Top page

This is the top page for the PoE control settings.

#### 2.1. PoE control basic settings

- The current settings of the PoE control for the entire system are show.

- Press the "Setting" button to access a page where you can change the settings.

#### 2.2. PoE control settings

- PoE control settings are shown for each interface that supports PoE power supply.

- Press the "Setting" button to access a page where you can change the settings of the selected interface.

- If you press the "Specify all" button, the settings can be changed for all interfaces whose check box contains a check mark.

- If you press the "Return to defaults" button, the settings will be initialized for all interfaces whose check box contains a check mark.

  - The default PoE power supply setting is "Enabled" and the default power priority setting is "Low" for all interfaces that support PoE power supply.

- If the PoE control settings is disabled for the entire system, the PoE control settings for each interface cannot be made.

### 3. PoE control basic settings page

In this page you can enable/disable PoE power supply for the entire system and set the guard band.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 3.1. PoE control basic settings

- PoE power supply for entire system

  - Enabled

    - The PoE power supply will be enabled for the entire system.

  - Disabled

    - The PoE power supply will be disabled for the entire system.

- Guard band

  - The guard band specifies the tolerance for the maximum power supply specified to avoid unintended power supply interruptions.

  - The default guard band setting is "7" W, and the input range is 0 - 30.

### 4. PoE control settings page

In this page you can enable/disable PoE power supply and set power priority for the selected interface.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the setting confirmation screen, press the "OK" button.

#### 4.1. PoE control settings

- Port

  - The interface for which settings are made is shown.

- PoE power supply

  - Enabled

    - The PoE power supply will be enabled for the selected interface.

  - Disabled

    - The PoE power supply will be disabled for the selected interface.

- Power priority

  - Select power priority from the following items.

    - Low

    - High

    - Critical

  - In descending order, the priority levels are Critical, High, or Low.

  - If interfaces have the same priority setting, the interface with the lower interface number is prioritized.

- Explanation

  - Sets the description text for the interface which supports PoE power supply.

  - Characters that can be inputted include single-byte alphanumeric characters and symbols, excluding ?.

  - Up to 64 characters can be inputted.

Search result
No more search results.
There are no topics that match your search query.