# Dante optimization

### 1. Summary

This is the page for operations related to the Dante optimization settings.

The Dante optimization settings can be made manually or by means of auto-configure via LLDP.

### 2. Top page

This is the top page for configuring the Dante optimization.

#### 2.1. Dante optimization

- The current settings for the auto-configure via LLDP function are displayed.

- Press "Next" button to begin the steps for Dante optimization settings.

- Press "Setting" button to display the page where the settings for the auto-configure via LLDP function can be modified.

- This function cannot be used when the stack function is enabled.

#### 2.2. Multicast basic settings (System)

- Displays the configuration for unknown multicast frames for the entire system.

- The table items are explained below.

  - Processing method for unknown multicast frames

    - Displays the processing method of unknown multicast frames.

  - Excluded frames from discarding (for all VLANs)

    - Displays excluded frames from discarding when configured to discard unknown multicast frames.

#### 2.3. Multicast basic settings (VLAN interface)

- Displays the configuration for unknown multicast frames for each VLAN.

- The table items are explained below.

  - VLAN ID

    - VLAN ID is displayed.

  - Unknown multicast frame

    - Displays the processing method for unknown multicast frames for the target VLAN.

  - Excluded frames from discarding

    - Displays the frames to be excluded fromdiscarding when unknown multicast frames are configured to be discardedin the target VLAN.

#### 2.4. QoS settings

- Displays the QoS settings for the entire system.

- The table items are explained below.

  - QoS function

    - Displays whether the QoS function is enabled.

  - CoS - transmit queue mapping table

    - Displays the transmit queue ID settings corresponding to the CoS value.

  - DSCP - transmit queue mapping table

    - Displays the transmit queue ID settings corresponding to the DSCP value.

### 3. Manual settings page

This is the page for the Dante optimization settings.

Select VLAN interfaces, and then press the "Confirm"button. If there are no mistakes in the input content of theconfirmation screen, press the "OK" button.

#### 3.1. Manual settings

- VLAN interface

  - Press the "Select" button to display the "VLAN interface list" dialog box.

  - You can select VLAN interfaces in the "VLAN interface list" dialog by checking the check boxes and pressing the "OK" button.

### 4. Auto-configure via LLDP function page

This is the page for setting auto-configure via LLDP function.

Enter the settings, and then press the "Confirm" button.

If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

#### 4.1. Auto-configure via LLDP function

- Auto-configure via LLDP function

  - Select whether to enable the auto-configure via LLDP function settings, from the options below.

    - Enable

    - Disable

Search result
No more search results.
There are no topics that match your search query.