# Update firmware

### 1. Summary

In this page you can perform operations related to firmware update.

### 2. Top page

This is the top page for firmware update.

You can start the procedure for updating the firmware via thenetwork. Various settings for updating the firmware via the network aredisplayed.

#### 2.1. Firmware update information

- Displays the firmware revision and basic settings.

- Displays the firmware revision for the next start-up if a restart is pending after a firmware update.

- Press the "Setting" button to access a page where you can change the settings.

#### 2.2. Update firmware from PC

- When you press the "Next" button, the procedure for updating the firmware from the PC will be started.

#### 2.3. Update firmware via network

- When you press the "Next" button, the procedure for updating the firmware via the network will be started.

- Various settings for updating the firmware via the network are displayed.

- Press the "Setting" button to access a page where you can change the settings.

### 3. Firmware update basic settings page

This page is for configuring the basic settings for the firmware update.

When you have entered the settings, press the "Confirm" button.If there are no mistakes in the input content confirmation screen, press the "OK" button.

#### 3.1. Firmware update basic settings

- Restart timing after the update

  - Specify the restart timing after the firmware update.

- Restart method after the update

  - If you want the system to restart after the firmware update in a stack configuration automatically, you can specify whethereach switch restarts in sequence or simultaneously.

  - This item cannot be configured when the stack function is disabled.

### 4. Update firmware from PC page

In this page you can specify the firmware file placed on the PCfrom which you are accessing the web GUI, and perform the firmwareupdate.

In "Select file," select the firmware file that you want to usefor the update, and press the "Confirm" button. If there are no mistakes in the confirmation screen, press the "OK" button.

#### 4.1. Update firmware from PC

- Specify update file

  - Selects the firmware file used for the update

- Restart after the update

  - Specify whether or not to restart after the firmware update automatically.

  - The timing for restarting depends on the Restart timing after the update in the Firmware update basic settings.

### 5. Update firmware via network page

In this page you can download a firmware file from a web server,and perform the firmware update. This function lets you easily performthe entire process of checking for the latest firmware, downloading it,and updating the firmware.

When you open the page, the revision of the firmware file on the web server is automatically checked.

If the download URL is the Yamaha website and an updateablefirmware revision is found. The "OK" button displays a guide to thesoftware license agreement website. Please read the contents on thewebsite and press the "OK" button if you agree to the terms. Press the"OK" button to start downloading the firmware file from the webserver.

#### 5.1. Update firmware via network

- Current firmware revision

  - The revision of the currently-used firmware file is shown.

- Firmware revision available for update

  - Updatable revisions of the firmware files on the web server are shown.

- Restart after the update

  - Specify whether or not to restart after the firmware update automatically.

  - The timing for restarting depends on the Restart timing after the update in the Firmware update basic settings.

### 6. Update via network settings page

In this page you can make various settings for updating the firmware via the network.

When you have entered the settings, press the "Confirm" button.If there are no mistakes in the input content confirmation screen, press the "OK" button.

#### 6.1. Update via network settings

- Download source URL

  - This is the setting of the URL at which the firmware is located.

- HTTP proxy server

  - This is the HTTP proxy server setting used to download the firmware via the network.

- Revision downgrade

  - This setting permits or forbids rewriting to an older version of firmware.

- Timeout

  - This setting specifies the timeout time during the process of updating the firmware via the network.

Search result
No more search results.
There are no topics that match your search query.