# Summary data management

## 1. Summary

This page is for performing operations related to the summary data.

## 2. Top page

This is the top page for summary data management.
The backup of summary data is automatically saved in ROM of this unit.
You can start the process of clearing the summary data and exporting summary data to a PC.

### 2.1. Clearing summary data

- Press the "Next" button to begin the process of clearing the summary data.

### 2.2. Export summary data

- Press the "Next" button to begin the process of exporting the summary data to a PC.

## 3. Page for clearing summary data

This page is for clearing the summary data.
When you have inputted the settings, press the "Confirm" button.
If there are no mistakes in the input content confirmation screen, press the "OK" button.
When the summary data has been cleared, both the data saved in internal volatile memory and the data backed up to microSD card will be cleared.

### 3.1. Clearing summary data

- Summary data to clear

  - Select the summary data to clear from one of the following.

    - Traffic information

    - Resource information

    - Power consumption information

## 4. Export page for summary data

This page is for exporting summary data.
When you have finished inputting, check the inputted content and press the "OK" button.
Implementing the summary data export will download a ZIP file.
See Export file configuration for more information on the configuration of the ZIP file.

### 4.1. Export summary data

- Summary data to export

  - Select the summary data to export from one of the following.

    - Traffic information(Transmit)

    - Traffic information(Reception)

    - Resource information

    - Power consumption information

- Specifying a timespan

  - Select the month(s) of the data to be exported.

  - Specify the month(s) from the previous year using the drop-down list box.

## 5. Export file configuration

This explains about the folder that will be extracted when decompressing the ZIP file.

The configuration when the October 2017 traffic information (received) is exported is shown below.

- 20171103150412_trf_rx_csv.zip

  - 20171103150412_trf_rx_csv

    - 20171001_trf_rx_hour.csv

    - :

    - 20171031_trf_rx_hour.csv

    - 201710_trf_rx_day.csv

This explains about the folder and files after extraction.

- 20171103150412_trf_rx_csv

  - The CSV files with the summary data are contained in this folder.

  - The time of export and data type are used in the folder name.

  - One of the following will be used for the data type, according to the type specified.

    - trf_tx
      For traffic information (transmission)

    - trf_rx
      For traffic information (reception)

    - resource
      For resource information

    - pwr
      For power consumption information

- 20171001_trf_rx_hour.csv

  - This is the CSV file with the summary data.

  - The date, data type and data unit time will be included in the file name for the target data.

  - The naming convention for the data type is the same as for the folders.

  - One of the following will be used for the data unit time.

    - hour
      Files that are totaled every hour, containing one days’ worth of data

    - day
      Files that are totaled every day, containing one months’ worth of data

Search result
No more search results.
There are no topics that match your search query.