# CONFIG management

## 1. Summary

In this page you can import and export CONFIG.

This unit operates in accordance with its CONFIG file (settingsdata). A CONFIG file consists of a combination of multiple commands.

## 2. Top page

This is the top page for CONFIG management.

You can start the process of importing a CONFIG, or the process of exporting a CONFIG.

### 2.1. Import

- Press the "Next" button to display a page where you can import a CONFIG.

### 2.2. Export

- Press the "Next" button to display a page where you can export a CONFIG.

## 3. Import page

In this page, a CONFIG from the PC can be copied to internal non-volatile memory, updating the CONFIG.

When you have entered the settings, press the "Confirm" button.If there are no mistakes in the input content confirmation screen, press the "OK" button.

If the currently used CONFIG is the same as theimport-destination CONFIG, the unit restarts automatically after theimport has ended successfully.

If you want to start up with a CONFIG file that is not currently being used, change the setting using the startup-config select command before restarting.

### 3.1. Import CONFIG

- Import method

  - Select the import method from the following options.

    - Import all settings (.zip)

      - Import information such as a CONFIG file and a L2MS agent CONFIG together.

      - You cannot be used when using YNO manager for access.

    - Import a CONFIG file (.txt)

      - Import a CONFIG file.

    - Import a L2MS agent CONFIG (.bin)

      - Import a L2MS agent CONFIG.

- Settings to import

  - Press the "Select a file" button to display the file selection dialog box.

  - You can use the settings obtained on the export page.

- Import-destination

  - Select the import-destination CONFIG in internal non-volatile memory.

  - Cannot be changed when the stack function is enabled. (The currently used CONFIG is selected.)

## 4. Export page

In this page you can copy a CONFIG from internal non-volatile memory to the PC.

When you have finished entry, check the entered content and press the "OK" button.

### 4.1. Export CONFIG

- Export method

  - Select the export method from the following options.

    - Export all settings (.zip)

      - Export information such as a CONFIG file and a L2MS agent CONFIG together.

      - You cannot be used when using YNO manager for access.

    - Export a CONFIG file (.txt)

      - Export a CONFIG file.

    - Export a L2MS agent CONFIG (.bin)

      - Export a L2MS agent CONFIG.

- Settings to export

  - Select the CONFIG in internal non-volatile memory that you want to export.

  - Cannot be changed when the stack function is enabled. (The currently used CONFIG is selected.)

Search result
No more search results.
There are no topics that match your search query.