# Schedule execution

## 1. Summary

In this page you can make settings for schedule execution.

The schedule execution function of this product has two setting items, schedule template and schedule.

Schedule template settings allow you to create a template of detailed settings for processes involved in executing scheduled functions and operations, such as the specific functions to be executed, the applicable item involved, and the execution sequence.

In schedule settings, you can select when to execute schedules and which templates to execute.

## 2. Top page

This is the top page for making settings for schedule execution.

### 2.1. List of schedule template

- Information for the currently registered schedule template are shown.

- The table items are explained below.

  - Template ID

    - Registered schedule template ID are shown.

  - Status

    - The status of the schedule template are shown.

  - Template description

    - Description of the schedule template are shown.

- If you press the "New" button, a page appears in which you can create a new schedule template.

- If you press the "Setting" button, a page appears in which you can edit the settings of the selected schedule template.

- If you press the "Delete" button, all schedule templates whose check box has a check mark will be deleted.

- Up to 10 schedule templates can be registered.

### 2.2. List of schedule

- Information for the currently registered schedule are shown.

- The table items are explained below.

  - Schedule ID

    - Registered schedule ID are shown.

  - Execution timing

    - The execution timing of the schedule are shown.

  - Template to be executed

    - The information about the template to be executed when the schedule executed are shown.

- If you press the "New" button, a page appears in which you can create a new schedule.

- If you press the "Setting" button, a page appears in which you can edit the settings of the selected schedule.

- If you press the "Delete" button, all schedules whose check box has a check mark will be deleted.

- Up to 10 schedules can be registered.

## 3. Schedule template settings page

In this page you can create a new schedule template or edit the settings of an already-registered schedule template.

Enter the settings, and then press the "Confirm" button.

If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

### 3.1. Schedule template settings

- Template ID

  - The ID of the schedule template being set is displayed.

  - Newly created templates are automatically assigned the lowest unregistered serial number as the template ID.

- Template description

  - Sets the schedule template description text.

  - Enter up to 64 single-byte alphanumeric characters/symbols, excluding ‘?’.

- Status

  - Select template status from the following items.

    - Enabled

      - Enables the template

    - Disabled

      - Disables the template

      - The contents of the template are not executed at the time of schedule execution.

- Import source of the schedule execution contents

  - Select the import source of the schedule execution contents from the following items.

    - CONFIG of the device

      - Executes the schedule execution contents saved in CONFIG of the device at the time of schedule execution.

      - The schedule execution contents entered on this page are saved in CONFIG of the device.

    - Script file in microSD card

      - Loads the schedule execution contents from the script file in microSD card at the time of schedule execution.

      - Please refer to How to use the script file for specific usage.

- Contents of schedule execution

  - Enter the commands to be executed by the scheduled execution.

  - You can enter multiple commands together by separating them with line-returns.

  - Specify settings that result in 20 or fewer command lines.

  - Schedule execution always starts with the specially-privileged EXEC mode (enable).

  - For prohibited commands and command details, refer to the command reference and the information provided on the Network device product information page and Yamaha Network Devices Technical Documentation.

  - If you press the "Easy input" button, you can quickly enter the corresponding commands for the following functions.

    - Shutdown

    - Cancel shutdown

    - Save TECHINFO into microSD card

    - Save settings

## 4. Schedule settings page

In this page you can create a new schedule or edit the settings of an already-registered schedule.

Enter the settings, and then press the "Confirm" button.

If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

### 4.1. Schedule settings

- Schedule ID

  - The ID of the schedule being set is displayed.

  - Newly created templates are automatically assigned the lowest unregistered serial number as the schedule ID.

- Trigger type

  - Select the trigger to execute the schedule execution from the following items.

    - Time

      - When the time specified in the execution timing arrives, the device executes the schedule execution.

    - Event

      - When the event specified in the execution timing occurs, the device executes the schedule execution.

- Execution timing

  - If you select Time for Trigger type, select the timing to execute the schedule execution.

    - Easy input

      - Select a typical frequency pattern for the schedule execution timing.

      - Period

        - Select the periodic pattern of schedule execution from the following items.

          - Every day

          - Every week

          - Every month

          - Every year

        - If "Every week" is selected, mark the checkbox for the day of the week when the schedule is to be executed.

        - If "Every month" is selected, enter the day when the schedule is to be executed in the "Day" box.

        - If "Every year" is selected, enter the month and the day when the schedule is to be executed in the "Month" box and the "Day" box.

        - Enter numeric values in the "Month" and "Day" boxes.

        - Multiple months/days can be specified as comma-delimited values. (Example: Enter "10,20" to specify 10 and 20.)

        - A hyphen can be used to indicate a range of values. (Example: Enter "1-3" to specify 1, 2, and 3.)

        - When you focus on the "Month" and "Day" boxes, the input form that can be operated with a mouse click is displayed.

      - Time

        - In the Hours:Minutes:Seconds box, enter the time in hh:mm:ss format.

        - When you focus on the "Hours:Minutes:Seconds" box, an input form that can be operated with a mouse click is displayed.

    - Input in command format

      - Enter the "Date" and "Time" in the command format.

      - This allows specifying settings in more detail than the Easy input mode.

      - Enter the "Date" in MONTH/DATE format.

      - Enter the "Time" in hh:mm:ss format.

      - For details on command format, refer to the command reference and to the information provided on the Network device product information page and Yamaha Network Devices Technical Documentation.

  - If you select Event for Trigger type, select the event that triggers to execute the schedule execution.

    - When you start up the device

      - When you start up the device, the device executes the schedule execution.

    - When you attached a microSD card

      - When you attached a microSD card, the device executes the schedule execution.

- Template to be executed

  - Select the template to be executed in the schedule execution.

## 5. How to use the script file

If you select the script file in microSD card as the import source of the schedule execution contents in the schedule template settings, the contents of the script file are executed at the time of schedule execution.

To use the script file, you need to insert a microSD card with the script file saved in the specified path "/(model name)/schedule/script.txt" into the device beforehand.

You can enter up to 100 lines of commands into the script file. Commands after the 101 line are not executed at the time of schedule execution.

Search result
No more search results.
There are no topics that match your search query.