# Restart and initialization

## 1. Summary

In this page you can restart this unit and return it to the factory-set state.

## 2. Top page

This is the top page for restart and initialization.

Here you can start the process of restarting this unit or returning it to the factory-set state.

### 2.1. Restart

- When you press the "Next" button, the process of restarting this unit will begin.

### 2.2. Initialization

- When you press the "Next" button, the process of returning this unit to the factory-set state will begin.

## 3. Restart Page

In this page you can restart this unit.

If the stack function is disabled, press the "OK" button to restart the unit.

If the stack function is enabled, select the device to restart from the input screen and press the "Confirm" button. Then, press the "OK" button on the execute screen to restart the specified device.

Note that when you execute restart, the settings that were being changed will not be saved. In addition, the GUI cannot be accessed until restart has completed.

## 4. Initialization Page

In this page you can return this unit to its factory-set state.

After you have entered the privileged password, press the "Confirm" button. Confirm the content to be executed, and if you want to return this unit to its factory-set state, press the "OK" button.

Note that when the unit is returned to its factory-set state, all settings will return to their default values, including the address for accessing the GUI.

If the stack function is enabled, only the main switch is initialized.

### 4.1. Initialization

- Privileged password

  - To return the unit to its factory-set state, enter the privileged password.

Search result
No more search results.
There are no topics that match your search query.