# RMON settings

### 1. Summary

This page is for configuring RMON settings.

You can enable or disable the RMON function for the entiresystem, and specify Ethernet statistics group and history group forphysical interface.

You cannot configure RMON function when the stack function is enabled.

### 2. Top page

This is the top page for the RMON settings.

#### 2.1. System settings

- Displays the RMON function settings for the entire system.

- Press the "Setting" button to display a page for configuring the system settings.

#### 2.2. Interface settings

- Displays the configuration of each port’s Ethernet statistics and history groups.

- The table items are explained below.

  - Port

    - Displays the port name.

  - Ethernet statistics group

    - Settings

      - Displays whether the Ethernet statistics group for the port is enabled.

    - Index

      - Displays the index of Ethernet statistics group specified for the port.

  - History group

    - Settings

      - Displays whether the history group for the port is enabled.

    - Index

      - Displays the index of history group specified for the port.

- Press the "Setting" button to display a page for configuring the selected interface settings.

- Press the "Return to defaults" button to initialize the settings for all interfaces with the check box selected.

### 3. System settings page

This page is for configuring the RMON function settings for the system.

Enter the settings, and then press the "Confirm" button.

If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

#### 3.1. System settings

- RMON function

  - Specify whether to enable or disable the RMON function for the entire system.

  - If this setting is disabled, the following processes are executed.

    - Collecting statistics for the Ethernet statistics group is stopped.

    - Collecting history for the history group is stopped.

    - Sampling the alarm group is stopped.

  - If this setting is enabled, the following processes are executed.

    - Deletes the previously collected Ethernet statistics and restarts the collection.

    - Deletes the previously collected history and restarts the collection.

    - Deletes the previously collected sampling data and restarts sampling.

### 4. Interface settings page

This page is for configuring RMON settings for the interface.

Enter the settings, and then press the "Confirm" button.

If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

#### 4.1. Interface settings

- Port

  - Displays the port name to configure the settings.

- Ethernet statistics group

  - Specify the Ethernet statistics group.

  - Index

    - Set the index of the Ethernet statistics group.

    - The input range is 1 - 65535.

    - An index that is already in use cannot be specified.

  - Owner name

    - Set the owner name of the Ethernet statistics group.

    - Characters that can be inputted include single-byte alphanumeric characters and symbols, excluding ?.

    - Up to 127 characters can be inputted.

  - Press the icon to add an Ethernet statistics group.

  - Press the "Delete" button to delete the Ethernet statistics group.

  - You can specify up to 8 Ethernet statistics groups.

  - If you check the"Delete previously collected statistics" check box, previously collected Ethernet statistics will be deleted for already registered indexeswhose settings have not been changed.

- History group

  - Specify the history group.

  - Index

    - Set the index of the history group.

    - The input range is 1 - 65535.

    - An index that is already in use cannot be specified.

  - Number of saved history

    - Set the number of saved history of the history group.

    - The input range is 1 - 65535.

  - Save interval

    - Set the history saving interval of the history group.

    - The input range is 1 - 3600.

  - Owner name

    - Set the owner name of the history group.

    - Characters that can be inputted include single-byte alphanumeric characters and symbols, excluding ?.

    - Up to 127 characters can be inputted.

  - Press the icon to add a history group.

  - Press the "Delete" button to delete the history group.

  - You can specify up to 8 history groups.

  - If you check the "Delete previously collected history" check box, previously collectedhistory will be deleted for already registered indexes whose settingshave not been changed.

Search result
No more search results.
There are no topics that match your search query.