# Introduction

### 1. What you can do using the Web GUI

The web GUI lets you perform basic settings and management of theYamaha switch (this unit). The web GUI contains the following screensfor you to make settings and perform management.

- Dashboard

- LAN MAP

- Detailed settings

- Management

- CONSOLE

- CONFIG

- SYSLOG

- TECHINFO

### 2. Operating environment

Here we explain the environment that is required in order to use the web GUI.

#### 2.1. Recommended web browser

We recommend the following web browser for use with the web GUI.

- Windows

  - Microsoft Edge

  - Google Chrome

  - Mozilla Firefox

- Mac

  - Apple Safari

- iPadOS

  - Apple Safari

The latest version of each browser is recommended.

Microsoft Internet Explorer is not supported.

<NOTE>

- Do not use the "Back" or "Forward" buttons of the web browser.

- In some cases, the display layout of a page may become disordered. If this occurs, please access that page once again.

<Memo>

- The web GUI uses UTF-8 character encoding.

#### 2.2. JavaScript settings

The web GUI uses JavaScript. If your web browser is set to disableJavaScript, you might be unable to use the web GUI.If JavaScript isdisabled, please enable JavaScript in your web browser before use.

#### 2.3. Cookie settings

The web GUI uses cookies. If your web browser is set to disablecookies, you might be unable to use the web GUI.Please allow cookies inyour web browser before use.

### 3. User access rights

Users who log in to the web GUI are divided into two types: generalusers and administrative users. These are referred to as "accesslevels." The differences between the access levels are described below.

- For general users
  Can view the settings of the unit, operate the Web console, and obtain SYSLOG. Cannot change the settings.

- For administrative users
  Can view and change the settings of the unit. Can obtain CONFIG andTECHINFO in addition to operating the Web console and obtaining SYSLOG.

### 4. Note when using together with command input

Settings for this unit can be made not only via the web GUI but alsofrom the command console screen by directly entering commands. Commandinput allows a broader range of settings than when using the web GUI,and also lets you make settings for functions that are not supported inthe web GUI. If you use both command input and the web GUI to makesettings, be aware that the commands that you input may be overwritten,or the settings may be cleared.

<Memo>

- The command console screen contains the following items.

  - Management → "Maintenance" → "Command execution"

- For details on commands, refer to "Command reference."

### 5. Language

The Web GUI allows you to switch the display language.To switch the display language, press the "Language Switch" button on the top menu, and select a language you want.

The supported languages are as follows.

- Japanese

- English

Search result
No more search results.
There are no topics that match your search query.