# L2MS filter

### 1. Summary

This page is for configuring L2MS filter settings.
If you enable L2MS filter, you can block L2MS frames.

### 2. Top page

Displays a list of L2MS filter settings for interfaces.

#### 2.1. Interface list

- Displays the current L2MS filter settings for each interface.

- Press the "Setting" button to display the page for configuring the selected interface.

- Press the "Specify all" button to configure the settings for all interfaces with the check box selected.

- Press the "Return to defaults" button to initialize the settings for all interfaces with the check box selected.
  The default setting of L2MS filter is "Disabled".

- Constraints
  If the L2MS operation mode is disabled, L2MS filter does not work.
  L2MS frames are forwarded.

### 3. Interface settings

This page is for configuring L2MS filter for the interface.
Enter the settings, and then press the "Confirm" button.
If there are no mistakes in the input content of the confirmation screen, press the "OK" button.

#### 3.1. Interface settings

- L2MS filter
  Specify whether to enable or disable L2MS filter for the target interface.
  If it is enabled, the filter blocks L2MS frames. If it is disabled, the filter does not block L2MS frames.

Search result
No more search results.
There are no topics that match your search query.