# Command execution

### 1. Summary

In this page you can perform operations related to command execution.

### 2. Command execution page

In this page you can execute commands and acquire the results ofcommand execution. After entering the command in the command entryfield, press the "OK" button to execute the command. If you press the"Clear" button, the contents of the command entry field are cleared.

#### 2.1. Command execution

- Command input

  - In the command entry field, enter the setting in console command format (abbreviated input is not accepted).

  - You can enter multiple commands together by separating them with line-returns.

  - Execution always starts with the specially-privileged EXEC mode (enable). Enter the mode change command each time.

  - For details on commands to enter, refer to the command reference and to the information provided on the Network device product information page and Yamaha Network Devices Technical Documentation.

  - The following commands cannot be entered.

    - ping

    - ping6

    - telnet

    - ssh

    - ssh-server host key generate

    - reload

    - restart

    - cold start

    - firmware-update execute

    - firmware-update sd execute

    - startup-config select

    - erase startup-config

    - copy running-config startup-config

    - copy startup-config

    - show config

    - show running-config

    - show startup-config

    - show history

    - show tech-support

    - backup system

    - restore system

    - remote-login

    - stack enable

    - stack disable

    - no stack

    - stack subnet

    - no stack subnet

    - boot prioritize sd

    - no boot prioritize sd

    - quit

    - disable

    - logout

    - exit ( When in special privilege EXEC mode )

    - copy radius-server local

    - crypto pki generate ca

    - no crypto pki generate ca

    - system-diagnostics on-demand execute

- Command execution result

  - Displays the command execution result.

    - Success …​ Shown if the command executed successfully.

    - Error …​ Shown if the command you entered could not be executed.

    - Prohibited …​ Shown if a prohibited command was entered.

- Command execution log

  - The console log is output as the command execution record.

  - The command execution log will not necessarilyalways show the identical result as when the console setting operationwas executed.

  - By pressing the "Obtain as text file" button, you can acquire the contents of the command execution log as a text file.

  - The name of the acquired file is "command_YYYYMMDDhhmmss.txt".

    YYYY | …​ | A.D. ( 4 Digit )
    MM | …​ | Month ( 2 Digit )
    DD | …​ | Day ( 2 Digit )
    hh | …​ | Hours ( 2 Digit )
    mm | …​ | Minutes ( 2 Digit )
    ss | …​ | Seconds ( 2 Digit )

Search result
No more search results.
There are no topics that match your search query.